FILE DESCRIPTION 2/198 18-CRA 119 1170/1-V1 Uen J

#

Enterprise MIBs

Contents

1 | Enterprise MIBs
1.1 | RBN-AAL5-VCL-STAT-MIB
1.2 | RBN-X-AAL5-VCL-STAT-MIB
1.3 | RBN-ALARM-EXT-MIB
1.4 | RBN-ATM-CELL-PW-MIB
1.5 | RBN-ATM-PROFILE-MIB
1.6 | RBN-ATM-PVC-OAM-MIB
1.7 | RBN-ATM2-MIB
1.8 | RBN-BGP-ACCOUNTING-MIB
1.9 | RBN-BIND-MIB
1.10 | RBN-BRIDGE-MIB
1.11 | RBN-BULKSTATS-MIB
1.12 | RBN-CARDMON-MIB
1.13 | RBN-CES-MIB
1.14 | RBN-CIRCUIT-GROUP-MIB
1.15 | RBN-CONFIG-FILE-MIB
1.16 | RBN-CPU-METER-MIB
1.17 | RBN-DHCP-MIB
1.18 | RBN-DS1-MIB
1.19 | RBN-DS3-MIB
1.20 | RBN-ENVMON-MIB
1.21 | RBN-FAST-VRRP-MIB
1.22 | RBN-IP-BIND-MIB
1.23 | RBN-IP-SECURITY-MIB
1.24 | RBN-IPPOOL-MIB
1.25 | RBN-L2TP-MIB
1.26 | RBN-L2VPN-MIB
1.27 | RBN-MEDIA-GATEWAY-MIB
1.28 | RBN-MEMORY-MIB
1.29 | RBN-MPLS-L3VPN-STD-EXT-MIB
1.30 | RBN-NOTIFY-ENHANCE-MIB
1.31 | RBN-PING-MIB
1.32 | RBN-PRODUCT-MIB
1.33 | RBN-PVC-MIB
1.34 | RBN-QOS-MIB
1.35 | RBN-RADIUS-MIB
1.36 | RBN-SFP-MIB
1.37 | RBN-SSE-MIB
1.38 | RBN-STACKEDVLAN-MIB
1.39 | RBN-SUBSCRIBER-ACTIVE-MIB
1.40 | RBN-SYS-RESOURCES-MIB
1.41 | RBN-SYS-SECURITY-MIB
1.42 | RBN-TACACS-MIB
1.43 | Type Appendix

Copyright | © Ericsson AB 2009–2011. All rights reserved. No part of this document may be reproduced in any form without the written permission of the copyright owner.
Disclaimer | The contents of this document are subject to revision without notice due to continued progress in methodology, design and manufacturing. Ericsson shall have no liability for any error or damage of any kind resulting from the use of this document.
Trademark List |
SmartEdge |  | is a registered trademark of Telefonaktiebolaget LM Ericsson.
NetOp |  | is a trademark of Telefonaktiebolaget LM Ericsson.

# 1 Enterprise MIBs

The SmartEdge router supports several enterprise MIBs. The enterprise Object Identifier (OID) number for the Management Information Base (MIB) hierarchical tree is 2352. Enterprise Redback Network (RBN) MIB OIDs begin with the syntax, `1.3.6.1.4.1.2352`.

This document applies to both the Ericsson SmartEdge® and SM family routers. However, the software that applies to the SM family of systems is a subset of the SmartEdge OS; some of the functionality described in this document may not apply to SM family routers.

For information specific to the SM family chassis, including line cards, refer to the SM family chassis documentation.

For specific information about the differences between the SmartEdge and SM family routers, refer to the Technical Product Description SM Family of Systems (part number 5/221 02-CRA 119 1170/1) in the `Product Overview` folder of this Customer Product Information library.

This document describes each enterprise MIB, the tables in that MIB, and object details, including OIDs for each object. Index objects are identified before each table as `index:`

The following sections provide details about each supported enterprise MIBs.

Note:
  Simple Network Management Protocol (SNMP) examples in this document utilize the open-source tool Net-SNMP. Depending on the product that is used to monitor the network, the SNMP examples may appear differently for each system.

  If you have a support contract, you can download the Enterprise MIBs after you log on at https://ebusiness.ericsson.net

## 1.1 RBN-AAL5-VCL-STAT-MIB

Defines objects used to report configuration and performance statistics beyond those reported by standard Internet Engineering Task Force (IETF) MIBs for an Asynchronous Transfer Mode (ATM) virtual channel link (VCL).

Note:
  This MIB has been deprecated by RBN-ATM2-MIB.

### 1.1.1 rbnAtmAal5VclStatTable

This table provides a collection of objects providing ATM adaptation layer type 5 (AAL5) configuration and performance statistics of a VCL.

`Index:` ifIndex, atmVclVpi, atmVclVci

Table 1 describes the object in rbnAtmAal5VclStatTable.

Table 1 Objects in rbnAtmAal5VclStatTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnAtmAal5VclOutDrops rbnAtmAal5VclStatEntry 1 1.3.6.1.4.1.2352.2.1.1.1.1.1 | Counter32 | 0..4294967295 | Number of AAL5 common part convergence sublayer (CPCS) protocol data units (PDUs), transmitted on the AAL5 virtual channel connection (VCC) for the interface specified by ifIndex, that the system dropped, even if the system did not detect errors that prevented PDU transmission. For example, the system might drop a PDU because there was not enough space in the interface output queue. This object is read-only.

## 1.2 RBN-X-AAL5-VCL-STAT-MIB

Defines objects used to track statistics associated with an ATM VCL.

Note:
  This MIB has been deprecated by ATM2-MIB.

### 1.2.1 rbnXAtmAal5VclStatTable

This table describes the collection of objects with information about AAL5 configuration and VCL performance statistics.

`Index:` ifIndex, atmVclVpi, atmVclVci

Table 2 describes the objects in rbnXAtmAal5VclStatTable.

Table 2 Objects in rbnXAtmAal5VclStatTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnXAtmAal5VclInPkts rbnXAtmAal5VclStatEntry 1 1.3.6.1.4.1.2352.3.1.1.1.1.1 | Counter32 | 0..4294967295 | Number of AAL5 CPCS PDUs received on the AAL5 VCC at the interface identified by the ifIndex object.
rbnXAtmAal5VclOutPkts rbnXAtmAal5VclStatEntry 2 1.3.6.1.4.1.2352.3.1.1.1.1.2 | Counter32 | 0..4294967295 | Number of AAL5 CPCS PDUs transmitted on the AAL5 VCC at the interface identified by the ifIndex object.
rbnXAtmAal5VclInOctets rbnXAtmAal5VclStatEntry 3 1.3.6.1.4.1.2352.3.1.1.1.1.3 | Counter32 | 0..4294967295 | Number of octets contained in AAL5 CPCS PDUs received on the AAL5 VCC at the interface identified by the ifIndex object.
rbnXAtmAal5VclOutOctets rbnXAtmAal5VclStatEntry 4 1.3.6.1.4.1.2352.3.1.1.1.1.4 | Counter32 | 0..4294967295 | Number of octets contained in AAL5 CPCS PDUs transmitted on the AAL5 VCC at the interface identified by the ifIndex object.

## 1.3 RBN-ALARM-EXT-MIB

Defines extensions to the alarmModelTable and alarmClearTable as defined in ALARM-MIB (RFC 3877).

### 1.3.1 rbnAlarmModelTable

This table provides a set of objects which augment a conceptual row in the alarmModelTable.

`Index`: alarmListName, alarmModelIndex, alarmModelState

Table 3 describes the object in rbnAlarmModelTable.

Table 3 Objects in rbnAlarmModelTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnAlarmModelResourceIdx rbnAlarmModelEntry 1 1.3.6.1.4.1.2352.5.53.1.1.1.1.1 | Unsigned32 | 0 | 3..512 | The index into the trap PDU varbind list that identifies a particular object and value for the trap identified by alarmModelNotificationId. rbnAlarmModelResourceIdx is used to identify a resource that cannot be identified using alarmModelVarbindSubtree and alarmModelResourcePrefix. A value of 0 indicates that rbnAlarmModelResourceIdx is not used. When rbnAlarmModelResourceIdx is set to a value other than 0, the value of alarmActiveResourceId is set to the RowPointer for the corresponding varbind in the alarmActiveVariableTable.

### 1.3.2 rbnAlarmClearResourceTable

This table contains a list of the resource IDs for entries in the alarmClearTable. Each row in this table is associated with a corresponding entry in the alarmClearTable indicated by the RowPointer for the row in this table.

`Index`: alarmListName, alarmClearDateAndTime, alarmClearIndex

Table 4 describes the objects in rbnAlarmClearResourceTable.

Table 4 Objects in rbnAlarmClearResourceTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnAlarmClearResourceID rbnAlarmClearResourceEntry 1 1.3.6.1.4.1.2352.5.53.1.3.1.1.1 | Object ID | N/A | The alarm variable's object identifier.
rbnAlarmClearResourceValueType rbnAlarmClearResourceEntry 3 1.3.6.1.4.1.2352.5.53.1.3.1.1.3 | Integer | 1—counter32 2—unsigned32 3—timeTicks 4—integer32 5—ipAddress 6—octetString 7—objectId 8—counter64 | The value type. Only one of the value objects that follow is used for a given row in this table.
rbnAlarmClearResourceCounter32Val rbnAlarmClearResourceEntry 4 1.3.6.1.4.1.2352.5.53.1.3.1.1.4 | Counter32 | 0..4294967295 | The value when rbnAlarmClearResourceType is counter32.
rbnAlarmClearResourceUnsigned32Val rbnAlarmClearResourceEntry 5 1.3.6.1.4.1.2352.5.53.1.3.1.1.5 | Unsigned32 | 0..4294967295 | The value when rbnAlarmClearResourceType is unsigned32.
rbnAlarmClearResourceTimeTicksVal rbnAlarmClearResourceEntry 6 1.3.6.1.4.1.2352.5.53.1.3.1.1.6 | TimeTicks | 0..4294967295 | The value when rbnAlarmClearResourceType is timeTicks.
rbnAlarmClearResourceInteger32Val rbnAlarmClearResourceEntry 7 1.3.6.1.4.1.2352.5.53.1.3.1.1.7 | Integer32 | 0..4294967295 | The value when rbnAlarmClearResourceType is integer32.
rbnAlarmClearResourceOctetStringVal rbnAlarmClearResourceEntry 8 1.3.6.1.4.1.2352.5.53.1.3.1.1.8 | Octet String | 0..65535 | The value when rbnAlarmClearResourceType is octetString. The range indicates the number of characters in the string.
rbnAlarmClearResourceIpAddressVal rbnAlarmClearResourceEntry 9 1.3.6.1.4.1.2352.5.53.1.3.1.1.9 | IpAddress Octet String | SIZE (4) | The value when rbnAlarmClearResourceType is ipAddress. The range indicates the number of characters in the string.
rbnAlarmClearResourceOidVal rbnAlarmClearResourceEntry 10 1.3.6.1.4.1.2352.5.53.1.3.1.1.10 | Object ID | N/A | The value when rbnAlarmClearResourceType is objectId.
rbnAlarmClearResourceCounter64Val rbnAlarmClearResourceEntry 11 1.3.6.1.4.1.2352.5.53.1.3.1.1.11 | Counter64 | 0..18446744073709551615 | The value when rbnAlarmClearResourceType is counter64.

## 1.4 RBN-ATM-CELL-PW-MIB

Defines objects used to retrieve statistics associated with an ATM cell pseudowire (PW) circuit.

### 1.4.1 rbnAtmCellPWStatTable

This table contains objects that provide statistics for ATM cell PW circuits used to carry ATM traffic.

`Index:` rbnAtmCellPWCircuitHandle

Table 5 describes the objects in rbnAtmCellPWStatTable.

Table 5 Objects in rbnAtmCellPWStatTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnAtmCellPWCircuitHandle rbnAtmCellPWStatEntry 1 1.3.6.1.4.1.2352.2.41.1.1.1.1 | rbnCircuitHandle Octet String | SIZE (8) | A key for identifying the PW circuit. This object is not-accessible. The string size is eight (8).
rbnAtmCellPWOutOfSeqDrops rbnAtmCellPWStatEntry 2 1.3.6.1.4.1.2352.2.41.1.1.1.2 | Counter32 | 0..4294967295 | Total number of cells that dropped because of out-of-sequence PDUs received on the PW circuit.
rbnAtmCellPWCellConcatDrops rbnAtmCellPWStatEntry 3 1.3.6.1.4.1.2352.2.41.1.1.1.3 | Counter32 | 0..4294967295 | Total number of cells that dropped because of cell-concatenated PDUs received on the PW circuit.

## 1.5 RBN-ATM-PROFILE-MIB

Contains information that helps manage ATM profiles.

### 1.5.1 rbnAtmProfileTable

This table provides a collection of auxiliary objects providing parameters for ATM profiles.

`Index`: atmTrafficDescrParamIndex

Table 6 describes the objects in rbnAtmProfileTable.

Table 6 Objects in rbnAtmProfileTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnAtmProfileName rbnAtmProfileEntry 1 1.3.6.1.4.1.2352.2.2.1.1.1.1 | AtmProfileName Octet String | 0..80 | Text handle assigned to an instance of rbnAtmProfileTable. Using a text handle instead of an arbitrary integer allows a configuration to contain human-friendly cross-references to the profiles from those places where they are used, such as in circuit configuration tables. This object is not accessible.
rbnAtmCountersEnabled rbnAtmProfileEntry 2 1.3.6.1.4.1.2352.2.2.1.1.1.2 | TruthValue Integer | 1—true 2—false | An indication whether circuits configured with this profile should enable per-circuit statistical counters. An ATM circuit keeps per-circuit statistical counters only if this object is set to true in the profile used by the circuit.
rbnAtmCellLossPriority rbnAtmProfileEntry 3 1.3.6.1.4.1.2352.2.2.1.1.1.3 | TruthValue Integer | 1—true 2—false | An indication whether circuits configured with this profile should enable the Cell Loss Priority (CLP) bit on transmitted cells. If the profile used by a circuit has this object set to true, all cells transmitted on that circuit will have the CLP bit set.
rbnAtmTransmitBuffers rbnAtmProfileEntry 4 1.3.6.1.4.1.2352.2.2.1.1.1.4 | Integer32 | 1..63 | Limit on the total number of outbound transmit packet buffers that may be used by the circuit referencing the profile. The default is 50. (1)

(1) Use this parameter with caution. Setting it improperly can affect overall system performance.

## 1.6 RBN-ATM-PVC-OAM-MIB

Monitors the ATM operations, administration, and maintenance (OAM) functions.

### 1.6.1 rbnAtmPvcOamStatusTable

This table contains the status of the ATM permanent virtual circuit (PVC) OAM function for every ATM PVC in the system. One entry in this table exists for each ATM PVC active in the system, whether the PVC is a static or on-demand circuit.

`Index:` rbnAtmPvcOamStatusSlot, rbnAtmPvcOamStatusPort, rbnAtmPvcOamStatusVpi, rbnAtmPvcOamStatusVci

Table 7 describes the objects in rbnAtmPvcOamStatusTable.

Table 7 Objects in rbnAtmPvcOamStatusTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnAtmPvcOamStatusSlot rbnAtmPvcOamStatusEntry 1 1.3.6.1.4.1.2352.2.19.1.1.1.1 | RbnSlot Unsigned32 | 0..255 | Slot containing the ATM PVC. This object is not-accessible.
rbnAtmPvcOamStatusPort rbnAtmPvcOamStatusEntry 2 1.3.6.1.4.1.2352.2.19.1.1.1.2 | RbnSlot Unsigned32 | 0..255 | Port containing the ATM PVC. This object is not-accessible.
rbnAtmPvcOamStatusVpi rbnAtmPvcOamStatusEntry 3 1.3.6.1.4.1.2352.2.19.1.1.1.3 | Integer32 | 0..4095 | VPI value of the ATM PVC. This object is not-accessible.
rbnAtmPvcOamStatusVci rbnAtmPvcOamStatusEntry 4 1.3.6.1.4.1.2352.2.19.1.1.1.4 | Integer32 | 0..65535 | VCI value of the ATM PVC. This object is not-accessible.
rbnAtmPvcOamStatusState rbnAtmPvcOamStatusEntry 5 1.3.6.1.4.1.2352.2.19.1.1.1.5 | Integer | 1—noOam 2—oamUp 3—oamDownLoopback 4—oamDownAis 5—oamDownRdi | State of the ATM PVC OAM function on an ATM PVC. The noOam value indicates the ATM PVC OAM function is not active on the ATM PVC. The oamUp value indicates the ATM PVC OAM function is active on the ATM PVC, and no failure condition is currently detected on the circuit. The oamDownLoopback value indicates the ATM PVC OAM function is active on the ATM PVC, and F5 OAM loopback cell management has detected a fault on the circuit. The oamDownAis value indicates the ATM PVC OAM function is active on the ATM PVC, and a VC-AIS cell was recently received, which indicates a fault on the circuit. The oamDownRdi value indicates the ATM PVC OAM function is active on the ATM PVC, and a VC-RDI cell was recently received, which indicates a fault on the circuit.

## 1.7 RBN-ATM2-MIB

Monitors statistics associated with ATM virtual path link (VPL) and VCL beyond those configured with ATM2-MIB.

### 1.7.1 rbnAtm2VplStatTable

This table provides a collection of statistics objects of a VPL.

`Index:` ifIndex, atmVplVpi

Table 8 describes the objects in rbnAtm2VplStatTable.

Table 8 Objects in rbnAtm2VplStatTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnAtm2VplOutPktDrops rbnAtm2VplStatEntry 1 1.3.6.1.4.1.2352.2.50.1.1.1.1 | Counter32 | 0..4294967295 | The number of transmit packets dropped by this VPL.

### 1.7.2 rbnAtm2VclStatTable

This table provides a collection of statistics objects of a VCL.

`Index:` ifIndex, atmVclVpi, atmVclVci

Table 9 describes the objects in rbnAtm2VclStatTable.

Table 9 Objects in rbnAtm2VclStatTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnAtm2VclOutPktDrops rbnAtm2VclStatEntry 1 1.3.6.1.4.1.2352.2.50.1.1.1.1 | Counter32 | 0..4294967295 | The number of transmit packets dropped by this VCL.

### 1.7.3 rbnAtm2Aal5VclStatTable

This table provides a collection of auxiliary objects providing AAL5 configuration and performance statistics of a VCL.

`Index:` ifIndex, atmVclVpi, atmVclVci

Table 10 describes the objects in rbnAtm2Aal5VclStatTable.

Table 10 Objects in rbnAtm2Aal5VclStatTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnAtm2Aal5VclOutPktDrops rbnAtm2Aal5VclStatEntry 1 1.3.6.1.4.1.2352.2.50.1.3.1.1 | Counter32 | 0..4294967295 | The number of AAL5 CPCS PDUs received for transmission on the AAL5 VCC at the interface are identified by the ifIndex. These PDUs are chosen to be dropped to prevent their being transmitted even though no errors had been detected. A lack of space on the interface output queue can cause PDUs to be dropped.

## 1.8 RBN-BGP-ACCOUNTING-MIB

Defines objects to account for IP traffic differentially using Border Gateway Protocol (BGP) policies. RBN-BGP-ACCOUNTING-MIB works only when the `snmp server enhance ifmib` command (in global configuration mode) is enabled.

### 1.8.1 rbnBpaTable

This table provides a list of BGP policy accounting entries. An entry contains statistics applicable to a BGP-based routing policy set on an interface. The index object, ifIndex, represent a port, channel, subchannel, or circuit layer that supports the IF-MIB ifPacketGroup object, ifHCPacketGroup object, or ifVHCPacketGroup object, and is bound to an IP interface for which BGP policy-based accounting is enabled.

Note:
  Because the IF-MIB may provide support for a subset of the physical interfaces available on the system, that support for BGP policy-based accounting information in this MIB is limited to the same subset of physical interfaces supported in the IF-MIB.

`Index`: ifIndex, rbnBpaBucketIndex

Table 11 describes the objects in rbnBpaTable.

Table 11 Objects in rbnBpaTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnBpaBucketIndex rbnBpaEntry 1 1.3.6.1.4.1.2352.2.20.1.1.1.1 | Integer32 | 1..2147483647 | Integer greater than 0 that uniquely identifies a BGP routing policy set on this interface.
rbnBpaInPacketCount rbnBpaEntry 2 1.3.6.1.4.1.2352.2.20.1.1.1.2 | Counter64 | 0..18446744073709551615 | Total number of packets received for a particular BGP routing policy on an interface.
rbnBpaInOctetCount rbnBpaEntry 3 1.3.6.1.4.1.2352.2.20.1.1.1.3 | Counter64 | 0..18446744073709551615 | Total number of octets received for a particular BGP routing policy on an interface.
rbnBpaCircuitDescr rbnBpaEntry 4 1.3.6.1.4.1.2352.2.20.1.1.1.4 | SnmpAdminString | 0..192 | Descriptive version of the interface that is consistent with information displayed in the CLI. The string is formatted as `slot/port:channel:subchannel authority/level/index`. The channel and subchannel are only included when appropriate. For example, 4/1 1/2/7, 4/1:1 1/2/7 or 4/1:1:1 1/2/7. If a circuit description is not available, this object contains a string of zero (0) length.
rbnBpaInterfaceName rbnBpaEntry 5 1.3.6.1.4.1.2352.2.20.1.1.1.5 | SnmpAdminString | 0..127 | Name of the IP interface bound to a circuit. If the IP interface name is not available, this object contains a string of zero (0) length.
rbnBpaContextName rbnBpaEntry 6 1.3.6.1.4.1.2352.2.20.1.1.1.6 | SnmpAdminString | 0..63 | Name of context in which this IP interface is defined. If context information is not available, this object contains a string of zero (0) length.

## 1.9 RBN-BIND-MIB

Defines the objects used to support the configuration and management of circuit bindings.

### 1.9.1 rbnBindTable

This table contains the objects that identify and configure circuit bindings. Rows in this table are created or deleted when a circuit is created or deleted. No explicit creation or deletion of rows is allowed or required.

`Index:` rbnBindCircuit

Table 12 describes the objects in rbnBindTable.

Table 12 Objects in rbnBindTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnBindCircuit rbnBindEntry 1 1.3.6.1.4.1.2352.2.17.1.1.1.1 | rbnCircuitHandle Octet String | SIZE (8) | A key identifying the circuit for which the binding applies.
rbnBindType rbnBindEntry 2 1.3.6.1.4.1.2352.2.17.1.1.1.2 | RbnBindType Integer | 1—unbound 2—authBind 3—bypassBind 4—interfaceBind 5—subscriberBind 6—l2tptunnelBind 7—sessionBind 8—dot1qBind 9—multiIntfBind 10—multiSubBind 11—multiClipsBind | Binding type. The bind type must be appropriate to the type of circuit that it is being applied to. When a circuit is created, an initial binding is established with the unbound type. If you change the bind type for a circuit, the previous binding is removed and active sessions are dropped. When changing the bind type to a new bind type, all objects mandatory for the new bind type must be included in the set operation. The bind type determines which group of objects in a row of rbnBindTable apply for that instance of a circuit.
rbnBindName rbnBindEntry 3 1.3.6.1.4.1.2352.2.17.1.1.1.3 | SnmpAdminString | 1..192 | A name associated with the binding. This field is only applicable when the value of the rbnBindType object is: bypassBind (3) interfaceBind (4) subscriberBind (5) l2tptunnelBind (6) sessionBind (7) multiIntfBind (9) multiSubBind (10)
rbnBindPassword rbnBindEntry 4 1.3.6.1.4.1.2352.2.17.1.1.1.4 | SnmpAdminString | 1..64 | The AAA password. This field is only applicable when the value of the rbnBindType object is subscriberBind (5).
rbnBindContext rbnBindEntry 5 1.3.6.1.4.1.2352.2.17.1.1.1.5 | SnmpAdminString | 1..64 | The name of the context associated with the binding. This field is applicable only when one of the following rbnBindType values is specified: bypassBind (3) interfaceBind (4) subscriberBind (5) l2tptunnelBind (6) sessionBind (7) multiIntfBind (9) multiSubBind (10) multiClipsBind (11)
rbnBindAuthContext rbnBindEntry 6 1.3.6.1.4.1.2352.2.17.1.1.1.6 | SnmpAdminString | 1..64 | The name of the authentication context associated with the binding. This object is the name of the context to which PPP sessions on the circuits being bound are restricted. When using this optional context name, all attempts to bind PPP sessions to contexts other than the one specified fail. This object is applicable only when one of the following rbnBindType values is specified: authBind (2) multiIntfBind (9) multiSubBind (10)
rbnBindServiceGrp rbnBindEntry 7 1.3.6.1.4.1.2352.2.17.1.1.1.7 | SnmpAdminString | 1..64 | The name of the service access list associated with the binding. This object is the name of the service access list that defines the services available to the PPP-encapsulated circuit. When using this optional service access list, all attempts to authenticate to contexts or domains not permitted by the named service access list fail. This object is applicable only when one of the following rbnBindType values is specified: authBind (2) multiIntfBind (9) multiSubBind (10) multiClipsBind (11)
rbnBindAcl rbnBindEntry 8 1.3.6.1.4.1.2352.2.17.1.1.1.8 | SnmpAdminString | 1..64 | Name of the bridge access control list associated with the binding. The access control list must already have been configured in the context of the session peer. This is typically used to filter packets so that only PPPoE traffic is allowed through an Ethernet L2TP tunnel. Specification of this column for a given entry is optional. This object is applicable only when therbnBindType, sessionBind (7 value is specified.
rbnBindAuthChap rbnBindEntry 9 1.3.6.1.4.1.2352.2.17.1.1.1.9 | TruthValue Integer | 1—true 2—false | If the value of this object is true, the PPP authentication protocol to be used is Challenge Handshake Authentication Protocol. This object is applicable only when one of the following rbnBindType values is specified: authBind (2) multiIntfBind (9) multiSubBind (10) When performing a set operation on a row that involves one of these bind types, either the rbnBindAuthChap object or rbnBindAuthPap object or both must be specified. If both the rbnBindAuthChap object and rbnBindAuthPap object are true, then either authentication protocol can be used.
rbnBindAuthPap rbnBindEntry 10 1.3.6.1.4.1.2352.2.17.1.1.1.10 | TruthValue Integer | 1—true 2—false | If the value of this object is true, the PPP authentication protocol to be used is Password Authentication Protocol. This object is applicable only when one of the following rbnBindType values is specified: authBind (2) multiIntfBind (9) multiSubBind (10) When performing a set operation on a row that involves one of these bind types, either the rbnBindAuthChap object or the rbnBindAuthPap object or both must be specified. If both the rbnBindAuthChap object and the rbnBindAuthPap object are true, then either authentication protocol can be used.
rbnBindAuthWait rbnBindEntry 11 1.3.6.1.4.1.2352.2.17.1.1.1.11 | TruthValue Integer | 1—true 2—false | If the value of this object is true, the inbound Challenge-Handshake Authentication Protocol (CHAP) authentication is completed first. That is, after the two sides have decided to use CHAP, the SMS waits for the inbound side to initiate authentication. If the value is true, the rbnBindAuthChap object must also be specified. This object is applicable only when one of the following rbnBindType values is specified: authBind (2) multiIntfBind (9) multiSubBind (10) When performing a set operation on a row that involves this bind type, specification of this column is optional.
rbnBindAuthPapFirst rbnBindEntry 12 1.3.6.1.4.1.2352.2.17.1.1.1.12 | TruthValue Integer | 1—true 2—false | If the value of this object is true, PAP is negotiated before CHAP. If the value of this object is false, CHAP is negotiated before PAP. With SNMP get operations, both the rbnBindAuthChap object and the rbnBindAuthPap object must be true, or this object is not instantiated. With SNMP set operations, if the value of this object is true, both the rbnBindAuthChap object and the rbnBindAuthPap object must also be specified as true. This object is applicable only when one of the following rbnBindType values is specified: authBind (2) multiIntfBind (9) multiSubBind (10) When performing a set operation on a row that involves one of these bind types, specification of this column is optional.
rbnBindMaxSessions rbnBindEntry 13 1.3.6.1.4.1.2352.2.17.1.1.1.13 | Unsigned32 | 1..65535 | The maximum number of concurrent sessions allowed on the circuit; applicable only to circuits that have an encapsulation of type PPPoE. If the circuit is not of this type, then this entry is ignored. This object is applicable only when one of the following rbnBindType values is specified: authBind (2) sessionBind (7) multiIntfBind (9) multiSubBind (10) multiClipsBind (11) The maximum number of concurrent sessions allowed on the circuit depends on the platform, as specified in the following example:
    Platform   Sessions     MemSize
    -------------------------------
    SMS10000       65535
    SMS1800/1000   10000    64MB FE
    SMS1800/1000    8000    48MB FE
    SMS1800/1000    4000    32MB FE
    SMS1800/1000    4000    16MB FE
    SMS1800/1000    4000    8MB FE
    SMS500          2000
rbnBindvcSlot rbnBindEntry 14 1.3.6.1.4.1.2352.2.17.1.1.1.14 | RbnSlot Unsigned32 | 0..255 | Chassis slot number associated with this binding. Use the 'dot1qBind' type for binding an ATM or Frame Relay PVC to an Ethernet port using the specified VLAN ID in the rbnBindVpn object. This object is applicable only when the rbnBindType values is dot1qBind (8).
rbnBindPvcPort rbnBindEntry 15 1.3.6.1.4.1.2352.2.17.1.1.1.15 | RbnPort Unsigned32 | 0..255 | Chassis port number associated with this binding. Use the 'dot1qBind' type for binding an ATM or Frame Relay PVC to an Ethernet port using the specified VLAN ID in the rbnBindVpn object. This object is applicable only when the rbnBindType value is dot1qBind (8).
rbnBindVpn rbnBindEntry 16 1.3.6.1.4.1.2352.2.17.1.1.1.16 | Unsigned32 | 2..4094 | The specific tag to which the PVC is mapped on the specified Ethernet port. Use the 'dot1qBind' type for binding an ATM or Frame Relay PVC to an Ethernet port using the specified VLAN ID in the rbnBindVpn object. This object is applicable only when the rbnBindType value is dot1qBind (8).
rbnBindAuthDhcp rbnBindEntry 17 1.3.6.1.4.1.2352.2.17.1.1.1.17 | TruthValue Integer | 1—true 2—false | If true, specifies an authentication mechanism where the DHCP server makes a request to the authentication subsystem on receipt of incoming DHCP discover packets. This object is applicable only when one of the following rbnBindType values is specified: multiIntfBind (9) multiClipsBind (11) When performing a set operation on a row that involves one of these bind types, if either the rbnBindAuthChap object or the rbnBindAuthPap object or both are specified, the rbnBindAuthDhcp object can not be specified. This object is read-create.

## 1.10 RBN-BRIDGE-MIB

Provides notification when a bridging loop has been detected.

To return information about a specific instance of a bridge in a context, you can use the following syntax during a MIB walk:

    community_string@bridge name@context name

The following sections contain object information for RBN-BRIDGE-MIB.

### 1.10.1 RBN-BRIDGE-MIB Objects

Table 13 describes global objects for RBN-BRIDGE-MIB.

Table 13 objects for RBN-BRIDGE-MIB
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnBridgeNotifyEnable rbnBridgeNotify 1 1.3.6.1.4.1.2352.2.42.1.1.1 | TruthValue Integer | 1—true 2—false | This object provides a mechanism for enabling and disabling bridge circuit state notifications. A value of true indicates that bridge circuit state notifications are enabled. A value of false indicates that bridge circuit state notifications are disabled. This object is read-write.
rbnBridgeGroupName rbnBridgeNotify 2 1.3.6.1.4.1.2352.2.42.1.1.2 | SnmpAdminString | 1..32 | Identifier for the bridge instance. This object is accessible-for-notify.
rbnBridgeCircuitDescriptor rbnBridgeNotify 3 1.3.6.1.4.1.2352.2.42.1.1.3 | SnmpAdminString | 1..255 | A descriptor for identifying the bridge circuit. This object is accessible-for-notify.
rbnBridgeCircuitStatus rbnBridgeNotify 4 1.3.6.1.4.1.2352.2.42.1.1.4 | Integer | 1—blocked 2—cleared | The status of the circuit in the bridge if it is blocked or cleared based on loop detection. This object is accessible-for-notify.
rbnBridgeGroupContextName rbnBridgeNotify 5 1.3.6.1.4.1.2352.2.42.1.1.5 | SnmpAdminString | 1..64 | The context in which the circuit is defined. This object is accessible-for-notify.
rbnBridgePortPreviousState rbnBridgeNotify 6 1.3.6.1.4.1.2352.2.42.1.1.6 | Integer | 1—deleted 2—disabled 3—blocked 4—listening 5—learning 6—forwarding | The state of the bridge port.

### 1.10.2 rbnBridgeIdTable

This table contains the bridge identifier.

`Index:` rbnBridgeName

Table 14 describes the objects in rbnBridgeIdTable.

Table 14 Objects in rbnBridgeIdTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnBridgeName rbnBridgeIdEntry 1 1.3.6.1.4.1.2352.2.42.1.2.1.1.1 | SnmpAdminString | 1..32 | The bridge name. This object is not-accessible.
rbnBridgeId rbnBridgeIdEntry 2 1.3.6.1.4.1.2352.2.42.1.2.1.1.2 | Integer32 | 1..65535 | The bridge identifier referring to this bridge.

### 1.10.3 rbnBridgePortCctDescrTable

This table contains a bridge port number and its circuit description.

`Index`: dot1dBasePort

Table 15 describes the object in rbnBridgePortCctDescrTable.

Table 15 Object in rbnBridgePortCctDescrTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnBridgePortCctDescr rbnBridgePortCctDescrEntry 1 1.3.6.1.4.1.2352.2.42.1.2.2.1.1 | SnmpAdminString | 0..64 | The circuit description of this bridge port.

## 1.11 RBN-BULKSTATS-MIB

Manages bulk-statistics-gathering functions on the SmartEdge router.

The following sections contain information for RBN-BULKSTATS-MIB.

### 1.11.1 RBN-BULKSTATS-MIB Objects

Table 16 describes the global objects for RBN-BULKSTATS-MIB.

Table 16 Global Objects for RBN-BULKSTATS-MIB
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnBulkStatsLastTrfrIpAddrType rbnBulkStatsLastTrfr 1 1.3.6.1.4.1.2352.2.21.1.1.1 | InetAddressType Integer | 0—unknown 1—ipv4 2—ipv6 16—dns | The address type contained in the rbnBulkStatsLastTrfrIpAddr object.
rbnBulkStatsLastTrfrIpAddr rbnBulkStatsLastTrfr 2 1.3.6.1.4.1.2352.2.21.1.1.2 | InetAddress Octet String | 0..255 | The IP Address of the receiver station to which transfer of bulk statistics data was last attempted. If the IP address type is unknown, or if no transfers have occurred, a string of zero (0) length is returned.
rbnBulkStatsLastTrfrStatus rbnBulkStatsLastTrfr 3 1.3.6.1.4.1.2352.2.21.1.1.3 | Integer | 1—none 2—success 3—genError 4—loginFailed 5—badFilename 6—remoteHostFailed 7—other | The status of the last bulk statistics data transfer. none (1): No status information is available. success (2): The data transfer was successful. genError (3): An error was generated. loginFailed (4): Login was unsuccessful. badFilename (5): The file name is incorrect. remoteHostFailed (6): Connecting to the remote host failed. other (7): Data transfer generated an other return value.

### 1.11.2 rbnBulkStatsLastTrfrTable

This table monitors the last attempted transfer of the bulk statistics data for each bulkstats policy. All rows in this table are accessible when the context 'local' is specified in the SNMP message. SNMP requests using other contexts return only the row that matches the context.

`Index:` vacmContextName, rbnBulkStatsLastTrfrPolicy

Table 17 describes the objects in rbnBulkStatsLastTrfrTable.

Table 17 Objects in rbnBulkStatsLastTrfrTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnBulkStatsLastTrfrPolicy rbnBulkStatsLastTrfrEntry 1 1.3.6.1.4.1.2352.2.21.1.1.4.1.1 | SnmpAdminString Octet String | 1..20 | The name of the bulkstats policy.
rbnBulkStatsLastTrfrIpAddrType2 rbnBulkStatsLastTrfrEntry 2 1.3.6.1.4.1.2352.2.21.1.1.4.1.2 | InetAddressType Integer | 0—unknown 1—ipv4 2—ipv6 6—dns | The address type contained in the rbnBulkStatsLastTrfrIpAddr2 object.
rbnBulkStatsLastTrfrIpAddr2 rbnBulkStatsLastTrfrEntry 3 1.3.6.1.4.1.2352.2.21.1.1.4.1.3 | InetAddress Octet String | 0..255 | The IP Address of the receiver station to which transfer of bulk statistics data was last attempted. If the IP address type is unknown, or if no transfers have occurred, a string of zero (0) length is returned.
rbnBulkStatsLastTrfrStatus2 rbnBulkStatsLastTrfrEntry 4 1.3.6.1.4.1.2352.2.21.1.1.4.1.4 | Integer | 1—none 2—success 3—genError 4—loginFailed 5—badFilename 6—remoteHostFailed 7—other | The status of the last bulk statistics data transfer. none (1): No status information is available. success (2): The data transfer was successful. genError (3): An error was generated. loginFailed (4): Login was unsuccessful. badFilename (5): The file name is incorrect. remoteHostFailed (6): Connecting to the remote host failed. other (7): Data transfer generated an other return value.

## 1.12 RBN-CARDMON-MIB

Manages the controller, alarm, and traffic card alarm functions. For a list of controller and traffic card alarms supported by this MIB, refer to the MIBs capability (CAP) file.

The following sections contain object information for RBN-CARDMON-MIB.

### 1.12.1 rbnCardAlarmActiveTable

This table contains the card alarms currently active on the system.

`Index`: rbnCardAlarmSlot, rbnCardAlarmActiveIndex

Table 18 describes the objects in rbnCardAlarmActiveTable.

Table 18 Objects in rbnCardAlarmActiveTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnCardAlarmSlot rbnCardAlarmActiveEntry 1 1.3.6.1.4.1.2352.2.31.1.1.1.1 | RbnSlot Unsigned32 | 0..255 | The chassis slot number in which the card is present.
rbnCardAlarmActiveIndex rbnCardAlarmActiveEntry 2 1.3.6.1.4.1.2352.2.31.1.1.1.2 | Unsigned32 | 1..4294967295 | A monotonically increasing integer index. It wraps back to 1 after it reaches its maximum value.
rbnCardAlarmId rbnCardAlarmActiveEntry 3 1.3.6.1.4.1.2352.2.31.1.1.1.3 | RbnAlarmId | Integer | An identifier for the alarm. See Section 1.43.1 RbnAlarmId for details.
rbnCardAlarmType rbnCardAlarmActiveEntry 4 1.3.6.1.4.1.2352.2.31.1.1.1.4 | RbnAlarmType Integer | 1—11 | The type of the alarm. See Section 1.43.3 RbnAlarmType for details.
rbnCardAlarmDateAndTime rbnCardAlarmActiveEntry 5 1.3.6.1.4.1.2352.2.31.1.1.1.5 | DateAndTime Octet String | SIZE (8) | The local date and time when the alarm was raised. The value range indicates 8 or 11 characters to display the time-zone information.
rbnCardAlarmDescription rbnCardAlarmActiveEntry 6 1.3.6.1.4.1.2352.2.31.1.1.1.6 | SnmpAdmin String | 0..64 | A text string that conveys additional information about the alarm.
rbnCardAlarmProbableCause rbnCardAlarmActiveEntry 7 1.3.6.1.4.1.2352.2.31.1.1.1.7 | RbnAlarm ProbableCause | Integer | The probable cause for this alarm.
rbnCardAlarmSeverity rbnCardAlarmActiveEntry 8 1.3.6.1.4.1.2352.2.31.1.1.1.8 | RbnAlarmPerceivedSeverity | Integer | The perceived severity of the alarm. See Section 1.43.9 RbnAlarmPerceivedSeverity for details.
rbnCardAlarmServiceAffecting rbnCardAlarmActiveEntry 9 1.3.6.1.4.1.2352.2.31.1.1.1.9 | RbnAlarmServiceAffecting Integer | 1—yes 2—no | Indicates whether the alarm is perceived to impact service.

### 1.12.2 rbnCardStatsTable

This table contains statistics for each traffic card and provides an entry for the card that contains the Ethernet management port.

`Index:` rbnCardStatsSlot

Table 19 describes the objects in rbnCardStatsTable.

Table 19 Objects in rbnCardStatsTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnCardStatsSlot rbnCardStatsEntry 1 1.3.6.1.4.1.2352.2.31.1.2.1.1 | rbnSlot Unsigned32 | 0..255 | The chassis slot number in which the card is present.
rbnCardStatsTotalCircuits rbnCardStatsEntry 2 1.3.6.1.4.1.2352.2.31.1.2.1.2 | Gauge32 | N/A | Number of circuits configured on the card.
rbnCardStatsUpCircuits rbnCardStatsEntry 3 1.3.6.1.4.1.2352.2.31.1.2.1.3 | Gauge32 | N/A | Number of circuits in an up state configured on the card.
rbnCardStatsDownCircuits rbnCardStatsEntry 4 1.3.6.1.4.1.2352.2.31.1.2.1.4 | Gauge32 | N/A | Number of circuits in a down state configured on the card.
rbnCardStatsUnboundCircuits rbnCardStatsEntry 5 1.3.6.1.4.1.2352.2.31.1.2.1.5 | Gauge32 | N/A | Number of circuits not bound to an interface that are configured on the card.
rbnCardStatsNoBindCircuits rbnCardStatsEntry 6 1.3.6.1.4.1.2352.2.31.1.2.1.6 | Gauge32 | N/A | Number of circuits configured on the card that are not bound to an interface and are not subscriber or CLIPS circuits.
rbnCardStatsBindTotalCircuits rbnCardStatsEntry 7 1.3.6.1.4.1.2352.2.31.1.2.1.7 | Gauge32 | N/A | Number of circuits bound to an interface that are configured on the card.
rbnCardStatsBindIfCircuits rbnCardStatsEntry 8 1.3.6.1.4.1.2352.2.31.1.2.1.8 | Gauge32 | N/A | Number of circuits configured on the card that are bound to an interface and are not subscriber circuits.
rbnCardStatsBindAuthCircuits rbnCardStatsEntry 9 1.3.6.1.4.1.2352.2.31.1.2.1.9 | Gauge32 | N/A | Number of subscriber and CLIPS bind authentication circuits configured on the card.
rbnCardStatsBindSubCircuits rbnCardStatsEntry 10 1.3.6.1.4.1.2352.2.31.1.2.1.10 | Gauge32 | N/A | Number of bind subscriber, including CLIPS, and bind auto-subscriber circuits configured on the card.
rbnCardStatsAtmCircuits rbnCardStatsEntry 11 1.3.6.1.4.1.2352.2.31.1.2.1.11 | Gauge32 | N/A | Number of ATM circuits configured on the card.
rbnCardStatsEthCircuits rbnCardStatsEntry 12 1.3.6.1.4.1.2352.2.31.1.2.1.12 | Gauge32 | N/A | Number of Ethernet circuits configured on the card.
rbnCardStatsPppCircuits rbnCardStatsEntry 13 1.3.6.1.4.1.2352.2.31.1.2.1.13 | Gauge32 | N/A | Number of PPP circuits configured on the card.
rbnCardStatsPppoeCircuits rbnCardStatsEntry 14 1.3.6.1.4.1.2352.2.31.1.2.1.14 | Gauge32 | N/A | Number of PPPoE circuits configured on the card.
rbnCardStatsDot1qCircuits rbnCardStatsEntry 15 1.3.6.1.4.1.2352.2.31.1.2.1.15 | Gauge32 | N/A | Number of 802.1Q circuits configured on the card.
rbnCardStatsFrCircuits rbnCardStatsEntry 16 1.3.6.1.4.1.2352.2.31.1.2.1.16 | Gauge32 | N/A | Number of Frame Relay circuits configured on the card.
rbnCardStatsChdlcCircuits rbnCardStatsEntry 17 1.3.6.1.4.1.2352.2.31.1.2.1.17 | Gauge32 | N/A | Number of Cisco HDLC circuits configured on the card.
rbnCardStatsGreCircuits rbnCardStatsEntry 18 1.3.6.1.4.1.2352.2.31.1.2.1.18 | Gauge32 | N/A | Number of GRE circuits configured on the card.
rbnCardStatsMplsCircuits rbnCardStatsEntry 19 1.3.6.1.4.1.2352.2.31.1.2.1.19 | Gauge32 | N/A | Number of MPLS circuits configured on the card.
rbnCardStatsClipsCircuits rbnCardStatsEntry 20 1.3.6.1.4.1.2352.2.31.1.2.1.20 | Gauge32 | N/A | Number of CLIPS circuits configured on the card.
rbnCardStatsVplsCircuits rbnCardStatsEntry 21 1.3.6.1.4.1.2352.2.31.1.2.1.21 | Gauge32 | N/A | Number of VPLS circuits configured on the card.
rbnCardStatsIpipCircuits rbnCardStatsEntry 22 1.3.6.1.4.1.2352.2.31.1.2.1.22 | Gauge32 | N/A | Number of IP-in-IP tunnel circuits configured on the card.
rbnCardStatsIpv6v4ManualCircuits rbnCardStatsEntry 23 1.3.6.1.4.1.2352.2.31.1.2.1.23 | Gauge32 | N/A | Number of IPv6v4-manual tunnel circuits configured on the card.
rbnCardStatsIpv6v4AutoCircuits rbnCardStatsEntry 24 1.3.6.1.4.1.2352.2.31.1.2.1.24 | Gauge32 | N/A | Number of IPv6v4-auto tunnel circuits configured on the card.

### 1.12.3 Example: Obtaining Tunnel Circuit Count

RBN-CARDMON-MIB can be used to obtain 802.1q PVC tunnel circuit count for each slot for trending analysis. The rbnCardStatsTable is indexed by slot number.

The following example gets a slot-level count for a specific circuit type:

    sh-3.00$ snmpbulkwalk -v2c -cpublic -m RBN-CARDMON-MIB SE-lab2 rbnCardStatsDot1qCircuits

    RBN-CARDMON-MIB::rbnCardStatsDot1qCircuits.7 = Gauge32: 0

    RBN-CARDMON-MIB::rbnCardStatsDot1qCircuits.11 = Gauge32: 2

Use the following CLI to view circuit information:

    [local]Redback#show circuit summary
    Summary:
    total: 7
    up: 7        down: 0
    bound: 5     unbound: 2
    auth: 0      interface: 5   subscriber: 0    bypass: 0
    no-bind: 2   atm: 0         chdlc: 0         dot1q: 2
    ether: 3     fr: 0          gre: 0
    mpls: 0      ppp: 0         pppoe: 0
    clips: 0     vpls: 0        ipip: 0
    ipsec: 2     ipv6v4-man: 0  ipv6v4-auto: 0
    [local]Redback#

## 1.13 RBN-CES-MIB

This MIB describes objects used to manage Circuit Emulation Service (CES) protocols, including RFC 5086, `Structure-Aware Time Division Multiplexed (TDM) Circuit Emulation Service over Packet Switched Network (CESoPSN)` and RFC 4553, `Structure Agnostic Circuit Emulation Service over Packet Switch Network (SAToP)`.

### 1.13.1 CES Global Object Definitions

Table 20 describes the CES global object.

Table 20 CES Global Objects
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnCesSlaInfoResetAll rbnCesMIBObjects 1 1.3.6.1.4.1.2352.2.56.1.2 | TruthValue | 1—true 2—false | Setting this object to "'true" resets all CES Service Level Agreement (SLA) information objects in the rbnCesSlaInfoTable. When set, object always returns "false" as a value.

### 1.13.2 rbnCesCfgTable

This table provides a collection of CES configuration objects.

`Index:` rbnCesCfgIndex

Table 21 describes the objects in rbnCesCfgTable.

Table 21 Objects in rbnCesCfgTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnCesCfgIndex rbnCesCfgEntry 1 1.3.6.1.4.1.2352.2.56.1.2.1.1 | InterfaceIndex | 1..2147483647 | This object is used to uniquely identify a CES circuit. The value of this object should be the same as the value of ifIndex when they are both used to identify the same CES interface.
rbnCesCfgPktLatency rbnCesCfgEntry 2 1.3.6.1.4.1.2352.2.56.1.2.1.2 | Unsigned32 | 0..4294967295 | This object specifies the time, in microseconds, required for packetizing frames into a packet. The packet latency is calculated by multiplying number of frames by a constant frame packetization time (125 microseconds). The system packetizes eight frames into a packet by default. Default value is 1000.
rbnCesCfgJtrBfrDepth rbnCesCfgEntry 3 1.3.6.1.4.1.2352.2.56.1.2.1.3 | Unsigned32 | 0..4294967295 | The number of microseconds of expected packet delay variation for this CES PW over PSN. The value must be at least two times the expected packet jitter through the network. Default value is 5000.
rbnCesCfgConsecPktsInSync rbnCesCfgEntry 4 1.3.6.1.4.1.2352.2.56.1.2.1.4 | Unsigned32 | 0..4294967295 | The number of consecutive packets that are required to exit a loss-of-packet state (LOPS). Default value is 10.
rbnCesCfgConsecMissPktsOutSync rbnCesCfgEntry 5 1.3.6.1.4.1.2352.2.56.1.2.1.5 | Unsigned32 | 0..4294967295 | The number of consecutive missing packets that are required to enter a loss-of-packet state (LOPS). Default value is 1.
rbnCesCfgIdlePattern rbnCesCfgEntry 6 1.3.6.1.4.1.2352.2.56.1.2.1.6 | Octet String | 0x54(E1) or 0x3F(T1) | This object determines the value to be used on the TDM channel when packets have over/underflow in the jitter buffer or are missing for any reason at the CES bound. The default value for E1 is 0x54; for T1, it is 0x3F.
rbnCesCfgTrunkCtl rbnCesCfgEntry 7 1.3.6.1.4.1.2352.2.56.1.2.1.7 | TruthValue | 1—true 2—false | This object enforces the RFC 5086 requirement that controls at most one CES PW state (AIS or RDI) on the outgoing T1/E1 trunk. Default value is 2 (false).
rbnCesCfgAdminStatus rbnCesCfgEntry 8 1.3.6.1.4.1.2352.2.56.1.2.1.8 | Integer | 1—up 2—down | This object controls the CES feature on the circuit. Setting this object to 'up' (1) enables CES on the circuit; setting this object to 'down' (2) disables CES on the circuit and removes corresponding entries in the rbnCesStatsTable, rbnCesEplStatsTable, and rbnCesSlaInfoTable. To modify other read-create objects in the conceptual row, this object must be set to 'down'. The value of the rbnCesCfgRowStatus object must be 'active' (1) in order for this object to be set to 'up'. Default value is 2 (down).
rbnCesCfgRowStatus rbnCesCfgEntry 9 1.3.6.1.4.1.2352.2.56.1.2.1.9 | Integer | 1—active 2—down 3—not ready 4—createAndGo 5—createAndWait 6—destroy | This object is used to manage the creation and deletion of CES configuration conceptual rows. Except for the rbnCesCfgAdminStatus object, read-create objects in the conceptual row cannot be modified while this object is set to 'active' (1). To change this object from 'active' to a different value, the rbnCesCfgAdminStatus object must be set to 'down' (2). To create an entry in this table, set this object to either createAndGo (4) or createAndWait (5). To delete an entry in this table, set this object to destroy (6). Until all objects in the conceptual row are appropriately configured, this object automatically transitions to notReady (3). There is no default value.

### 1.13.3 1.18.1 rbnCesStatsTable

This table provides a collection of CES statistics objects.

Table 22 describes the objects in rbnCesStatsTable.

Table 22 Objects in rbnCesStatsTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnCesStatsEgressOutOfBfrDroppedPkts rbnCesStatsEntry 1 1.3.6.1.4.1.2352.2.56.1.3.1.1 | Counter64 | 0..18446744073709551615 | Number of packets dropped due to buffer starvation in the PSN to TDM direction (egress).
rbnCesStatsEgressMissingPkts rbnCesStatsEntry 2 1.3.6.1.4.1.2352.2.56.1.3.1.2 | Counter64 | 0..18446744073709551615 | Number of missing packets detected through control word sequence number gaps in the PSN to TDM direction (egress).
rbnCesStatsEgressMalformedPkts rbnCesStatsEntry 3 1.3.6.1.4.1.2352.2.56.1.3.1.3 | Counter64 | 0..18446744073709551615 | Number of malformed packets, including unexpected size in the PSN to TDM direction (egress).
rbnCesStatsEgressJtrBfrOverrunPkts rbnCesStatsEntry 4 1.3.6.1.4.1.2352.2.56.1.3.1.4 | Counter64 | 0..18446744073709551615 | Number of packets dropped due to jitter buffer overrun in the PSN to TDM direction (egress).
rbnCesStatsEgressJtrBfrUnderruns rbnCesStatsEntry 5 1.3.6.1.4.1.2352.2.56.1.3.1.5 | Counter64 | 0..18446744073709551615 | Number of times jitter buffer underrun has been detected in the PSN to TDM direction (egress).
rbnCesStatsEgressMisOrderPkts rbnCesStatsEntry 6 1.3.6.1.4.1.2352.2.56.1.3.1.6 | Counter64 | 0..18446744073709551615 | Number of out of sequence packets received in the PSN to TDM direction (egress).
rbnCesStatsEgressRemoteLossPkts rbnCesStatsEntry 7 1.3.6.1.4.1.2352.2.56.1.3.1.7 | Counter64 | 0..18446744073709551615 | Number of packets received with the R bit set in the PSN to TDM direction (egress).
rbnCesStatsEgressWindowSwitchovers rbnCesStatsEntry 8 1.3.6.1.4.1.2352.2.56.1.3.1.8 | Counter64 | 0..18446744073709551615 | Number of times the serial number lost synchronization and was forced to move to a new window in the PSN to TDM direction (egress).
rbnCesStatsEgressRemoteAcDownPkts rbnCesStatsEntry 9 1.3.6.1.4.1.2352.2.56.1.3.1.9 | Counter64 | 0..18446744073709551615 | Number of packets received with L bit set to 1, indicating that the far end's attachment circuit is down (in LOF or LOS or AIS) in the PSN to TDM direction (egress). Either AIS or idle pattern was played out on the local access circuit.
rbnCesStatsEgressDuplicatePkts rbnCesStatsEntry 10 1.3.6.1.4.1.2352.2.56.1.3.1.10 | Counter64 | 0..18446744073709551615 | Number of packets dropped due to being duplicated, as determined by the PW codeword sequence number in the PSN to TDM direction (egress).
rbnCesStatsEgressDeniedPkts rbnCesStatsEntry 11 1.3.6.1.4.1.2352.2.56.1.3.1.11 | Counter64 | 0..18446744073709551615 | Number of packets dropped because they are denied in the PSN to TDM direction (egress).
rbnCesStatsEgressErrorEvents rbnCesStatsEntry 12 1.3.6.1.4.1.2352.2.56.1.3.1.12 | Counter64 | 0..18446744073709551615 | Number of times a packet is replaced with a dummy packet in the PSN to TDM direction (egress) because the system is in underrun mode or the packet was lost.
rbnCesStatsEgressErrorDataBlocks rbnCesStatsEntry 13 1.3.6.1.4.1.2352.2.56.1.3.1.13 | Counter64 | 0..18446744073709551615 | Block of data transmitted to the TDM attachment circuit and of a size defined in accordance with the rules specified in ITU-T G.826 `Error performance parameters and objectives for international, constant bit rate digital paths at or above the primary rate` for the corresponding TDM service that has undergone at least one CESoPSN/SAToP error event in the PSN to TDM direction (egress). For example, consider a T1/E1 Attachment Circuit Error Data Block for T1 = Error Event * (192 * Packet Latency) Error Data Block for E1 = Error Event * (256 * Packet Latency)
rbnCesStatsIngressOutOfBfrDroppedPkts rbnCesStatsEntry 14 1.3.6.1.4.1.2352.2.56.1.3.1.14 | Counter64 | 0..18446744073709551615 | Number of packets that could not be sent due to buffer starvation in the PSN to TDM direction (egress).
rbnCesStatsIngressSizeViolationDroppedPkts rbnCesStatsEntry 15 1.3.6.1.4.1.2352.2.56.1.3.1.15 | Counter64 | 0..18446744073709551615 | Number of packets not transmitted because their size is greater than the largest supported in the PSN to TDM direction (egress).
rbnCesStatsIngressTransmitDroppedPkts rbnCesStatsEntry 16 1.3.6.1.4.1.2352.2.56.1.3.1.16 | Counter64 | 0..18446744073709551615 | Number of packets not transmitted due to congestion in the transmit queue in the PSN to TDM direction (egress).

### 1.13.4 rbnCesEplCfgTable

This table provides a collection of CES excessive packet loss configuration objects.

`Index:` rbnCesEplCfgIndex

Table 23 describes the objects in rbnCesEplCfgTable.

Table 23 Objects in rbnCesEplCfgTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnCesEplCfgIndex rbnCesEplCfgEntry 1 1.3.6.1.4.1.2352.2.56.1.4.1.1 | Integer32 | 1..2147483647 | This object is used to uniquely identify a set of CES excessive packet loss configuration.
rbnCesEplCfgThreshold rbnCesEplCfgEntry 2 1.3.6.1.4.1.2352.2.56.1.4.1.2 | RbnPercentage | 0..100 | Threshold in percentage representing the upper limits of measurement for excessive packet loss. It is the ratio of (Total Lost Packets) / (Total Transmitted Packets).
rbnCesEplCfgFaultDeclarationTime rbnCesEplCfgEntry 3 1.3.6.1.4.1.2352.2.56.1.4.1.3 | Unsigned32 | 0..4294967295 | This object controls fault declaration time of excessive packet loss alarm. It is a successive duration that experience excessive packet loss defect. Default value is 2500 milliseconds.
rbnCesEplCfgClearingTime rbnCesEplCfgEntry 4 1.3.6.1.4.1.2352.2.56.1.4.1.4 | Unsigned32 | 0..4294967295 | This object controls how excessive packet loss alarms are cleared. The counter represents the number of successive periods of duration `t` that do not experience an excessive packet loss defect, where `t`is a system constant of 25 milliseconds. Default value is 10000 milliseconds.
rbnCesEplCfgStatsResetAll rbnCesEplCfgEntry 5 1.3.6.1.4.1.2352.2.56.1.4.1.5 | TruthValue | 1—true 2—false | Setting this object to "true" resets all CES excessive packet loss statistic objects in the rbnCesEplStatsTable object. When set, this object always returns a value of "false." Default is false (2).
rbnCesEplCfgAdminStatus rbnCesEplCfgEntry 6 1.3.6.1.4.1.2352.2.56.1.4.1.6 | Integer | 1—up 2—down | This object controls the excessive packet loss configurations. Setting this object to 'up' (1) enables CES excessive packet loss monitoring on all CES circuits in the system; setting this object to 'down' (2) disables the feature and removes all entries in the rbnCesEplStatsTable. Only one active CES excessive packet loss configuration is allowed. To modify other 'read-create' objects in the conceptual row, the rbnCesEplCfgAdminStatus object must be set to 'down'. The value of the 'rbnCesEplCfgRowStatus' object must be 'active' (1) in order for this object to be set to 'up'. Default value is 2 (down).
rbnCesEplCfgRowStatus rbnCesEplCfgEntry 7 1.3.6.1.4.1.2352.2.56.1.4.1.7 | Integer | 1—active 2—down 3—not ready 4—createAndGo 5—createAndWait 6—destroy | This object is used to manage the creation and deletion of CES excessive packet loss configuration conceptual rows. Except for the rbnCesEplCfgAdminStatus object, 'read-create' objects in the conceptual row cannot be modified while this object is set to active (1). To change this object from 'active' to a different value, the rbnCesEplCfgAdminStatus object must be 'down' (2). To create a row in this table, set this object to either 'createAndGo' (4) or 'createAndWait' (5). To delete an entry in this table, set this object to destroy (6). Until all objects in the conceptual row are appropriately configured, this object will transit to 'notReady' (3).

### 1.13.5 rbnCesEplStatsTable

This table provides a collection of CES excessive packet loss statistics.

Table 24 describes the objects in rbnCesEplStatsTable.

Table 24 Objects in rbnCesEplStatsTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnCesEplStatsIndex rbnCesEplStatsEntry 1 1.3.6.1.4.1.2352.2.56.1.5.1.1 | InterfaceIndex | 1..2147483647 | This object is used to uniquely identify a CES circuit. The value of this object should be the same as the value of ifIndex when they are used to identify the same CES circuit.
rbnCesEplStatsEntryTime rbnCesEplStatsEntry 2 1.3.6.1.4.1.2352.2.56.1.5.1.2 | DateAndTime Octet String | SIZE (8) | Date and time when the current excessive packet loss snapshot starts.
rbnCesEplStatsEntryTotalPktLossTime rbnCesEplStatsEntry 3 1.3.6.1.4.1.2352.2.56.1.5.1.3 | TimeInterval | 0..2147483647 | The entry total packet loss time of current excessive packet loss snapshot. Value is measured in units of 0.01 seconds.
rbnCesEplStatsExitTime rbnCesEplStatsEntry 4 1.3.6.1.4.1.2352.2.56.1.5.1.4 | TimeInterval | 0..2147483647 | The exit packet loss time of current excessive packet loss snapshot. Value is measured in units of 0.01 seconds.
rbnCesEplStatsExitTotalPktLossTime rbnCesEplStatsEntry 5 1.3.6.1.4.1.2352.2.56.1.5.1.5 | TimeInterval | 0..2147483647 | The exit total packet loss time of current excessive packet loss snapshot. Value is measured in units of 0.01 seconds.
rbnCesEplStatsCount rbnCesEplStatsEntry 6 1.3.6.1.4.1.2352.2.56.1.5.1.6 | Gauge32 | 0..4294967295 | The total number of times the CES PW was in excessive packet loss defect.
rbnCesEplStatsTotalCircuitTime rbnCesEplStatsEntry 7 1.3.6.1.4.1.2352.2.56.1.5.1.7 | TimeInterval | 0..2147483647 | Total CES PW up-time, including CES PW up-time and time spent in excessive packet loss state.
rbnCesEplStatsTotalFailureRate rbnCesEplStatsEntry 8 1.3.6.1.4.1.2352.2.56.1.5.1.8 | RbnPercentage | 0..100 | The percentage of time the CES PW spent in the excessive packet loss state during the total CES PW time.
rbnCesEplStatsReset rbnCesEplStatsEntry 9 1.3.6.1.4.1.2352.2.56.1.5.1.9 | TruthValue | 1—true 2—false | This object is used to reset CES EPL statistic objects in the entry. Setting this object to "true" resets the rbnCesEplStatsEntryTime object to the current time and sets other CES EPL statistic objects to zero. When set, this object always returns a value of "false." Default is false (2).

### 1.13.6 rbnCesSlaInfoTable

This table provides a collection of CES Service Level Agreement (SLA) information objects.

`Index:` rbnCesSlaInfoIndex

Table 25 describes the objects in rbnCesSlaInfoTable.

Table 25 Objects in rbnCesSlaInfoTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnCesSlaInfoIndex rbnCesSlaInfoEntry 1 1.3.6.1.4.1.2352.2.56.1.6.1.1 | InterfaceIndex | 1..2147483647 | This object is used to uniquely identify a CES circuit. The value of this object should be the same as the value of ifIndex when they are both used to identify the same CES interface.
rbnCesSlaInfoLatestOutageTime rbnCesSlaInfoEntry 2 1.3.6.1.4.1.2352.2.56.1.6.1.2 | TimeInterval | 0..2147483647 | The amount time during the latest occurrence when the CES PW was in a packet loss or underrun state. Value is measured in units of 0.01 seconds.
rbnCesSlaInfoEntryLatestOutage rbnCesSlaInfoEntry 3 1.3.6.1.4.1.2352.2.56.1.6.1.3 | DateAndTime Octet String | SIZE (8) | Date and time of the most recent occurrence when the CES PW entered the packet loss or underrun state.
rbnCesSlaInfoExitLatestOutage rbnCesSlaInfoEntry 4 1.3.6.1.4.1.2352.2.56.1.6.1.4 | DateAndTime Octet String | SIZE (8) | Date and time of the most recent occurrence when the CES PW exited the packet loss or underrun state. NOTE: All fields of the DateAndTime MUST be filled out, including the hours and minutes from UTC.
rbnCesSlaInfoLastOutageTime rbnCesSlaInfoEntry 5 1.3.6.1.4.1.2352.2.56.1.6.1.5 | TimeInterval | 0..2147483647 | The duration of the previous occurrence (the one prior to the most recent occurrence) when the CES PW was in the packet loss or underrun state. Value is measured in units of 0.01 seconds.
rbnCesSlaInfoLastUpTime rbnCesSlaInfoEntry 6 1.3.6.1.4.1.2352.2.56.1.6.1.6 | TimeInterval | 0..2147483647 | Total CES PW up time before the most recent outage occurred. Value is measured in units of 0.01 seconds.
rbnCesSlaInfoTotalOutageTime rbnCesSlaInfoEntry 7 1.3.6.1.4.1.2352.2.56.1.6.1.7 | TimeInterval | 0..2147483647 | Total outage time since the CES PW was created. Value is measured in units of 0.01 seconds.
rbnCesSlaInfoTotalUpTime rbnCesSlaInfoEntry 8 1.3.6.1.4.1.2352.2.56.1.6.1.8 | TimeInterval | 0..2147483647 | Total CES PW up time since the CES PW was created, excluding the cumulative outage time. Value is measured in units of 0.01 seconds.
rbnCesSlaInfoOutageCount rbnCesSlaInfoEntry 9 1.3.6.1.4.1.2352.2.56.1.6.1.9 | Gauge32 | 0..4294967295 | Number of times a CES PW outage occurred.
rbnCesSlaInfoReset rbnCesSlaInfoEntry 10 1.3.6.1.4.1.2352.2.56.1.6.1.10 | TruthValue | 1—true 2—false | Setting this object to "true" resets CES SLA objects to zero. When set, this object always returns a value of "false." Default is false (2).

### 1.13.7 rbnCesCardAlarmTable

Table 20 describes the CES card alarm table object. This table consists of CES-specific card alarms; these alarms are used to indicate CES card-level communication errors. (Other card alarms are not included in the table.)

Table 26 Objects in rbnCesCardAlarmTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnCesCardAlarmId | RbnAlarmId | Integer | This object is used to uniquely identify a CES card alarm.
rbnCesCardAlarmNotificationEnable rbnCesCardAlarmEntry 2 1.3.6.1.4.1.2352.2.56.1.7.1.2 | TruthValue | 1—true 2—false | This object indicates whether the rbnCardAlarm notification is to be generated. If set to "true," a notification is generated for the card alarm specified by the rbnCesCardAlarmId object. Otherwise, no notification is generated. Default is false (2.)

## 1.14 RBN-CIRCUIT-GROUP-MIB

Defines the objects used to monitor circuit group policies.

The following sections contain object information for RBN-CIRCUIT-GROUP-MIB.

### 1.14.1 rbnCircuitGroupStatsTable

This table contains various transmit, receive, and drop counters for each circuit group.

`Index:` rbnCctGrpName

Table 27 describes the objects in rbnCircuitGroupStatsTable.

Table 27 Objects in rbnCircuitGroupStatsTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnCctGrpName rbnCircuitGroupStatsEntry 1 1.3.6.1.4.1.2352.2.43.1.1.1.1 | SnmpAdminString Octet String | 1..80 | The name of the hierarchical group.
rbnCctGrpTxOctets rbnCircuitGroupStatsEntry 2 1.3.6.1.4.1.2352.2.43.1.1.1.2 | Counter64 | 0..18446744073709551615 | Number of octets transmitted by the group including its children.
rbnCctGrpTxPackets rbnCircuitGroupStatsEntry 3 1.3.6.1.4.1.2352.2.43.1.1.1.3 | Counter64 | 0..18446744073709551615 | Number of packets transmitted by the group including its children.
rbnCctGrpTxMulticastOctets rbnCircuitGroupStatsEntry 4 1.3.6.1.4.1.2352.2.43.1.1.1.4 | Counter64 | 0..18446744073709551615 | Number of multicast octets transmitted by the group including its children.
rbnCctGrpTxMulticastPackets rbnCircuitGroupStatsEntry 5 1.3.6.1.4.1.2352.2.43.1.1.1.5 | Counter64 | 0..18446744073709551615 | Number of multicast packets transmitted by the group including its children.
rbnCctGrpRxOctets rbnCircuitGroupStatsEntry 6 1.3.6.1.4.1.2352.2.43.1.1.1.6 | Counter64 | 0..18446744073709551615 | Number of octets received by the group including its children.
rbnCctGrpRxPackets rbnCircuitGroupStatsEntry 7 1.3.6.1.4.1.2352.2.43.1.1.1.7 | Counter64 | 0..18446744073709551615 | Number of packets received by the group including its children.
rbnCctGrpRxMulticastOctets rbnCircuitGroupStatsEntry 8 1.3.6.1.4.1.2352.2.43.1.1.1.8 | Counter64 | 0..18446744073709551615 | Number of multicast octets received by the group including its children.
rbnCctGrpRxMulticastPackets rbnCircuitGroupStatsEntry 9 1.3.6.1.4.1.2352.2.43.1.1.1.9 | Counter64 | 0..18446744073709551615 | Number of multicast packets received by the group including its children.
rbnCctGrpAdjDroppedOctets rbnCircuitGroupStatsEntry 10 1.3.6.1.4.1.2352.2.43.1.1.1.10 | Counter64 | 0..18446744073709551615 | Number of adjacency octets dropped.
rbnCctGrpAdjDroppedPackets rbnCircuitGroupStatsEntry 11 1.3.6.1.4.1.2352.2.43.1.1.1.11 | Counter64 | 0..18446744073709551615 | Number of adjacency packets dropped.
rbnCctGrpDownDroppedOctets rbnCircuitGroupStatsEntry 12 1.3.6.1.4.1.2352.2.43.1.1.1.12 | Counter64 | 0..18446744073709551615 | Number of down octets dropped.
rbnCctGrpDownDroppedPackets rbnCircuitGroupStatsEntry 13 1.3.6.1.4.1.2352.2.43.1.1.1.13 | Counter64 | 0..18446744073709551615 | Number of down packets dropped.
rbnCctGrpUnreachDroppedOctets rbnCircuitGroupStatsEntry 14 1.3.6.1.4.1.2352.2.43.1.1.1.14 | Counter64 | 0..18446744073709551615 | Number of unreachable octets dropped.
rbnCctGrpUnreachDroppedPackets rbnCircuitGroupStatsEntry 15 1.3.6.1.4.1.2352.2.43.1.1.1.15 | Counter64 | 0..18446744073709551615 | Number of unreachable packets dropped.
rbnCctGrpUnknownEncapsOctets rbnCircuitGroupStatsEntry 16 1.3.6.1.4.1.2352.2.43.1.1.1.16 | Counter64 | 0..18446744073709551615 | Number octets dropped due to unknown encapsulation.
rbnCctGrpUnknownEncapsPackets rbnCircuitGroupStatsEntry 17 1.3.6.1.4.1.2352.2.43.1.1.1.17 | Counter64 | 0..18446744073709551615 | Number of packets dropped due to unknown encapsulation.

### 1.14.2 rbnCircuitGroupQTable

This table contains various counters for each transmit queue assigned to a circuit group.

Note:
  Discontinuities in the value of the type counter64 can occur at reinitialization of the management system.

`Index:` rbnCctGrpName, rbnCctGrpQueueId

Table 28 describes the objects in rbnCircuitGroupQTable.

Table 28 Objects in rbnCircuitGroupQTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnCctGrpQueueId rbnCircuitGroupQEntry 1 1.3.6.1.4.1.2352.2.43.1.2.1.1 | Unsigned32 | 0..7 | A unique identifier for a transmit queue used by the circuit.
rbnCctGrpQTxOctets rbnCircuitGroupQEntry 2 1.3.6.1.4.1.2352.2.43.1.2.1.2 | Counter64 | 0..18446744073709551615 | Number of octets transmitted out of this queue.
rbnCctGrpQTxPackets rbnCircuitGroupQEntry 3 1.3.6.1.4.1.2352.2.43.1.2.1.3 | Counter64 | 0..18446744073709551615 | Number of packets transmitted out of this queue.
rbnCctGrpQWredDroppedOctets rbnCircuitGroupQEntry 4 1.3.6.1.4.1.2352.2.43.1.2.1.4 | Counter64 | 0..18446744073709551615 | Number of octets dropped due to the application of a weighted random early detection (WRED) algorithm.
rbnCctGrpQWredDroppedPkts rbnCircuitGroupQEntry 5 1.3.6.1.4.1.2352.2.43.1.2.1.5 | Counter64 | 0..18446744073709551615 | Number of packets dropped due to the application of a WRED algorithm.
rbnCctGrpQTailDroppedOctets rbnCircuitGroupQEntry 6 1.3.6.1.4.1.2352.2.43.1.2.1.6 | Counter64 | 0..18446744073709551615 | Number of octets dropped when the total number of packets in this queue is greater than the maximum threshold.
rbnCctGrpQTailDroppedPkts rbnCircuitGroupQEntry 7 1.3.6.1.4.1.2352.2.43.1.2.1.7 | Counter64 | 0..18446744073709551615 | Number of packets dropped when the total number of packets in this queue is greater than the maximum threshold.

### 1.14.3 rbnCctGrpRLPolicyStatsTable

This table contains counters for rate-limiting policies applied to circuit groups.

`Index:` rbnCctGrpName, rbnCctGrpRLPolicyType

Table 29 describes the objects in rbnCctGrpRLPolicyStatsTable.

Table 29 Objects in rbnCctGrpRLPolicyStatsTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnCctGrpRLPolicyType rbnCctGrpRLPolicyStatsEntry 1 1.3.6.1.4.1.2352.2.43.1.3.1.1 | RbnQosPolicyType Integer | 1—policing 2—metering | The type of the rate-limit policy which is applied to the circuit group.
rbnCctGrpRLPolicyName rbnCctGrpRLPolicyStatsEntry 2 1.3.6.1.4.1.2352.2.43.1.3.1.2 | SnmpAdminString | 1..39 | Name of the rate-limit policy.
rbnCctGrpRLPolicyConformOctets rbnCctGrpRLPolicyStatsEntry 3 1.3.6.1.4.1.2352.2.43.1.3.1.3 | Counter64 | 0..18446744073709551615 | Number of octets that conform to the rate limit set on the circuit group for which counters are enabled.
rbnCctGrpRLPolicyConformPkts rbnCctGrpRLPolicyStatsEntry 4 1.3.6.1.4.1.2352.2.43.1.3.1.4 | Counter64 | 0..18446744073709551615 | Number of packets that conform to the rate limit set on the circuit group for which counters are enabled.
rbnCctGrpRLPolicyExceedOctets rbnCctGrpRLPolicyStatsEntry 5 1.3.6.1.4.1.2352.2.43.1.3.1.5 | Counter64 | 0..18446744073709551615 | Number of octets that exceed the rate limit set on the interface for which class counters are enabled.
rbnCctGrpRLPolicyExceedPkts rbnCctGrpRLPolicyStatsEntry 6 1.3.6.1.4.1.2352.2.43.1.3.1.6 | Counter64 | 0..18446744073709551615 | Number of packets that exceed the rate limit set on the interface.
rbnCctGrpRLPolicyExceedDroppedOctets rbnCctGrpRLPolicyStatsEntry 7 1.3.6.1.4.1.2352.2.43.1.3.1.7 | Counter64 | 0..18446744073709551615 | Number of octets that were dropped due to the application of an exceed action on packets that exceed the rate limit set on the circuit group for which counters are enabled.
rbnCctGrpRLPolicyExceedDroppedPkts rbnCctGrpRLPolicyStatsEntry 8 1.3.6.1.4.1.2352.2.43.1.3.1.8 | Counter64 | 0..18446744073709551615 | Number of packets that were dropped due to the application of an exceed action on packets that exceed the rate limit set on the circuit group for which counters are enabled.
rbnCctGrpRLPolicyViolateOctets rbnCctGrpRLPolicyStatsEntry 9 1.3.6.1.4.1.2352.2.43.1.3.1.9 | Counter64 | 0..18446744073709551615 | Number of octets that violate the normal and maximum burst sizes on the circuit group for which counters are enabled.
rbnCctGrpRLPolicyViolatePkts rbnCctGrpRLPolicyStatsEntry 10 1.3.6.1.4.1.2352.2.43.1.3.1.10 | Counter64 | 0..18446744073709551615 | Number of packets that violate the normal and maximum burst sizes on the circuit group for which counters are enabled.
rbnCctGrpRLPolicyViolateDroppedOctets rbnCctGrpRLPolicyStatsEntry 11 1.3.6.1.4.1.2352.2.43.1.3.1.11 | Counter64 | 0..18446744073709551615 | Number of octets that were dropped due to the application of a violate action on packets that violate the normal and maximum burst sizes on the circuit group for which counters are enabled.
rbnCctGrpRLPolicyViolateDroppedPkts rbnCctGrpRLPolicyStatsEntry 12 1.3.6.1.4.1.2352.2.43.1.3.1.12 | Counter64 | 0..18446744073709551615 | Number of packets that were dropped due to the application of a violate action on packets that violate the normal and maximum burst sizes on the circuit group for which counters are enabled.

### 1.14.4 rbnCctGrpRLClassStatsTable

This table contains counters for rate limit policy classes applied to circuit groups.

`Index:` rbnCctGrpName, rbnCctGrpRLPolicyType, rbnCctGrpRLClassId

Table 30 describes the objects in rbnCctGrpRLClassStatsTable.

Table 30 Objects in rbnCctGrpRLClassStatsTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnCctGrpRLClassId rbnCctGrpRLClassStatsEntry 1 1.3.6.1.4.1.2352.2.43.1.4.1.1 | RbnQosClassId Unsigned32 | 1..8 | A value that uniquely identifies a class defined in the rate-limit policy access list.
rbnCctGrpRLClassName rbnCctGrpRLClassStatsEntry 2 1.3.6.1.4.1.2352.2.43.1.4.1.2 | SnmpAdminString | 1..39 | Name of the class in the rate-limiting policy access list.
rbnCctGrpRLClassConformOctets rbnCctGrpRLClassStatsEntry 3 1.3.6.1.4.1.2352.2.43.1.4.1.3 | Counter64 | 0..18446744073709551615 | Number of octets that conform to the policy class rate limit set on the circuit group.
rbnCctGrpRLClassConformPkts rbnCctGrpRLClassStatsEntry 4 1.3.6.1.4.1.2352.2.43.1.4.1.4 | Counter64 | 0..18446744073709551615 | Number of packets that conform to the policy class rate limit set on the circuit group.
rbnCctGrpRLClassConformDroppedOctets rbnCctGrpRLClassStatsEntry 5 1.3.6.1.4.1.2352.2.43.1.4.1.5 | Counter64 | 0..18446744073709551615 | Number of octets that were dropped due to the application of a conform action on packets that conform to the policy class rate limit set on the circuit group.
rbnCctGrpRLClassConformDroppedPkts rbnCctGrpRLClassStatsEntry 6 1.3.6.1.4.1.2352.2.43.1.4.1.6 | Counter64 | 0..18446744073709551615 | Number of packets that were dropped due to the application of a conform action on packets that conform to the policy class rate limit set on the circuit group.
rbnCctGrpRLClassExceedOctets rbnCctGrpRLClassStatsEntry 7 1.3.6.1.4.1.2352.2.43.1.4.1.7 | Counter64 | 0..18446744073709551615 | Number of octets that exceed the policy class rate limit set on the circuit group.
rbnCctGrpRLClassExceedPkts rbnCctGrpRLClassStatsEntry 8 1.3.6.1.4.1.2352.2.43.1.4.1.8 | Counter64 | 0..18446744073709551615 | Number of packets that exceed the policy class rate limit set on the circuit group.
rbnCctGrpRLClassExceedDroppedOctets rbnCctGrpRLClassStatsEntry 9 1.3.6.1.4.1.2352.2.43.1.4.1.9 | Counter64 | 0..18446744073709551615 | Number of octets that were dropped due to the application of an exceed action on packets that exceed the policy class rate limit set on the circuit group.
rbnCctGrpRLClassExceedDroppedPkts rbnCctGrpRLClassStatsEntry 10 1.3.6.1.4.1.2352.2.43.1.4.1.10 | Counter64 | 0..18446744073709551615 | Number of packets that were dropped due to the application of an exceed action on packets that exceed the policy class rate limit set on the circuit group.
rbnCctGrpRLClassViolateOctets rbnCctGrpRLClassStatsEntry 11 1.3.6.1.4.1.2352.2.43.1.4.1.11 | Counter64 | 0..18446744073709551615 | Number of octets that violate the normal and maximum burst sizes on the circuit group.
rbnCctGrpRLClassViolatePkts rbnCctGrpRLClassStatsEntry 12 1.3.6.1.4.1.2352.2.43.1.4.1.12 | Counter64 | 0..18446744073709551615 | Number of packets that violate the normal and maximum burst sizes on the circuit group.
rbnCctGrpRLClassViolateDroppedOctets rbnCctGrpRLClassStatsEntry 13 1.3.6.1.4.1.2352.2.43.1.4.1.13 | Counter64 | 0..18446744073709551615 | Number of octets that were dropped due to the application of a violate action on packets that violate the normal and maximum burst sizes on the circuit group.
rbnCctGrpRLClassViolateDroppedPkts rbnCctGrpRLClassStatsEntry 14 1.3.6.1.4.1.2352.2.43.1.4.1.14 | Counter64 | 0..18446744073709551615 | Number of packets that were dropped due to the application of a violate action on packets that violate the normal and maximum burst sizes on the circuit group.

## 1.15 RBN-CONFIG-FILE-MIB

Saves the running SmartEdge router configuration on a File Transfer Protocol (FTP) or Trivial FTP (TFTP) server and loads the configuration files from that server.

The following sections contain object information for RBN-CONFIG-FILE-MIB.

### 1.15.1 RBN-CONFIG-FILE-MIB Objects

Table 31 describes the objects in the RBN-CONFIG-FILE-MIB.

Table 31 Objects in RBN-CONFIG-FILE-MIB
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rcfJobSpinLock rcfJobs 1 1.3.6.1.4.1.2352.2.13.1.1.1 | TestAndIncr | 0..2147483647 | An advisory lock used to allow several cooperating Command Generator Applications to coordinate their use of facilities to create and modify entries in rcfJobTable. This object is read-write.
rcfJobNextIndex rcfJobs 2 1.3.6.1.4.1.2352.2.13.1.1.2 | Unsigned32 | 0..4294967295 | The next available index which can be used to create an rcfJobEntry object. This object is read-write.

### 1.15.2 rcfJobTable

This table starts and monitors a process that loads a configuration file or saves the current configuration to a file.

Use one of the following methods to create a new entry:

- `snmpget` command (rcfJobSpinLock.0, rcfJobNextIndex.0) and the save in slValue, niValue, respectively
- `snmpset` command (rcfJobSpinLock.0 = slValue, rcfJobXxx.niValue = ... rcfJobYyy.niValue = ... rcfJobRowStatus.niValue = 'createAndGo')

Entries with a completed state are automatically deleted by the system after some system-dependent time.

`Index:` rcfJobIndex

Table 32 describes objects in the rcfJobTable. All objects presented in this table are read-create unless noted otherwise.

Table 32 Objects in rcfJobTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rcfJobIndex rcfJobEntry 1 1.3.6.1.4.1.2352.2.13.1.1.3.1.1 | Unsigned32 Integer | 1..4294967295 | A unique identifier for an entry in this table. This object is not-accessible.
rcfJobOp rcfJobEntry 2 1.3.6.1.4.1.2352.2.13.1.1.3.1.2 | Integer | 1—save | The current system configuration is written to the file specified in the rcfJobFilename object.
rcfJobProtocol rcfJobEntry 3 1.3.6.1.4.1.2352.2.13.1.1.3.1.3 | Integer | 1—tftp 2—ftp | The file transfer protocol to use.. If tftp, the filename specified in the rcfJobFilename object is read or written from or to the system identified by the rcfJobIpAddress object through the TFTP file transfer protocol. If ftp, the filename specified in rcfJobFilename is read or written from or to the system identified by the rcfJobIpAddress object through the FTP file transfer protocol.
rcfJobFilename rcfJobEntry 4 1.3.6.1.4.1.2352.2.13.1.1.3.1.4 | SnmpAdminString | 1..128 | The name of the destination file.
rcfJobIpAddressType rcfJobEntry 5 1.3.6.1.4.1.2352.2.13.1.1.3.1.5 | InetAddressType Integer | 1—ipv4 | The address type for the rcfJobIpAddress object.
rcfJobIpAddress rcfJobEntry 6 1.3.6.1.4.1.2352.2.13.1.1.3.1.6 | InetAddress String | 0..255 | The IP address for the file server that contains the destination file.
rcfJobUsername rcfJobEntry 7 1.3.6.1.4.1.2352.2.13.1.1.3.1.7 | SnmpAdminString | 1..32 | The username to use for authentication with the file server. This object is only relevant for the FTP protocol. If the rcfJobProtocol object does not equal ftp, any value for this object is ignored. For security reasons, all SNMP get actions on this object return a string of zero (0) length.
rcfJobPassword rcfJobEntry 8 1.3.6.1.4.1.2352.2.13.1.1.3.1.8 | SnmpAdminString | 0..128 | The password to use for authentication with the file server. A string of zero (0) length value is used for usernames that do not require a password. This object is only relevant for the FTP protocol. For security reasons, all SNMP gets on this object return a string of zero (0) length.
rcfJobPassiveMode rcfJobEntry 9 1.3.6.1.4.1.2352.2.13.1.1.3.1.9 | TruthValue Integer | 1—true 2—false | Enables true or disables false passive mode on FTP connections. This object is only relevant for the FTP protocol. The default value is false (2).
rcfJobStopAtLine rcfJobEntry 10 1.3.6.1.4.1.2352.2.13.1.1.3.1.10 | Unsigned32 | 0..4294967295 | If this object instance has a non zero value, parsing and loading of the configuration file stops after the specified line number. The default value is zero (0).
rcfJobSaveDefaults rcfJobEntry 11 1.3.6.1.4.1.2352.2.13.1.1.3.1.11 | TruthValue Integer | 1—true 2—false | If the value of this object is true, the default values for all configuration values are saved. If the value of this object is false, only the values that have been explicitly configured are saved. The default value is false (2).
rcfJobState rcfJobEntry 12 1.3.6.1.4.1.2352.2.13.1.1.3.1.12 | Integer | 0—pending 1—inProgress 2—completed | The current state of the configuration job. pending (0): The initial state of all jobs. Jobs are queued and processed in order of creation. inProgress (1): The job is actively being performed. completed (2): The job has completed. This object is read-only.
rcfJobResult rcfJobEntry 13 1.3.6.1.4.1.2352.2.13.1.1.3.1.13 | Integer | 0—success 1—other 2—noMemory 3—parse 4—io 5—access | A generic result code. This object is instantiated only when the value of the rcfJobStatus object is completed. success (0): The job completed successfully. other(1): An error that doesn't fall into one of the categories below. noMemory(2): Insufficient system resources to perform the operation. parse(3): A parse failure occurred. ie- there was a syntax error in the source configuration file. io (4): An i/o error occurred. access (5): A file access error occurred. This could be caused by a non-existant source file, or insufficient access/permission to create/modify the destination file. This object is read-only.
rcfJobErrorMsgs rcfJobEntry 14 1.3.6.1.4.1.2352.2.13.1.1.3.1.14 | SnmpAdminString | 1..4294967295 | Detailed error messages generated during the configuration operation. This object is instantiated only when the rcfJobState object equals completed (2). NOTE: The amount of error messages produced by a configuration operation may exceed the maximum size of this object (255 bytes). If this happens, the last character in the rcfJobErrorMsgs value is '$' to indicate that a truncation occurred. NOTE: Some messages that appear when you configure an operation through the CLI are not seen in the values for this object. For example, on the SMS platform, the CLI displays messages when there is a parse failure. These messages are not captured in this object. This object is read-only.
rcfJobCreateTime rcfJobEntry 15 1.3.6.1.4.1.2352.2.13.1.1.3.1.15 | TimeStamp TimeTicks | 0..4294967295 | The value of sysUpTime when this job entry was created. This object is read-only.
rcfJobStartTime rcfJobEntry 16 1.3.6.1.4.1.2352.2.13.1.1.3.1.16 | TimeStamp TimeTicks | 0..4294967295 | The value of the sysUpTime object when the rcfJobState object moved from pending to inProgress. This object is not instantiated until the value of the rcfJobState object changes to inProgress. The object is uninstantiated if the value of the rcfJobRowStatus object is set to notInService. This object is read-only.
rcfJobStopTime rcfJobEntry 17 1.3.6.1.4.1.2352.2.13.1.1.3.1.17 | TimeStamp TimeTicks | 0..4294967295 | This object is not instantiated until the value of the rcfJobState object changes to completed. The object will be uninstantiated if the rcfJobRowStatus object is set to notInService. This object is read-only.
rcfJobNotifyOnCompletion rcfJobEntry 18 1.3.6.1.4.1.2352.2.13.1.1.3.1.18 | TruthValue Integer | 1—true 2—false | If the value of this object is true, an rcfJobCompleted notification is generated when the job completes.
rcfJobOwner rcfJobEntry 19 1.3.6.1.4.1.2352.2.13.1.1.3.1.19 | OwnerString String | 0..127 | This object can be used to identify who created this job entry and at what time the entry was created.
rcfJobRowStatus rcfJobEntry 20 1.3.6.1.4.1.2352.2.13.1.1.3.1.20 | RowStatus Integer | 1—active 2—notInService 3—notReady 4—createAndGo 5—createAndWait 6—destroy | The row status for creating, modifying, or deleting an entry in the table. Entries with a value of active cannot be modified. Any attempt to modify an object in this entry while the rcfJobRowStatus object equals active results in an inconsistentValue error. To modify objects in an active entry, the rcfJobRowStatus object must first be set to notInService. All entries are automatically deleted by the agent after some system-dependent time.

### 1.15.3 Example: Saving System Configuration

The rcfJobTable in RBN-CONFIG-FILE-MIB enterprise MIB is used to save or load configuration files to and from a TFTP or FTP server. To create a save request job, do the following:

1. Use the rcfJobNextIndex object to obtain the next available index for rcfJobTable.

    sh$ snmpget -c public -v 2c SE-lab2 rcfJobNextIndex.0
    RBN-CONFIG-FILE-MIB::rcfJobNextIndex.0 = Gauge32: 1
    sh$

2. The preceding output shows that the ‘1’ is the next available index. The save config request can be made with rcfJobNextIndex = 1 by creating a row entry in rcfJobTable:

    sh$ snmpset -c private -v 2c SE-lab2 rcfJobOp.1 i save rcfJobProtocol.1
     i local rcfJobFilename.1 s /md/snmpsave.cfg rcfJobOwner.1 s jsmith
    rcfJobRowStatus.1 i createAndGo
    RBN-CONFIG-FILE-MIB::rcfJobOp.1 = INTEGER: save(1)
    RBN-CONFIG-FILE-MIB::rcfJobProtocol.1 = INTEGER: local(0)
    RBN-CONFIG-FILE-MIB::rcfJobFilename.1 = STRING: /md/snmpsave.cfg
    RBN-CONFIG-FILE-MIB::rcfJobOwner.1 = STRING: "jsmith"
    RBN-CONFIG-FILE-MIB::rcfJobRowStatus.1 = INTEGER: createAndGo(4)

Note:
  The rcfJobOwner object is optional.

To view the request status, the rcfJobState object must be retrieved as follows:

    sh$ snmpget -c public -v 2c SE-lab2 rcfJobState.1
    RBN-CONFIG-FILE-MIB::rcfJobState.1 = INTEGER: inProgress(1)

After a few seconds, performing snmpget on rcfJobState, will display `completed` as follows:

    sh$ snmpget -c public -v 2c SE-lab2 rcfJobState.1
    RBN-CONFIG-FILE-MIB::rcfJobState.1 = INTEGER: completed(2)

To view the job status, perform an snmpwalk of rcfJobs:

    sh$ snmpwalk -c public -v 2c SE-lab2 rcfJobs
    RBN-CONFIG-FILE-MIB::rcfJobSpinLock.0 = INTEGER: 1
    RBN-CONFIG-FILE-MIB::rcfJobNextIndex.0 = Gauge32: 2
    RBN-CONFIG-FILE-MIB::rcfJobOp.1 = INTEGER: save(1)
    RBN-CONFIG-FILE-MIB::rcfJobProtocol.1 = INTEGER: local(0)
    RBN-CONFIG-FILE-MIB::rcfJobFilename.1 = STRING: /md/snmpsave.cfg
    RBN-CONFIG-FILE-MIB::rcfJobStopAtLine.1 = Gauge32: 0
    RBN-CONFIG-FILE-MIB::rcfJobSaveDefaults.1 = INTEGER: false(2)
    RBN-CONFIG-FILE-MIB::rcfJobState.1 = INTEGER: completed(2)
    RBN-CONFIG-FILE-MIB::rcfJobResult.1 = INTEGER: success(0)
    RBN-CONFIG-FILE-MIB::rcfJobErrorMsgs.1 = STRING:
    RBN-CONFIG-FILE-MIB::rcfJobCreateTime.1 = Timeticks: (22738049) 2 days,
     15:09:40.49
    RBN-CONFIG-FILE-MIB::rcfJobStartTime.1 = Timeticks: (22738049) 2 days,
     15:09:40.49
    RBN-CONFIG-FILE-MIB::rcfJobStopTime.1 = Timeticks: (22740317) 2 days,
     15:10:03.17
    RBN-CONFIG-FILE-MIB::rcfJobNotifyOnCompletion.1 = INTEGER: false(2)
    RBN-CONFIG-FILE-MIB::rcfJobOwner.1 = STRING: "jsmith"
    RBN-CONFIG-FILE-MIB::rcfJobRowStatus.1 = INTEGER: active(1)

To save the file to an FTP server perform an snmpset on rcfJobOp.2.

    sh$ snmpset -c public -v 2c SE-lab2 rcfJobOp.2 i save rcfJobProtocol.2
     i ftp rcfJobIpAddressType.2 i ipv4

    rcfJobIpAddress.2 d 172.16.8.2 rcfJobUsername.2 s lab rcfJobPassword.2
     s lab123 rcfJobFilename.2 s snmpsave.cfg  rcfJobOwner.2 s jsmith
    rcfJobRowStatus.2 i createAndGo
    RBN-CONFIG-FILE-MIB::rcfJobOp.2 = INTEGER: save(1)
    RBN-CONFIG-FILE-MIB::rcfJobProtocol.2 = INTEGER: ftp(2)
    RBN-CONFIG-FILE-MIB::rcfJobIpAddressType.2 = INTEGER: ipv4(1)
    RBN-CONFIG-FILE-MIB::rcfJobIpAddress.2 = Hex-STRING: AC 10 08 02
    RBN-CONFIG-FILE-MIB::rcfJobUsername.2 = STRING: lab
    RBN-CONFIG-FILE-MIB::rcfJobPassword.2 = STRING: lab123
    RBN-CONFIG-FILE-MIB::rcfJobFilename.2 = STRING: snmpsave.cfg
    RBN-CONFIG-FILE-MIB::rcfJobNotifyOnCompletion.2 = INTEGER: false(2)
    RBN-CONFIG-FILE-MIB::rcfJobOwner.2 = STRING: "jsmith"
    RBN-CONFIG-FILE-MIB::rcfJobRowStatus.2 = INTEGER: createAndGo(4)

To load a configuration file from the FTP server, issue the snmpset command as follows:

    sh$ snmpset -c public -v 2c SE-lab2 rcfJobOp.3 i load rcfJobProtocol.3
     i ftp rcfJobIpAddressType.3 i ipv4 rcfJobIpAddress.3 d 172.16.8.2
     rcfJobUsername.3 s lab

    rcfJobPassword.3 s lab123 rcfJobFilename.3 s snmpsave.cfg
    rcfJobOwner.3 s jsmith rcfJobRowStatus.3 i createAndGo
    RBN-CONFIG-FILE-MIB::rcfJobOp.3 = INTEGER: load(0)
    RBN-CONFIG-FILE-MIB::rcfJobProtocol.3 = INTEGER: ftp(2)
    RBN-CONFIG-FILE-MIB::rcfJobIpAddressType.3 = INTEGER: ipv4(1)
    RBN-CONFIG-FILE-MIB::rcfJobIpAddress.3 = Hex-STRING: AC 10 08 02
    RBN-CONFIG-FILE-MIB::rcfJobUsername.3 = STRING: lab
    RBN-CONFIG-FILE-MIB::rcfJobPassword.3 = STRING: lab123
    RBN-CONFIG-FILE-MIB::rcfJobFilename.3 = STRING: snmpsave.cfg
    RBN-CONFIG-FILE-MIB::rcfJobNotifyOnCompletion.3 = INTEGER: false(2)
    RBN-CONFIG-FILE-MIB::rcfJobOwner.3 = STRING: "jsmith"
    RBN-CONFIG-FILE-MIB::rcfJobRowStatus.3 = INTEGER: createAndGo(4)

To view the system configuration using the CLI, use the following commands:

    [local]Redback#save configuration ?
    /md    Save into the Micro Drive
    WORD   source file in format [/dir/]filename
    ftp:   File Transfer Protocol
    rcp:   Remote Copy Protocol
    scp:   Secured Copy Protocol
    sftp:  Secured File Transfer Protocol
    tftp:  Trivial File Transfer Protocol
    <cr>

    [local]Redback# configuration ?
    WORD   URL of configuration file
    ftp:   File Transfer Protocol
    rcp:   Remote Copy Protocol
    scp:   Secured Copy Protocol
    sftp:  Secured File Transfer Protocol
    tftp:  Trivial File Transfer Protocol
    <cr>

## 1.16 RBN-CPU-METER-MIB

Manages central processing unit (CPU) utilization.

The following sections contain object information for RBN-CPU-METER-MIB.

### 1.16.1 RBN-CPU-METER-MIB Objects

Table 33 describes the objects in RBN-CPU-METER-MIB.

Table 33 Objects in RBN-CPU-METER-MIB
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnCpuMeterFiveSecondAvg rbnCpuMeterMIBObjects 1 1.3.6.1.4.1.2352.2.6.1.1 | RbnPercentage Integer32 | 0..100 | Provides the CPU percentage used over the first five-second period in the scheduler.
rbnCpuMeterOneMinuteAvg rbnCpuMeterMIBObjects 2 1.3.6.1.4.1.2352.2.6.1.2 | RbnPercentage Integer32 | 0..100 | Provides a cumulative average of the CPU percentage used over a one minute period.
rbnCpuMeterFiveMinuteAvg rbnCpuMeterMIBObjects 3 1.3.6.1.4.1.2352.2.6.1.3 | RbnPercentage Integer32 | 0..100 | Provides a cumulative average of the CPU percentage used over a five-minute period.

### 1.16.2 rbnCpuProcTable

This table contains the objects that identify CPU processes. Entries in the table are created or deleted as processes are started or terminated.

`Index:` IMPLIED rbnCpuProcName

Table 34 describes the objects in rbnCpuProcTable.

Table 34 Objects in rbnCpuProcTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnCpuProcName rbnCpuProcEntry 1 1.3.6.1.4.1.2352.2.6.3.1.1.1 | DisplayString | 1..128 | The name for this process.
rbnCpuProcPriority rbnCpuProcEntry 2 1.3.6.1.4.1.2352.2.6.3.1.1.2 | Unsigned32 | 0..255 | The priority of this process. This value ranges from 0 to 255, with 0 being the highest priority.
rbnCpuProcTime rbnCpuProcEntry 3 1.3.6.1.4.1.2352.2.6.3.1.1.3 | Counter32 | 0..4294967295 | The total time, in milliseconds, spent in this process.
rbnCpuProcCalls rbnCpuProcEntry 4 1.3.6.1.4.1.2352.2.6.3.1.1.4 | Counter32 | 0..4294967295 | The number of times that this process has acquired the CPU.
rbnCpuProc5Sec rbnCpuProcEntry 5 1.3.6.1.4.1.2352.2.6.3.1.1.5 | RbnPercentage Integer32 | 0..100 | The average CPU usage in a five-second window for this process.
rbnCpuProc1Min rbnCpuProcEntry 6 1.3.6.1.4.1.2352.2.6.3.1.1.6 | RbnPercentage Integer32 | 0..100 | The average CPU usage in a one-minute window for this process.
rbnCpuProc5Min rbnCpuProcEntry 7 1.3.6.1.4.1.2352.2.6.3.1.1.7 | RbnPercentage Integer32 | 0..100 | The average CPU usage in a five-minute window for this process.
rbnCpuProcLongest rbnCpuProcEntry 8 1.3.6.1.4.1.2352.2.6.3.1.1.8 | Gauge32 | 0..4294967295 | The maximum time, in milliseconds, spent in this process.

### 1.16.3 Example: Collecting CPU Usage

To collect CPU usage for the five-second average, perform an snmpbulkwalk for rbnCpuMeterFiveSecondAvg:

    sh-3.00$ snmpbulkwalk -v2c -cpublic -m RBN-CPU-METER-MIB oak.lab
    rbnCpuMeterFiveSecondAvg
    RBN-CPU-METER-MIB::rbnCpuMeterFiveSecondAvg.0 = INTEGER: 3

To collect CPU usage for the one-minute average, perform an snmpbulkwalk for rbnCpuMeterOneMinuteAvg:

    sh-3.00$ snmpbulkwalk -v2c -cpublic -m RBN-CPU-METER-MIB oak.lab
    rbnCpuMeterOneMinuteAvg
    RBN-CPU-METER-MIB::rbnCpuMeterOneMinuteAvg.0 = INTEGER: 0

To collect CPU usage for the five-minute average, perform an snmpbulkwalk for rbnCpuMeterFiveMinuteAvg:

    sh-3.00$ snmpbulkwalk -v2c -cpublic -m RBN-CPU-METER-MIB oak.lab
    rbnCpuMeterFiveMinuteAvg
    RBN-CPU-METER-MIB::rbnCpuMeterFiveMinuteAvg.0 = INTEGER: 0

To view CPU status using the CLI, issue the following command:

    [local]Redback#show process cpustats
    Total system CPU % usage (5s, 1m, 5m):  3.41,  0.83,  0.29 <output truncated>

## 1.17 RBN-DHCP-MIB

Provides a table for monitoring the configuration and statistics of Dynamic Host Configuration Protocol (DHCP) range thresholds in an interface, and a group of scalars for monitoring the configuration and statistics of DHCP thresholds for the context.

### 1.17.1 DHCP Threshold Per Context Objects

Table 35 describes the DHCP Threshold Per Context Objects in RBN-DHCP-MIB.

Table 35 Objects in DHCP Threshold Per Context
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnDhcpCtxThresholdName rbnDhcpCtxThreshold 1 1.3.6.1.4.1.2352.2.30.1.2.1 | SnmpAdminString | 0..63 | Identifies the context in which a falling or rising per-context threshold event occurs. This object is accessible-for-notify.
rbnDhcpCtxThresholdSize rbnDhcpCtxThreshold 2 1.3.6.1.4.1.2352.2.30.1.2.2 | Unsigned32 | 0..4294967295 | Total number of leases in all DHCP ranges of all interfaces in the context valid in the current view.
rbnDhcpCtxThresholdAvailable rbnDhcpCtxThreshold 3 1.3.6.1.4.1.2352.2.30.1.2.3 | Unsigned32 | 0..4294967295 | Total number of leases available in all DHCP ranges of all interfaces in the context valid in the current view.
rbnDhcpCtxThresholdInuse rbnDhcpCtxThreshold 4 1.3.6.1.4.1.2352.2.30.1.2.4 | Unsigned32 | 0..4294967295 | Total number of leases in use in all DHCP ranges of all interfaces in the context valid in the current view.
rbnDhcpCtxThresholdFallingThreshold rbnDhcpCtxThreshold 5 1.3.6.1.4.1.2352.2.30.1.2.5 | Unsigned32 | 0..196608 | The falling threshold value for the context valid in the current view. Just as the rbnDhcpIntfThresholdFallingThreshold object is the per-interface falling threshold, this object is the per-context falling threshold. When the sum of the all available DHCP leases in all interfaces of the context valid in the current view reaches the value of this object, a trap, a log message, or both are generated. Evaluation of whether to perform the action occurs on allocation of a lease from the available pool of leases from any interface within the context. The values of the rbnDhcpCtxThresholdFallingSendTrap object and the rbnDhcpCtxThresholdFallingLogMessage object determine whether to send a trap or a log message. If there is no per-context rising threshold, the value of this object is zero and the values of the rbnDhcpCtxThresholdFallingSendTrap object and the rbnDhcpCtxThresholdFallingLogMessage object are false.
rbnDhcpCtxThresholdFallingSendTrap rbnDhcpCtxThreshold 6 1.3.6.1.4.1.2352.2.30.1.2.6 | TruthValue Integer | 1—true 2—false | If the value of this object is true, on reaching the per-context falling threshold, a trap is sent.
rbnDhcpCtxThresholdFallingLogMessage rbnDhcpCtxThreshold 7 1.3.6.1.4.1.2352.2.30.1.2.7 | TruthValue Integer | 1—true 2—false | If the value of this object is true on reaching the per-context falling threshold, a message is logged.
rbnDhcpCtxThresholdRisingThreshold rbnDhcpCtxThreshold 8 1.3.6.1.4.1.2352.2.30.1.2.8 | Unsigned32 | 0..196608 | The rising threshold value for the context valid in the current view. Just as the rbnDhcpIntfThresholdRisingThreshold object is the per interface rising threshold, this object is the per context rising threshold. When the sum of the all available DHCP leases in all interfaces of the context valid in the current view reaches the value of this object a rising threshold action of a trap, a log message, or both is generated. This is a rising threshold, so the evaluation of whether to perform the action occurs upon return of a lease to the available pool of leases defined in any interface within the context. The action of whether to send a trap or log message is specified by the values of the rbnDhcpCtxThresholdRisingSendTrap object and the rbnDhcpCtxThresholdRisingLogMessage object. If there is no per context rising threshold, the value of this object will be zero and the values of the rbnDhcpCtxThresholdRisingSendTrap object and the rbnDhcpCtxThresholdRisingLogMessage object will be false.
rbnDhcpCtxThresholdRisingSendTrap rbnDhcpCtxThreshold 9 1.3.6.1.4.1.2352.2.30.1.2.9 | TruthValue Integer | 1—true 2—false | If the value of this object is true, upon detection of reaching the per context rising threshold, a trap will be sent.
rbnDhcpCtxThresholdRisingLogMessage rbnDhcpCtxThreshold 10 1.3.6.1.4.1.2352.2.30.1.2.10 | TruthValue Integer | 1—true 2—false | If the value of this object is true, upon detection of reaching the per context rising threshold, a message is logged.

### 1.17.2 rbnDhcpIntfThresholdTable

This table allows monitoring of per-interface DHCP server thresholds through SNMP. This table contains the objects that characterize DHCP server thresholds. The row corresponds to information about the leases in a DHCP server range for a particular interface and the corresponding capacity, usage, and falling and rising thresholds. Objects defined in this table are only accessible within the context identified in the SNMP protocol (that is, the community string in SNMPv1 or SNMPv2 or the contextName in SNMPv3).

`Index:` IMPLIED rbnDhcpIntfThresholdName

Table 36 describes the object in rbnDhcpIntfThresholdTable.

Table 36 Objects in rbnDhcpIntfThresholdTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnDhcpIntfThresholdName rbnDhcpIntfThresholdEntry 1 1.3.6.1.4.1.2352.2.30.1.1.1.1 | SnmpAdminString | 0..80 | The name of the interface. If you configure this entry using another tool (for example, a CLI), you can set it to a length greater than 80 characters. Names that exceed this length are not accessible through SNMP operations. This object is not accessible.

### 1.17.3 rbnDhcpRangeThresholdTable

This table contains the objects which characterize DHCP server ranges. Each row in the table corresponds to information about the leases in a DHCP server for a particular range on a particular interface and the corresponding capacity, usage, and falling and rising thresholds.

Objects defined in this table are only accessible within the context identified in the SNMP protocol (that is, the community string in SNMPv1 or SNMPv2 or the contextName in SNMPv3).

`Index:` rbnDhcpRangeThresholdInterfaceIdx, rbnDhcpRangeThresholdAddr

Table 37 describes the objects in rbnDhcpRangeThresholdTable.

Table 37 Objects in rbnDhcpRangeThresholdTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnDhcpRangeThresholdInterfaceIdx rbnDhcpRangeThresholdEntry 1 1.3.6.1.4.1.2352.2.30.1.3.1.1 | Unsigned32 | 0..4294967295 | The index of the interface containing the DHCP range.
rbnDhcpRangeThresholdAddr rbnDhcpRangeThresholdEntry 2 1.3.6.1.4.1.2352.2.30.1.3.1.2 | IpAddress Octet String | SIZE (4) | The start address of the DHCP range.
rbnDhcpRangeThresholdEndAddr rbnDhcpRangeThresholdEntry 3 1.3.6.1.4.1.2352.2.30.1.3.1.3 | IpAddress Octet String | SIZE (4) | The end address of the DHCP range.
rbnDhcpRangeThresholdContextName rbnDhcpRangeThresholdEntry 4 1.3.6.1.4.1.2352.2.30.1.3.1.4 | SnmpAdminString | 0..63 | The name of the context that contains the interface.
rbnDhcpRangeThresholdInterfaceName rbnDhcpRangeThresholdEntry 5 1.3.6.1.4.1.2352.2.30.1.3.1.5 | SnmpAdminString | 1..80 | The name of the interface containing the DHCP range.
rbnDhcpRangeThresholdSize rbnDhcpRangeThresholdEntry 6 1.3.6.1.4.1.2352.2.30.1.3.1.6 | Unsigned32 | 0..4294967295 | The number of leases reserved for the DHCP server in this range.
rbnDhcpRangeThresholdAvailable rbnDhcpRangeThresholdEntry 7 1.3.6.1.4.1.2352.2.30.1.3.1.7 | Unsigned32 | 0..4294967295 | The number of leases available in this range.
rbnDhcpRangeThresholdInuse rbnDhcpRangeThresholdEntry 8 1.3.6.1.4.1.2352.2.30.1.3.1.8 | Unsigned32 | 0..4294967295 | The number of leases that are in use in this range.
rbnDhcpRangeThresholdFallingThreshold rbnDhcpRangeThresholdEntry 9 1.3.6.1.4.1.2352.2.30.1.3.1.9 | Unsigned32 | 0..196608 | Value that specifies that enabled falling threshold events are generated when the value of available leases drops to the falling threshold value. The value of available leases drops to the falling threshold value when a lease is taken from the range. The number of available leases is reported in the rbnDhcpRangeThresholdAvailable object. A falling threshold event is a notification, a log message, or both. Falling threshold events are enabled if either or both of the rbnDhcpRangeThresholdFallingSendTrap object and the rbnDhcpRangeThresholdFallingLogMessage object are true. A falling threshold event is triggered only on a transition of the value of the rbnDhcpRangeThresholdAvailable object dropping from rbnDhcpRangeThresholdFallingThreshold+1 to rbnDhcpRangeThresholdFallingThreshold.
rbnDhcpRangeThresholdFallingSendTrap rbnDhcpRangeThresholdEntry 10 1.3.6.1.4.1.2352.2.30.1.3.1.10 | TruthValue Integer | 1—true 2—false | If the value of this object is true, on reaching a falling threshold, a trap is sent.
rbnDhcpRangeThresholdFallingLogMessage rbnDhcpRangeThresholdEntry 11 1.3.6.1.4.1.2352.2.30.1.3.1.11 | TruthValue Integer | 1—true 2—false | If the value of this object is true, on reaching a falling threshold, a message is logged.
rbnDhcpRangeThresholdRisingThreshold rbnDhcpRangeThresholdEntry 12 1.3.6.1.4.1.2352.2.30.1.3.1.12 | Unsigned32 | 0..196608 | Value that specifies that any enabled rising threshold events are generated when the value of the currently available leases reaches the rising threshold value when a lease is returned to the range. The number of available leases is reported in the rbnDhcpRangeThresholdAvailable object. A rising threshold event is a notification, a log message, or both. Rising threshold events are enabled if either or both of the rbnDhcpRangeThresholdRisingSendTrap object and the rbnDhcpRangeThresholdRisingLogMessage object are true. A rising threshold event is triggered only on a transition of the value of the rbnDhcpRangeThresholdAvailable object increasing from rbnDhcpRangeThresholdRisingThreshold-1 to rbnDhcpRangeThresholdRisingThreshold.
rbnDhcpRangeThresholdRisingSendTrap rbnDhcpRangeThresholdEntry 13 1.3.6.1.4.1.2352.2.30.1.3.1.13 | TruthValue Integer | 1—true 2—false | If the value of this object is true, on reaching a rising threshold, a trap is sent.
rbnDhcpRangeThresholdRisingLogMessage rbnDhcpRangeThresholdEntry 14 1.3.6.1.4.1.2352.2.30.1.3.1.14 | TruthValue Integer | 1—true 2—false | If the value of this object is true, on reaching a rising threshold, a message is logged.

## 1.18 RBN-DS1-MIB

Describes DS1, E1, DS2, and E2 interface objects beyond those instrumented by standard MIBs. RBN-DS1-MIB is not supported on the SmartEdge 100 router.

### 1.18.1 rbnDsx1ConfigTable

This table extends the use of the dsx1ConfigTable table.

Table 38 describes the objects in rbnDsx1ConfigTable, the DS-1 configuration table.

Table 38 Objects in rbnDsx1ConfigTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnDsx1AlarmSeverity rbnDsx1ConfigEntry 1 1.3.6.1.4.1.2352.2.37.1.1.1.1 | RbnAlarmPerceivedSeverity | Integer | The perceived severity of the alarm. See Section 1.43.9 RbnAlarmPerceivedSeverity for details.
rbnDsx1AlarmServiceAffecting rbnDsx1ConfigEntry 2 1.3.6.1.4.1.2352.2.37.1.1.1.2 | RbnAlarmServiceAffecting Integer | 1—yes 2—no | Indicates whether the interface alarm affects service.

## 1.19 RBN-DS3-MIB

Describes DS-3 and E3 interface objects, beyond those instrumented by standard MIBs. RBN-DS3-MIB is unsupported on the SmartEdge 100 router.

### 1.19.1 rbnDsx3ConfigTable

This table extends the use of the dsx3ConfigTable table.

Table 39 describes the objects in rbnDsx3ConfigTable, the DS-3 or E-3 configuration table. All objects in the table are read-only

Table 39 Objects in rbnDsx3ConfigTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnDsx3AlarmSeverity rbnDsx3ConfigEntry 1 1.3.6.1.4.1.2352.2.38.1.1.1.1 | RbnAlarmPerceivedSeverity | Integer | The perceived severity of the alarm. See Section 1.43.9 RbnAlarmPerceivedSeverity for details.
rbnDsx3AlarmServiceAffecting rbnDsx3ConfigEntry 2 1.3.6.1.4.1.2352.2.38.1.1.1.2 | RbnAlarmServiceAffecting Integer | 1—yes 2—no | Indicates whether the interface alarm affects service.

## 1.20 RBN-ENVMON-MIB

Generically manages environmental monitoring functions on SmartEdge router. Alarm conditions that are reported in this MIB are normal, failed, absent, or unknown. A new MIB table, rbnFanSpeedTable, displays the speed of the fan unit on the SmartEdge 100 router.

### 1.20.1 rbnFanStatusTable

This table contains one row for each fan test point. There is not necessarily a one-to-one relationship between fan test points and fan assemblies; a single test point may be used to monitor the status of multiple fans.

`Index:` rbnFanIndex

Table 40 describes the objects in rbnFanStatusTable.

Table 40 Objects in rbnFanStatusTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnFanIndex rbnFanStatusEntry 1 1.3.6.1.4.1.2352.2.4.1.1.1.1 | Integer32 | 1..2147483647 | The unique index of a fan test point.
rbnFanDescr rbnFanStatusEntry 2 1.3.6.1.4.1.2352.2.4.1.1.1.2 | DisplayString | 0..32 | The description of a fan test point. If an instance of this object is associated with a single fan assembly, the value of this object should be the same as the name by which the assembly is normally referenced. If an instance is associated with multiple fan assemblies, the value of this object should contain the names of all of the fan assemblies being monitored.
rbnFanFail rbnFanStatusEntry 3 1.3.6.1.4.1.2352.2.4.1.1.1.3 | TruthValue Integer | 1—true 2—false | The status of a fan test point. If an instance of this object has the value true, then a fan monitored by the test point has failed. If an instance of this object has the value false, then the fan or fans monitored by the test point are operational.
rbnFanStatus rbnFanStatusEntry 4 1.3.6.1.4.1.2352.2.4.1.1.1.4 | Integer | 1—normal 2—failed 3—absent 4—unknown | The status of a fan test point. If an instance of this object has the value normal, then the fan or fans monitored by the test point is operational. If an instance of this object has the value failed, then the fan or fans monitored by the test point has failed. If an instance of this object has the value absent, then the fan or fans monitored by this test point is not present. If an instance of this object has the value unknown, then the test point is unable to monitor the fan or fans.

### 1.20.2 rbnPowerStatusTable

This table contains one row for each power test point.

Note:
  There is not necessarily a one-to-one relationship between power test points and power supply assemblies; a single test point may be used to monitor the status of multiple power supplies.

`Index:` rbnPowerIndex

Table 41 describes the objects in rbnPowerStatusTable.

Table 41 Objects in rbnPowerStatusTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnPowerIndex rbnPowerStatusEntry 1 1.3.6.1.4.1.2352.2.4.1.2.1.1 | Integer32 | 1..2147483647 | The index of a power test point.
rbnPowerDescr rbnPowerStatusEntry 2 1.3.6.1.4.1.2352.2.4.1.2.1.2 | OctetString | 0..32 | Description of a power supply test point. If an instance of this object is associated with a single power supply assembly, the value of this object should be the same as the name by which the assembly is normally referenced. If an instance is associated with multiple power supply assemblies, the value of this object should contain the names of all of the power supply assemblies being monitored.
rbnPowerFail rbnPowerStatusEntry 3 1.3.6.1.4.1.2352.2.4.1.2.1.3 | TruthValue Integer | 1—true 2—false | Status of a power test point. If an instance of this object has the value true, then a power supply monitored by the test point has failed. If an instance of this object has the value false, then the power supply (or supplies) monitored by the test point are operational.
rbnPowerStatus rbnPowerStatusEntry 4 1.3.6.1.4.1.2352.2.4.1.2.1.4 | Integer | 1—normal 2—failed 3—absent 4—unknown | Status of a power test point. If an instance of this object has the value normal, the power supply (or supplies) monitored by the test point is operational. If an instance of this object has the value failed, the power supply (or supplies) monitored by the test point has failed. If an instance of this object has the value absent, the power supply (or supplies) monitored by this test point is not present. If an instance of this object has the value unknown, the test point is unable to monitor the power supply (or supplies).

### 1.20.3 rbnVoltageSensorTable

This table contains one row for each voltage test point. Each physical entity (for example, a card) in the system may have zero or more voltage test points.

`Index:` entPhysicalIndex, rbnVoltageIndex

Table 42 describes the objects in rbnVoltageSensorTable.

Table 42 Objects in rbnVoltageSensorTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnVoltageIndex rbnVoltageSensorEntry 1 1.3.6.1.4.1.2352.2.4.1.3.1.1 | Integer32 | 1..2147483647 | An arbitrary value which uniquely identifies a voltage test point on a particular physical entity. Index values for different test points are not necessarily contiguous.
rbnVoltageDescr rbnVoltageSensorEntry 2 1.3.6.1.4.1.2352.2.4.1.3.1.2 | DisplayString | 0..48 | Description of a voltage test point. Typically an instance of this object holds a user-friendly description of the physical entity and the level of voltage being monitored by this test point.
rbnVoltageDesired rbnVoltageSensorEntry 3 1.3.6.1.4.1.2352.2.4.1.3.1.3 | RbnVoltage Unsigned32 | 0..50000 | Desired voltage level for this test point. If the monitored voltage level (rbnVoltageCurrent) is equal to this value, the system is performing as designed.
rbnVoltageCurrent rbnVoltageSensorEntry 4 1.3.6.1.4.1.2352.2.4.1.3.1.4 | RbnVoltage Unsigned32 | 0..50000 | Current voltage level at this test point.

### 1.20.4 rbnFanSpeedTable

This table contains one row for each fan unit within a fan test point.

`Index:` rbnFanIndex, rbnFanUnitID

Table 43 describes the objects in rbnFanSpeedTable.

Table 43 Objects in rbnFanSpeedTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnFanUnitID rbnFanSpeedEntry 1 1.3.6.1.4.1.2352.2.4.1.5.1.1 | Integer32 | 1..2147483647 | This is the fan identification number that describes the specific location of the fan unit within a fan test point
rbnFanUnitDescr rbnFanSpeedEntry 2 1.3.6.1.4.1.2352.2.4.1.5.1.2 | DisplayString | 0..32 | Description of the fan unit within a fan test point. This object is only available on the SE100.
rbnFanSpeedCurrent rbnFanSpeedEntry 3 1.3.6.1.4.1.2352.2.4.1.5.1.3 | RbnFanSpeed Unsigned32 | 0..4294967295 | Current speed of this fan unit. This object is only available on the SE100.

### 1.20.5 rbnEntityTempSensorTable

This table contains one row for each physical entity temperature sensor. Each physical entity that has a temperature sensor appears here.

`Index:` entPhysicalIndex, rbnEntityTempIndex

Table 44 describes the objects in rbnEntityTempSensorTable.

Table 44 Objects in rbnEntityTempSensorTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnEntityTempIndex rbnEntityTempSensorEntry 1 1.3.6.1.4.1.2352.2.4.1.6.1.1 | Integer32 | 1..2147483647 | An arbitrary value which uniquely identifies a particular physical entity. Index values are not necessarily contiguous.
rbnEntityTempDescr rbnEntityTempSensorEntry 2 1.3.6.1.4.1.2352.2.4.1.6.1.2 | DisplayString | 0..48 | The description of a temperature test point. Typically an instance of this object will hold a user-friendly description of the physical entity being monitored by this test point.
rbnEntityTempCurrent rbnEntityTempSensorEntry 3 1.3.6.1.4.1.2352.2.4.1.6.1.3 | RbnTemperature Unsigned32 | 0..100 | The current temperature of this entity in degrees Celsius.

## 1.21 RBN-FAST-VRRP-MIB

Describes objects used for managing Fast Virtual Router Redundancy Protocol (VRRP) routers.

### 1.21.1 rbnFastVrrpOperTable

This table contains the Fast VRRP objects.

`Index:` ifIndex, rbnFastVrrpOperVrId

Table 45 describes the objects in rbnFastVrrpOperTable.

Table 45 Objects in rbnFastVrrpOperTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnFastVrrpOperVrId rbnFastVrrpOperEntry 1 11.3.6.1.4.1.2352.2.45.1.1.1.1 | VrId Integer32 | 1...255 | This object contains the Virtual Router Identifier (VRID) of Fast VRRP routers.
rbnFastVrrpOperAdvertisementInterval rbnFastVrrpOperEntry 2 21.3.6.1.4.1.2352.2.45.1.1.1.2 | Integer32 | 100...999 | The Fast VRRP advertisement messages time interval in milliseconds. This MIB object is used to replace the standard vrrpOperAdvertisementInterval (seconds) when Fast VRRP is enabled. Either vrrpOperAdvertisementInterval or rbnFastVrrpOperAdvertisementInterval is valid based on the VRRP configurations. Value is in milliseconds.

## 1.22 RBN-IP-BIND-MIB

Monitors IP interface binding to physical ports and circuits as they are represented in the IF-MIB.

### 1.22.1 rbnIpBindTable

This table shows IP interface bindings to physical ports and circuit encapsulation layers as they are represented in the IF-MIB. This table displays all IP interface bindings in all contexts but is only visible from the local context.

`Index:` ifIndex, rbnIpBindCircuitHandle

Table 46 describes the objects in rbnIpBindTable.

Table 46 Objects in rbnL2tpTunnelCntTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnIpBindCircuitHandle rbnIpBindEntry 1 1.3.6.1.4.1.2352.2.26.1.1.1.1 | RbnCircuitHandle OctetString | SIZE (8) | A unique identifier for the circuit the IP interface is bound to. The term circuit as defined in this table can represent a port, channel, sub-channel or a virtual circuit configured to run over a port, channel or sub-channel.
rbnIpBindIfIndex rbnIpBindEntry 2 1.3.6.1.4.1.2352.2.26.1.1.1.2 | InterfaceIndexOrZero Integer32 | 0..2147483647 | If the IP interface is bound to a port, channel, subchannel, or virtual circuit that is included in the IF-MIB, this object contains the ifIndex of that layer; otherwise, this object is set to zero.
rbnIpBindHierarchicalIfIndex rbnIpBindEntry 3 1.3.6.1.4.1.2352.2.26.1.1.1.3 | InterfaceIndexOrZero Integer32 | 0..2147483647 | If the IP interface is bound to a port, channel, subchannel, or virtual circuit that is not included in the IF-MIB, but that interface is part of a port stack that is included in the IF-MIB, this object contains the ifIndex of the port encapsulation layer that sits on top of that port stack. If the rbnIpBindIfIndex object is set to a nonzero value, this object is set to zero.
rbnIpBindCircuitDescr rbnIpBindEntry 4 1.3.6.1.4.1.2352.2.26.1.1.1.4 | SnmpAdminString | 0..192 | Descriptive version of the rbnIpBindCircuitHandle object that is consistent with information displayed in the CLI. On the SmartEdge router, this string is formatted as `slot/port:channel:subchannel authority/level/index`, with the exception that channel and subchannel are only included when appropriate. For example, 4/1 1/2/7, 4/1:1 1/2/7 or 4/1:1:1 1/2/7.
rbnIpBindContextName rbnIpBindEntry 5 1.3.6.1.4.1.2352.2.26.1.1.1.5 | SnmpAdminString | 0..63 | Name of the context in which this IP interface is defined.

## 1.23 RBN-IP-SECURITY-MIB

Defines the objects necessary to support the management of Internet Protocol Security (IPSec) objects.

### 1.23.1 IPSec Notification Objects

This section provides information on accessible-for-notify objects presented in the RBN-IP-SECURITY-MIB.

Table 47 describes the notification objects in RBN-IP-SECURITY-MIB.

Table 47 RBN-IP-SECURITY-MIB Notification Objects
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnIpSecEventDateAndTime rbnIpSecNotify 1 1.3.6.1.4.1.2352.2.55.1.1.1 | DateAndTime Octet String | SIZE (8) | The local date and time when the alarm was raised.
rbnIpSecEventSeverity rbnIpSecNotify 2 1.3.6.1.4.1.2352.2.55.1.1.2 | ItuPerceivedSeverity | Integer | The current severity of the alarm. See Section 1.43.6 ItuPerceivedSeverity for details.
rbnIpSecEventType rbnIpSecNotify 3 1.3.6.1.4.1.2352.2.55.1.1.3 | IANAItuEventType | Integer | The type of alarm. See Section 1.43.5 IANAItuEventType for details.
rbnIpSecEventProbableCause rbnIpSecNotify 4 1.3.6.1.4.1.2352.2.55.1.1.4 | IANAItuProbableCause | Integer | The probable cause for this alarm. See Section 1.43.4 IANAItuProbableCause for details.
rbnIpSecTunnelIdentifier rbnIpSecNotify 5 1.3.6.1.4.1.2352.2.55.1.1.5 | SnmpAdminString | 0..270 | Key to identify the tunnel alarm, consists of the remote-id type and remote-id, or tunnel name. The string starts with a substring identifying the type, followed by the value, as follows. ipv4- fqdn- rfc822Addr- ipv6- derAsn1Dn- derAsn1Gn- keyId- name-
rbnIpSecTunnelName rbnIpSecNotify 6 1.3.6.1.4.1.2352.2.55.1.1.6 | SnmpAdminString | 0..50 | A text string which conveys additional information about the alarm.
rbnIpSecTunnelType rbnIpSecNotify 7 1.3.6.1.4.1.2352.2.55.1.1.7 | Integer | 1—static 2—dynamic 3—manual | The type of tunnel.
rbnIpSecTunnelDownCause rbnIpSecNotify 8 1.3.6.1.4.1.2352.2.55.1.1.8 | Integer | 0—general 1—noRoute 2—aspHomingFailure 3—ppaHomingFailure 4—configuredDown 5—keepaliveFailure 6—downByPeer 7—rekeyFailure 8—aspSoftReset 9—indeterminate | Additional information to describe the cause for tunnel being down.
rbnIpSecRemoteIdType rbnIpSecNotify 9 1.3.6.1.4.1.2352.2.55.1.1.9 | Integer | 0—reserved 1—ipv4 2—fqdn 3—rfcAddr Values 4, 6-8, 12-200 and 201-255 are reserved for IANA 5—ipv6 9—derAsn1Dn 10—derAsn1Gn 11—keyId | Remote Id Type of rbnIpSecRemoteId.
rbnIpSecRemoteId rbnIpSecNotify 10 1.3.6.1.4.1.2352.2.55.1.1.10 | SnmpAdminString | 0..256 | Remote ID.
rbnIpSecLocalAddrContextName rbnIpSecNotify 11 1.3.6.1.4.1.2352.2.55.1.1.11 | SnmpAdminString | 0..32 | Context name of the local address.
rbnIpSecLocalAddressType rbnIpSecNotify 12 1.3.6.1.4.1.2352.2.55.1.1.12 | InetAddressType | 0—unknown 1—ipv4 2—ipv6 16—dns | Specifies the type of local address to be used.
rbnIpSecLocalAddress rbnIpSecNotify 13 1.3.6.1.4.1.2352.2.55.1.1.13 | InetAddress | 0..255 | Local IP address of the tunnel.
rbnIpSecRemoteAddressType rbnIpSecNotify 14 1.3.6.1.4.1.2352.2.55.1.1.14 | InetAddressType | 0—unknown 1—ipv4 2—ipv6 16—dns | Specifies the type of remote address to be used.
rbnIpSecRemoteAddress rbnIpSecNotify 15 1.3.6.1.4.1.2352.2.55.1.1.15 | InetAddress | 0..255 | Remote IP address of the tunnel.
rbnIpSecTunnelState rbnIpSecNotify 16 1.3.6.1.4.1.2352.2.55.1.1.16 | Integer | 1—up 2—down | Tunnel state.
rbnIpSecSelfCertificateIdentifier rbnIpSecNotify 17 1.3.6.1.4.1.2352.2.55.1.1.17 | SnmpAdminString | 0..522 | <Subject Name> :ISSUER-<Issuer name>
rbnIpSecCertificateHandle rbnIpSecNotify 18 1.3.6.1.4.1.2352.2.55.1.1.18 | Unsigned32 | 0..4294967295 | Self Certificate Handle.
rbnIpSecExpiryDateAndTime rbnIpSecNotify 19 1.3.6.1.4.1.2352.2.55.1.1.19 | SnmpAdminString | 0..128 | Date and Time the certificate will expire.
rbnIpSecCertificateSubjectName rbnIpSecNotify 20 1.3.6.1.4.1.2352.2.55.1.1.20 | SnmpAdminString | 0..256 | Subject Name of the self certificate.

## 1.24 RBN-IPPOOL-MIB

Provides information that matches the information displayed by the `show ip pool falling-threshold` command (in any mode).

The following sections contain object information for RBN-IPPOOL-MIB.

### 1.24.1 IP Pool Per-Context Objects

This section provides information on IP Pool per context objects.

Table 48 describes the IP Pool (per pool) objects in RBN-IPPOOL-MIB.

Table 48 RBN-IPPOOL-MIB Global Objects
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnIpPoolContextName rbnIpPoolSummary 1 1.3.6.1.4.1.2352.2.15.1.2.1 | SnmpAdminString | 0..63 | Name of the context containing the IPv4 pool.
rbnIpPoolContextAvailable rbnIpPoolSummary 2 1.3.6.1.4.1.2352.2.15.1.2.2 | Unsigned32 | 0..4294967295 | Total number of IP addresses available in all pools of all interfaces in the context valid in the current view.
rbnIpPoolContextThreshold rbnIpPoolSummary 3 1.3.6.1.4.1.2352.2.15.1.2.3 | Unsigned32 | 0..4294967295 | Per-context threshold of an IP pool is the value for currently available per-context addresses, as reported in the rbnIpPoolContextAvailable object, which causes a trap or log message to be generated when this value is reached. A trap or log message is sent only on a transition of the value of available address from (rbnIpPoolContextThreshold+1) addresses to rbnIpPoolContextThreshold addresses. Additionally, sending of the trap or log message is subject to the values of the rbnIpPoolContextSendTrap object and the rbnIpPoolContextLogMessage object. A value of zero means there is no per-context threshold.
rbnIpPoolContextSendTrap rbnIpPoolSummary 4 1.3.6.1.4.1.2352.2.15.1.2.4 | TruthValue Integer | 1—true 2—false | If the value of this object is true, on a per-context threshold crossing event, a trap is sent.
rbnIpPoolContextLogMessage rbnIpPoolSummary 5 1.3.6.1.4.1.2352.2.15.1.2.5 | TruthValue Integer | 1—true 2—false | If the value of this object is true, on a per-context threshold crossing event, a message is logged.
rbnIpPoolContextTotalSize rbnIpPoolSummary 6 1.3.6.1.4.1.2352.2.15.1.2.6 | Unsigned32 | 0..4294967295 | Total number of IP addresses configured in all pools of all interfaces in the context valid in the current view. The value of this object is the sum of the available addresses plus the unusable addresses.

### 1.24.2 rbnIpPoolContextThresholdPercentTable

This table monitors the status of per-context IPv4 pool percentage thresholds through SNMP. It contains the objects that identify information about per-context IP pool thresholds, expressed in percentage. Each row in the table corresponds to one IP pool percentage threshold configured within a particular context. Objects defined in this table are only accessible within the context identified in the SNMP protocol (that is, the community string in SNMPv1 or SNMPv2 or the contextName in SNMPv3).

`Index:` rbnIpPoolContextThresholdIndex

Table 49 describes the IP pool (per context) objects in rbnIpPoolContextThresholdPercentTable.

Table 49 Objects in rbnIpPoolContextThresholdPercentTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnIpPoolContextThresholdIndex rbnIpPoolContextThresholdPercentEntry 1 1.3.6.1.4.1.2352.2.15.1.2.7.1.1 | Unsigned32 | 0..4294967295 | The index of the IP Pool percentage threshold.
rbnIpPoolContextThresholdPercentage rbnIpPoolContextThresholdPercentEntry 2 1.3.6.1.4.1.2352.2.15.1.2.7.1.2 | RbnPercentage Integer32 | 0..100 | Threshold for the percentage of the number of currently available IP pool addresses against the total number of IP pool addresses configured within the context. An SNMP trap or log message is sent only when the current value, which is the percentage of the rbnIpPoolContextAvailable object and the rbnIpPoolContextTotalSize object truncated to a whole number, is less than or equal to this threshold, and the percentage value at the last check was greater than this threshold. Additionally, sending of the SNMP trap or logging a message is subject to the values of the rbnIpPoolContextThresholdSendTrap object and the rbnIpPoolContextThresholdLogMessage object.
rbnIpPoolContextThresholdSendTrap rbnIpPoolContextThresholdPercentEntry 3 1.3.6.1.4.1.2352.2.15.1.2.7.1.3 | TruthValue Integer | 1—true 2—false | If the value of this object is true, on a per-context threshold crossing event, an SNMP trap is sent.
rbnIpPoolContextThresholdLogMessage rbnIpPoolContextThresholdPercentEntry 4 1.3.6.1.4.1.2352.2.15.1.2.7.1.4 | TruthValue Integer | 1—true 2—false | If the value of this object is true, on a per-context threshold crossing event, a message is logged.

### 1.24.3 rbnIpPoolTable

This table monitors the status of IP pools through SNMP. It contains the objects that identify information about IP pools per context. Objects defined in this table are only accessible within the context identified in the SNMP protocol (that is, the community string in SNMPv1 or SNMPv2 or the contextName in SNMPv3).

Index: rbnIpPoolInterfaceIdx

Table 50 describes the objects in rbnIpPoolTable.

Table 50 Objects in rbnIpPoolTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnIpPoolInterfaceIdx rbnIpPoolEntry 1 1.3.6.1.4.1.2352.2.15.1.1.1.1 | Unsigned32 | 0..4294967295 | The index of the interface containing the IP Pool.
rbnIpPoolAddr rbnIpPoolEntry 2 1.3.6.1.4.1.2352.2.15.1.1.1.2 | IpAddress Octet String | SIZE (4) | The IPv4 starting address for the IP pool
rbnIpPoolInterfaceName rbnIpPoolEntry 3 1.3.6.1.4.1.2352.2.15.1.1.1.3 | SnmpAdminString | 0..127 | The name of the interface containing the IP pool.
rbnIpPoolMask rbnIpPoolEntry 4 1.3.6.1.4.1.2352.2.15.1.1.1.4 | IpAddress Octet String | SIZE (4) | The subnet mask of the IP pool. This object is instantiated for IP pools of type subnet only.
rbnIpPoolSize rbnIpPoolEntry 5 1.3.6.1.4.1.2352.2.15.1.1.1.5 | Unsigned32 | 0..4294967295 | The size of the IP pool is the sum of the available addresses plus the unusable addresses.
rbnIpPoolAvailable rbnIpPoolEntry 6 1.3.6.1.4.1.2352.2.15.1.1.1.6 | Unsigned32 | 0..4294967295 | The number of addresses of an IP pool that are available.
rbnIpPoolUnusable rbnIpPoolEntry 7 1.3.6.1.4.1.2352.2.15.1.1.1.7 | Unsigned32 | 0..4294967295 | Unusable IP addresses in an IP pool, consisting of the IP address of the interface and those used by the network address and the broadcast address of the interface.
rbnIpPoolInuse rbnIpPoolEntry 8 1.3.6.1.4.1.2352.2.15.1.1.1.8 | Unsigned32 | 0..4294967295 | The number of addresses of an IP pool that are in use.
rbnIpPoolThreshold rbnIpPoolEntry 9 1.3.6.1.4.1.2352.2.15.1.1.1.9 | Unsigned32 | 0..65535 | The value of currently available IP addresses, as reported in the rbnIpPoolAvailable object, which causes a trap or log message to be generated when this value is reached. This is a falling threshold, so a trap or log message is sent only on a transition of the value of available address from (rbnIpPoolThreshold+1) addresses to rbnIpPoolThreshold addresses. Additionally, the action of sending the trap or log message is subject to the values of the rbnIpPoolSendTrap object and the rbnIpPoolLogMessage object. A value of zero means there is no threshold.
rbnIpPoolSendTrap rbnIpPoolEntry 10 1.3.6.1.4.1.2352.2.15.1.1.1.10 | TruthValue Integer | 1—true 2—false | If true, on reaching a per-pool threshold event, a trap is sent.
rbnIpPoolLogMessage rbnIpPoolEntry 11 1.3.6.1.4.1.2352.2.15.1.1.1.11 | TruthValue Integer | 1—true 2—false | If true, on detection of reaching a per-pool threshold event, a message is logged.
rbnIpPoolName rbnIpPoolEntry 12 1.3.6.1.4.1.2352.2.15.1.1.1.12 | SnmpAdminString | 0..32 | The name of the IP pool.
rbnIpPoolType rbnIpPoolEntry 13 1.3.6.1.4.1.2352.2.15.1.1.1.13 | Integer | 0—subnet 1—range | The type of the IP pool.
rbnIpPoolEndAddr rbnIpPoolEntry 14 1.3.6.1.4.1.2352.2.15.1.1.1.14 | IpAddress Octet String | SIZE (4) | The end address of the IP pool. This object is instantiated for range IP pools only.

### 1.24.4 rbnInetIpPoolTable

This table monitors the status of IPv6 generic pools (for example, ND pool) per pool.

Objects defined in this table are only accessible within the context identified in the SNMP protocol (that is, the community string in SNMPv1 or SNMPv2 or the contextName in SNMPv3).

Index: rbnInetIpPoolType, rbnInetIpPoolIfIndex, rbnInetIpPoolStartPrefixType, rbnInetIpPoolPrefix, rbnInetIpPoolStartPrefixLen

Table 51 describes the objects in rbnInetIpPoolTable.

Table 51 Objects in rbnInetIpPoolTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnInetIpPoolType rbnInetIpPoolEntry 1 1.3.6.1.4.1.2352.2.15.1.3.1.1 | RbnInetPoolType Integer | 1—IPv6 2—DHCPv6 | IP pool type, either IPv6 or DHCPv6.
rbnInetIpPoolIfIndex rbnInetIpPoolEntry 2 1.3.6.1.4.1.2352.2.15.1.3.1.2 | InterfaceIndex Integer32 | 1..2147483647 | The index of the interface containing the IP Pool. The interface identified by a particular value of this index is the same interface as identified by the same value of the IF-MIB ifIndex
rbnInetIpPoolStartPrefixType rbnInetIpPoolEntry 3 1.3.6.1.4.1.2352.2.15.1.3.1.3 | InetAddressType Integer | 2—IPv6 | Address type.
rbnInetIpPoolStartPrefix rbnInetIpPoolEntry 4 1.3.6.1.4.1.2352.2.15.1.3.1.4 | InetAddress OctetString | 0..255 | The start address prefix for this pool. Any bits after rbnInetIpPoolStartPrefixLen must be zero.
rbnInetIpPoolStartPrefixLen rbnInetIpPoolEntry 5 1.3.6.1.4.1.2352.2.15.1.3.1.5 | InetAddressPrefixLength Unsigned32 | 0..128 | Advertised or delegated prefix length.
rbnInetIpPoolEndPrefixType rbnInetIpPoolEntry 6 1.3.6.1.4.1.2352.2.15.1.3.1.6 | InetAddressType Integer | 2—IPv6 | IPv6 address type; always ipv6 (2).
rbnInetIpPoolEndPrefix rbnInetIpPoolEntry 7 1.3.6.1.4.1.2352.2.15.1.3.1.7 | InetAddress OctetString | 0..255 | The end address prefix for this pool. Any bits after rbnInetIpPoolEndPrefixLen must be zero.
rbnInetIpPoolEndPrefixLen rbnInetIpPoolEntry 8 1.3.6.1.4.1.2352.2.15.1.3.1.8 | InetAddressPrefixLength Unsigned32 | 0..128 | Advertised or delegated prefix length.
rbnInetIpPoolInterfaceName rbnInetIpPoolEntry 9 1.3.6.1.4.1.2352.2.15.1.3.1.9 | SnmpAdminString OctetString | 0..255 | Name of the interface associated with the IP pool.
rbnInetIpPoolName rbnInetIpPoolEntry 10 1.3.6.1.4.1.2352.2.15.1.3.1.10 | SnmpAdminString OctetString | 0..255 | IP pool name.
rbnInetIpPoolSize rbnInetIpPoolEntry 11 1.3.6.1.4.1.2352.2.15.1.3.1.111 | Unsigned32 | 0..4294967295 | Sum of the available prefixes plus the unusable prefixes.
rbnInetIpPoolAvailable rbnInetIpPoolEntry 12 1.3.6.1.4.1.2352.2.15.1.3.1.12 | Unsigned32 | 0..4294967295 | Number of available IP address prefixes in an IP pool.
rbnInetIpPoolUnusable rbnInetIpPoolEntry 13 1.3.6.1.4.1.2352.2.15.1.3.1.13 | Unsigned32 | 0..4294967295 | Number of unusable IP address prefixes in an IP pool.
rbnInetIpPoolInuse rbnInetIpPoolEntry 14 1.3.6.1.4.1.2352.2.15.1.3.1.14 | Unsigned32 | 0..4294967295 | Number of IP address prefixes in use.
rbnInetIpPoolThrshType rbnInetIpPoolEntry 15 1.3.6.1.4.1.2352.2.15.1.3.1.15 | RbnInetIpPoolThresholdType Integer | 0—none 1—absolute; from 1 to the IP pool size (IP pool size divided by the configured percentage.) 2—percentage; from 1 to 100% of the IP pool size | Type of all threshold values in this logical row, including rbnInetIpPoolHiFallingThrsh and rbnInetIpPoolLoFallingThrsh.
rbnInetIpPoolHiFallingThrsh rbnInetIpPoolEntry 16 1.3.6.1.4.1.2352.2.15.1.3.1.16 | Unsigned32 | 0 to the IP pool size | The falling threshold of an IP pool. When the value of rbnInetIpPoolAvailable crosses from rbnInetIpPoolHiFallingThrsh + 1 to the rbnInetIpPoolHiFallingThrsh value (either absolute or percentage), an rbnInetIpPoolHiFallingThrshMet notification or log or both are generated. The value of this object should never be smaller than the value of rbnInetIpPoolLoFallingThrsh. A value of zero means that this falling threshold is not configured.
rbnInetIpPoolHiFallingNotify rbnInetIpPoolEntry 17 1.3.6.1.4.1.2352.2.15.1.3.1.17 | RbnInetIpPoolThresholdNotify Integer | 0—none 1—log file 2—trap 3—both | Specifies that the rbnInetIpPoolHiFallingThrshMet trap or log or both are generated.
rbnInetIpPoolLoFallingThrsh rbnInetIpPoolEntry 18 1.3.6.1.4.1.2352.2.15.1.3.1.18 | Unsigned32 | 0 to the IP pool size | The falling threshold of an IP pool. When the value of rbnInetIpPoolAvailable crosses from rbnInetIpPoolLoFallingThrsh + 1 to rbnInetIpPoolLoFallingThrsh (either absolute value or percentage), an rbnInetIpPoolLoFallingThrshMet notification or log or both are generated. The value of this object should never be greater than the value of rbnInetIpPoolHiFallingThrsh. A value of zero means that this falling threshold is not configured.
rbnInetIpPoolLoFallingNotify rbnInetIpPoolEntry 19 1.3.6.1.4.1.2352.2.15.1.3.1.19 | RbnInetIpPoolThresholdNotify Integer | 0—none 1—log file 2—trap 3—both | Specifies that the rbnInetIpPoolLoFallingThrshMet trap or log or both are generated.

### 1.24.5 rbnInetIpPoolCtxTable

This table monitors the status of IPv6 pools per context through SNMP.

Index: rbnInetIpPoolCtxPoolType

Objects defined in this table are only accessible within the context identified in the SNMP protocol (that is, the community string in SNMPv1 or SNMPv2 or the contextName in SNMPv3).

Table 52 describes the objects in rbnInetIpPoolCtxTable.

Table 52 Objects in rbnInetIpPoolCtxTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnInetIpPoolCtxPoolType RbnInetIpPoolCtxEntry 1 1.3.6.1.4.1.2352.2.15.1.4.2.1.1 | RbnInetPoolType Integer | 1—IPv6 2—DHCPv6 | IP pool type, either IPv6 or DHCPv6.
rbnInetIpPoolCtxAvailable RbnInetIpPoolCtxEntry 2 1.3.6.1.4.1.2352.2.15.1.4.2.1.21 | Unsigned32 | 0..4294967295 | Number of available IP address prefixes in an IP pool.
rbnInetIpPoolCtxPoolSize RbnInetIpPoolCtxEntry 3 1.3.6.1.4.1.2352.2.15.1.4.2.1.3 | Unsigned32 | 0..4294967295 | Sum of the available prefixes plus the unusable prefixes.
rbnInetIpPoolCtxThrshType RbnInetIpPoolCtxEntry 4 1.3.6.1.4.1.2352.2.15.1.4.2.1.4 | RbnInetIpPoolThresholdType Integer | 0—none 1—absolute; from 1 to the IP pool size (IP pool size divided by the configured percentage.) 2—percentage; from 1 to 100% of the IP pool size | Type of all threshold values in this logical row, including rbnInetIpPoolCtxHiFallingThrsh and rbnInetIpPoolCtxLoFallingThrsh.
rbnInetIpPoolCtxHiFallingThrsh RbnInetIpPoolCtxEntry 5 1.3.6.1.4.1.2352.2.15.1.4.2.1.5 | RbnInetIpPoolThreshold Unsigned32 | 0 to the IP pool size | The falling threshold of an IP pool. When the value of rbnInetIpCtxPoolAvailable crosses from rbnInetIpPoolCtxHiFallingThrsh + 1 to the value of rbnInetIpPoolCtxHiFallingThrsh (either absolute or percentage), an rbnInetIpPoolCtxHiFallingThrshMet notification or log or both are generated. The value of this object should never be smaller than the value of rbnInetIpPoolCtxLoFallingThrsh. A value of zero means that this falling threshold is not configured.
rbnInetIpPoolCtxHiFallingNotify RbnInetIpPoolCtxEntry 6 1.3.6.1.4.1.2352.2.15.1.4.2.1.6 | RbnInetIpPoolThresholdNotify Integer | 0—none 1—log file 2—trap 3—both | Specifies that the rbnInetIpPoolCtxHiFallingThrshMet trap or log or both are generated when triggered by a rbnInetIpPoolHiFallingThrsh event.
rbnInetIpPoolCtxLoFallingThrsh RbnInetIpPoolCtxEntry 7 1.3.6.1.4.1.2352.2.15.1.4.2.1.7 | RbnInetIpPoolThreshold Unsigned32 | 0 to the IP pool size | "The falling threshold of an IP pool. When the value of rbnInetIpPoolCtxAvailable crosses from rbnInetIpPoolCtxLoFallingThrsh + 1 to rbnInetIpPoolCtxLoFallingThrsh (either absolute value or percentage), an rbnInetIpPoolCtxLoFallingThrshMet notification or log is generated. The value of this object should never be greater than the value of rbnInetIpPoolCtxHiFallingThrsh. A value of zero means that this falling threshold is not configured.
rbnInetIpPoolCtxLoFallingNotify RbnInetIpPoolCtxEntry 8 1.3.6.1.4.1.2352.2.15.1.4.2.1.8 | RbnInetIpPoolThresholdNotify | 0—none 1—log file 2—trap 3—both | Specifies that the rbnInetIpPoolCtxLoFallingThrshMet trap or log or both are generated when triggered by a rbnInetIpPoolLoFallingThrsh event.

## 1.25 RBN-L2TP-MIB

Defines the objects used to monitor Layer 2 Tunneling Protocol (L2TP) configuration information.

### 1.25.1 rbnL2tpPeerCfgTable

This table contains objects that you can use to display information about an L2TP Peer.

`Index:` rbnL2tpMibPeerName

Table 53 describes the objects in rbnL2tpPeerCfgTable.

Table 53 Objects in rbnL2tpPeerCfgTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnL2tpMibPeerName rbnL2tpPeerCfgEntry 1 1.3.6.1.4.1.2352.2.28.1.1.1 | SnmpAdminString | 1..255 | This object identifies the name of the Peer on the local system. This peer is the name of an identifier for a tunnel configuration and each tunnel that is assigned to this peer will take on the peer's configuration parameters.
rbnL2tpPCfgMedia rbnL2tpPeerCfgEntry 2 1.3.6.1.4.1.2352.2.28.1.1.2 | SnmpAdminString | 0..10 | Transport media utilized between communicating peers. A media length of 0 means that no transport media type was set. This object is read-create.
rbnL2tpPCfgVendor rbnL2tpPeerCfgEntry 3 1.3.6.1.4.1.2352.2.28.1.1.3 | SnmpAdminString | 0..60 | Vendor of L2TP stack running on the remote peer. The length of the string is zero if no vendor name can be obtained from the peer.
rbnL2tpPCfgRev rbnL2tpPeerCfgEntry 4 1.3.6.1.4.1.2352.2.28.1.1.4 | Unsigned32 | 0..4294967295 | Firmware revision for the L2TP protocol stack running on the remote peer.
rbnL2tpPCfgHostName rbnL2tpPeerCfgEntry 5 1.3.6.1.4.1.2352.2.28.1.1.5 | SnmpAdminString | 0..255 | The name assigned to this peer on the remote host system. A host name length of 0 means that this information could not be obtained from the remote host.
rbnL2tpPCfgRadius rbnL2tpPeerCfgEntry 6 1.3.6.1.4.1.2352.2.28.1.1.6 | TruthValue Integer | 1—true 2—false | Whether a RADIUS server has been configured for this peer group. A value of true indicates that there is a RADIUS server, it is used for authenticating and authorizing access to a tunnel in this group, and accounting information is sent to the RADIUS server. A value of false indicates that there is no RADIUS server, and authentication and authorization are performed locally.
rbnL2tpPCfgRemIPAddType rbnL2tpPeerCfgEntry 7 1.3.6.1.4.1.2352.2.28.1.1.7 | InetAddressType Integer | 0—unknown 1—ipv4 2—ipv6 16—dns | The address type contained in the rbnL2tpPCfgRemIPAdd object.
rbnL2tpPCfgRemIPAdd rbnL2tpPeerCfgEntry 8 1.3.6.1.4.1.2352.2.28.1.1.8 | InetAddress Octet String | 0..255 | The remote IP address for this tunnel (utilized only with UDP). This object is read-create.
rbnL2tpPCfgStatic rbnL2tpPeerCfgEntry 9 1.3.6.1.4.1.2352.2.28.1.1.9 | TruthValue Integer | 1—true 2—false | Indicates whether the tunnel is static or dynamic. A value of true means that it is static. A value of false indicates that it is dynamic. This object is read-create.
rbnL2tpPCfgLocalIPAddType rbnL2tpPeerCfgEntry 10 1.3.6.1.4.1.2352.2.28.1.1.10 | InetAddressType Integer | 0—unknown 1—ipv4 2—ipv6 16—dns | Identifies the address type contained in the rbnL2tpPCfgLocalIPAdd object.
rbnL2tpPCfgLocalIPAdd rbnL2tpPeerCfgEntry 11 1.3.6.1.4.1.2352.2.28.1.1.11 | InetAddress Octet String | 0..255 | The local IP address for this tunnel (utilized only with UDP). This object is read-create.
rbnL2tpPCfgMode rbnL2tpPeerCfgEntry 12 1.3.6.1.4.1.2352.2.28.1.1.12 | LacLnsType Integer | 1—other 2—lac 3—lns 4—lacLns | Indicates whether the peer is operating as an LNS, a LAC, or both. This object is read-create.
rbnL2tpPCfgMaxTunnels rbnL2tpPeerCfgEntry 14 1.3.6.1.4.1.2352.2.28.1.1.14 | Gauge32 | 0..4294967295 | The maximum number of tunnels that can be configured on this peer. This object is read-create.
rbnL2tpPCfgMaxSesPerTun rbnL2tpPeerCfgEntry 15 1.3.6.1.4.1.2352.2.28.1.1.15 | Gauge32 | 0..4294967295 | The maximum number of sessions that can be allocated to one tunnel. This object is read-create.
rbnL2tpPCfgCtlRetranCnt rbnL2tpPeerCfgEntry 16 1.3.6.1.4.1.2352.2.28.1.1.16 | Counter32 | 0..4294967295 | The number of times that a control packet was retransmitted.
rbnL2tpPCfgCtlRetranTO rbnL2tpPeerCfgEntry 17 1.3.6.1.4.1.2352.2.28.1.1.17 | Unsigned32 | 0..255 | The control retransmit timeout in seconds. This object is read-create.
rbnL2tpPCfgSessAuth rbnL2tpPeerCfgEntry 18 1.3.6.1.4.1.2352.2.28.1.1.18 | AuthType Integer | 0—other 1—pap 2—chap 3—chapPap | The session authentication type. This object is read-create.
rbnL2tpPCfgCtlWin rbnL2tpPeerCfgEntry 19 1.3.6.1.4.1.2352.2.28.1.1.19 | Gauge32 | 0..65535 | The control window size. This object is read-create.
rbnL2tpPCfgDNIS rbnL2tpPeerCfgEntry 20 1.3.6.1.4.1.2352.2.28.1.1.20 | DNISType Integer | 0—other 1—dnis 2—dnisonly | Indicates whether the criteria used for a tunnel switch is Dialed Number Identification String first (a value of (1)), DNIS only (a value of (2)) or that no preference has been set (a value of (0)). This object is read-create.
rbnL2tpPCfgPoliceRate rbnL2tpPeerCfgEntry 21 1.3.6.1.4.1.2352.2.28.1.1.21 | Unsigned32 | 0..4294967295 | The received aggregate stream limit, in kilobits per second (kbps). This object is read-create.
rbnL2tpPCfgPoliceBurst rbnL2tpPeerCfgEntry 22 1.3.6.1.4.1.2352.2.28.1.1.22 | Unsigned32 | 0..4294967295 | The packet burst tolerance for tunnels received by this peer group. This object is read-create.
rbnL2tpPCfgLimitRate rbnL2tpPeerCfgEntry 23 1.3.6.1.4.1.2352.2.28.1.1.23 | Unsigned32 | 0..4294967295 | The limit of the aggregate packet stream transmitted through a tunnel in kpbs. This object is read-create.
rbnL2tpPCfgLimitBurst rbnL2tpPeerCfgEntry 24 1.3.6.1.4.1.2352.2.28.1.1.24 | Unsigned32 | 0..4294967295 | The packet burst tolerance limit transmitted on a tunnel. This object is read-create.
rbnL2tpPCfgGroup rbnL2tpPeerCfgEntry 25 1.3.6.1.4.1.2352.2.28.1.1.25 | SnmpAdminString Octet String | 0..255 | The L2TP group assigned to this peer. Each peer configuration can be assigned only one tunnel group. A length of 0 means that the group name was not assigned.
rbnL2tpPCfgPref rbnL2tpPeerCfgEntry 26 1.3.6.1.4.1.2352.2.28.1.1.26 | Unsigned32 | 0..4294967295 | The RADIUS-based preference number (used by tunnel groups only). A lower number indicates a higher preference. This object is read-create.
rbnL2tpPCfgPasswd rbnL2tpPeerCfgEntry 27 1.3.6.1.4.1.2352.2.28.1.1.27 | SnmpAdminString Octet String | 0..20 | The password used for this account when performing the connection handshake protocol with the remote host. A length of 0 indicates that no password has been assigned. This object is read-create.
rbnL2tpPCfgHelloTimer rbnL2tpPeerCfgEntry 28 1.3.6.1.4.1.2352.2.28.1.1.28 | Unsigned32 | 0..3600 | The interval (in seconds) in which Hello (or keepalive) packets are sent by local tunnels belonging to this tunnel configuration. This object is read-create.
rbnL2tpPCfgRecQue rbnL2tpPeerCfgEntry 29 1.3.6.1.4.1.2352.2.28.1.1.29 | TruthValue Integer | 1—true 2—false | Indicates whether there is receive queueing of out-of-sequence messages. A value of true indicates that the messages are queued.
rbnL2tpPCfgSessContext rbnL2tpPeerCfgEntry 30 1.3.6.1.4.1.2352.2.28.1.1.30 | SnmpAdminString Octet String | 0..80 | The name of the session context. A size of 0 indicates that the context could not be determined. Any context name length greater than 80 is truncated. This object holds a value for PPPoE only. This object is read-create.
rbnL2tpPCfgSessService rbnL2tpPeerCfgEntry 31 1.3.6.1.4.1.2352.2.28.1.1.31 | SnmpAdminString Octet String | 0..20 | The service group to which this session belongs. A length of 0 indicates that no service group was assigned. This object is read-create.
rbnL2tpPCfgEthEncap rbnL2tpPeerCfgEntry 32 1.3.6.1.4.1.2352.2.28.1.1.32 | EthEncapType Integer | 0—other 1—ethPpoe 2—ethMulti 3—ethernet | The Ethernet encapsulation type. This object is read-create.
rbnL2tpPCfgEthSession rbnL2tpPeerCfgEntry 33 1.3.6.1.4.1.2352.2.28.1.1.33 | SnmpAdminString Octet String | 0..20 | The Ethernet session of which this is a part. This object is set only for non-PPPoE sessions; otherwise, it has a zero length. This object is read-create.
rbnL2tpPCfgTunnelCount rbnL2tpPeerCfgEntry 34 1.3.6.1.4.1.2352.2.28.1.1.34 | Counter32 | 0..4294967295 | The number of tunnels that are active for this peer configuration. This object is read-create.
rbnL2tpPCfgTunCtlErrs rbnL2tpPeerCfgEntry 35 1.3.6.1.4.1.2352.2.28.1.1.35 | Counter32 | 0..4294967295 | The number of tunnel control errors encountered by tunnels connected to this peer.
rbnL2tpPCfgSessionCount rbnL2tpPeerCfgEntry 36 1.3.6.1.4.1.2352.2.28.1.1.36 | Counter32 | 0..4294967295 | The of sessions that are part of this peer.

### 1.25.2 rbnL2tpTunnelCfgTable

This table contains objects related to L2TP Tunnel information.

`Index:` rbnL2tpMibTunnelID

Table 54 describes the objects in rbnL2tpTunnelCfgTable, L2TP Peer Information Table.

Table 54 Objects in rbnL2tpPeerCfgTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnL2tpMibTunnelID rbnL2tpTunnelCfgEntry 1 1.3.6.1.4.1.2352.2.28.1.2.1.1 | Unsigned32 | 0..65535 | The identification number of a tunnel.
rbnL2tpTCfgTunnelNm rbnL2tpTunnelCfgEntry 2 1.3.6.1.4.1.2352.2.28.1.2.1.2 | SnmpAdminString | 1..80 | The local name of the tunnel.
rbnL2tpTCfgPeerName rbnL2tpTunnelCfgEntry 3 1.3.6.1.4.1.2352.2.28.1.2.1.3 | SnmpAdminString | 1..80 | The remote peer to which this tunnel is connected.
rbnL2tpTCfgTunCtlErrs rbnL2tpTunnelCfgEntry 4 1.3.6.1.4.1.2352.2.28.1.2.1.4 | Counter32 | 0..4294967295 | The number of tunnel control errors encountered by this tunnel.
rbnL2tpTCfgLastCtlErr rbnL2tpTunnelCfgEntry 5 1.3.6.1.4.1.2352.2.28.1.2.1.5 | CtlErrType | Integer | The value of the last control error. See Section 1.43.7 CtlErrType for details.
rbnL2tpTCfgLastCErrTime rbnL2tpTunnelCfgEntry 6 1.3.6.1.4.1.2352.2.28.1.2.1.6 | DateAndTime Octet String | SIZE (8) | The time of the last control error.
rbnL2tpTCfgTunDataErrs rbnL2tpTunnelCfgEntry 7 1.3.6.1.4.1.2352.2.28.1.2.1.7 | Counter32 | 0..4294967295 | The number of tunnel data errors.
rbnL2tpTCfgLastDataErr rbnL2tpTunnelCfgEntry 8 1.3.6.1.4.1.2352.2.28.1.2.1.8 | Unsigned32 | 0..4294967295 | The value of the last tunnel data error.
rbnL2tpTCfgLastDErrTime rbnL2tpTunnelCfgEntry 9 1.3.6.1.4.1.2352.2.28.1.2.1.9 | DateAndTime Octet String | SIZE (8) | The time of the last tunnel data error.
rbnL2tpTCfgSessionCount rbnL2tpTunnelCfgEntry 10 1.3.6.1.4.1.2352.2.28.1.2.1.10 | Gauge32 | 0..4294967295 | The number of sessions belonging to this tunnel.
rbnL2tpTCfgTotActSessions rbnL2tpTunnelCfgEntry 11 1.3.6.1.4.1.2352.2.28.1.2.1.11 | Counter32 | 0..4294967295 | The total number of sessions that, at some time, reached the established state.
rbnL2tpTCfgActSessCnt rbnL2tpTunnelCfgEntry 12 1.3.6.1.4.1.2352.2.28.1.2.1.12 | Gauge32 | 0..4294967295 | The total number of sessions that are presently in the established state.
rbnL2tpTCfgTotFailSessions rbnL2tpTunnelCfgEntry 13 1.3.6.1.4.1.2352.2.28.1.2.1.13 | Counter32 | 0..4294967295 | The number of sessions that failed to reach the established state.
rbnL2tpMibTunnelState rbnL2tpTunnelCfgEntry 14 1.3.6.1.4.1.2352.2.28.1.2.1.14 | TunStateType Integer | 0—invalid 1—deleted 2—idle 3—created 4—waitAAA 5—waitCtlReply 6—waitCtlConn 7—established 8—waitRouteUp | The current state of the tunnel.
rbnL2tpTCfgRemoteTunnelID rbnL2tpTunnelCfgEntry 15 1.3.6.1.4.1.2352.2.28.1.2.1.15 | Unsigned32 | 0..65535 | The remote tunnel ID. A value of zero indicates that the remote tunnel ID could not be determined.
rbnL2tpTCfgTunnelContext rbnL2tpTunnelCfgEntry 16 1.3.6.1.4.1.2352.2.28.1.2.1.16 | SnmpAdminString | 0..80 | Identifies the context of this tunnel. The empty context name (zero length) indicates that the context could not be determined. Any context name length greater than 80 is truncated.

### 1.25.3 rbnL2tpPeerCntTable

This table contains objects related to the L2TP Peer Statistics Table.

`Index:` IMPLIED rbnL2tpMibPeerName

Table 55 describes the objects in rbnL2tpPeerCntTable.

Table 55 Objects in rbnL2tpPeerCntTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnL2tpPCDataPktSent rbnL2tpPeerCntEntry 1 1.3.6.1.4.1.2352.2.28.1.4.1.1 | Counter32 | 0..4294967295 | A count of the total number of data packets sent through tunnels that are part of this group to the L2TP peer.
rbnL2tpPCDataPktRx rbnL2tpPeerCntEntry 2 1.3.6.1.4.1.2352.2.28.1.4.1.2 | Counter32 | 0..4294967295 | A count of the total number of data packets received through tunnels that are part of this group from the L2TP peer.
rbnL2tpPCDataByteSent rbnL2tpPeerCntEntry 3 1.3.6.1.4.1.2352.2.28.1.4.1.3 | Counter32 | 0..4294967295 | Number of data bytes sent through tunnels that are part of this group to the L2TP peer.
rbnL2tpPCDataByteRx rbnL2tpPeerCntEntry 4 1.3.6.1.4.1.2352.2.28.1.4.1.4 | Counter32 | 0..4294967295 | Number of data bytes received through tunnels that are part of this group from the L2TP peer.
rbnL2tpPCCtlPktSent rbnL2tpPeerCntEntry 5 1.3.6.1.4.1.2352.2.28.1.4.1.5 | Counter32 | 0..4294967295 | Number of control packets sent through tunnels that are part of this group to the L2TP peer.
rbnL2tpPCCtlPktRx rbnL2tpPeerCntEntry 6 1.3.6.1.4.1.2352.2.28.1.4.1.6 | Counter32 | 0..4294967295 | Number of control packets received through tunnels that are a part of this group from the L2TP peer.
rbnL2tpPCCtlByteSent rbnL2tpPeerCntEntry 7 1.3.6.1.4.1.2352.2.28.1.4.1.7 | Counter32 | 0..4294967295 | Number of control bytes sent through tunnels that are a part of this group to the L2TP peer.
rbnL2tpPCCtlByteRx rbnL2tpPeerCntEntry 8 1.3.6.1.4.1.2352.2.28.1.4.1.8 | Counter32 | 0..4294967295 | Number of control bytes received through tunnels that are a part of this group from the L2TP peer.
rbnL2tpPCPolicePktDrop rbnL2tpPeerCntEntry 9 1.3.6.1.4.1.2352.2.28.1.4.1.9 | Counter32 | 0..4294967295 | Number of packets received from L2TP peers of tunnels that are a part of this group that were dropped.
rbnL2tpPCRatePktDrop rbnL2tpPeerCntEntry 10 1.3.6.1.4.1.2352.2.28.1.4.1.10 | Counter32 | 0..4294967295 | Number of packets transmitted to the L2TP peers of tunnels in this group that were dropped.
rbnL2tpPCTxSCCRQCnt rbnL2tpPeerCntEntry 11 1.3.6.1.4.1.2352.2.28.1.4.1.11 | Counter32 | 0..4294967295 | Number of SCCRQ transmits for this group.
rbnL2tpPCRxSCCRQCnt rbnL2tpPeerCntEntry 12 1.3.6.1.4.1.2352.2.28.1.4.1.12 | Counter32 | 0..4294967295 | Number of received SCCRQs for this group.
rbnL2tpPCActTunnels rbnL2tpPeerCntEntry 13 1.3.6.1.4.1.2352.2.28.1.4.1.13 | Counter32 | 0..4294967295 | Number of active tunnels for this group.
rbnL2tpPCTunnelCtlErr rbnL2tpPeerCntEntry 14 1.3.6.1.4.1.2352.2.28.1.4.1.14 | Counter32 | 0..4294967295 | Number of tunnel control errors for all of the tunnels that are a part of this group.
rbnL2tpPCSessionCount rbnL2tpPeerCntEntry 15 1.3.6.1.4.1.2352.2.28.1.4.1.15 | Counter32 | 0..4294967295 | Number of sessions for this group.
rbnL2tpPCTunnelDataErr rbnL2tpPeerCntEntry 16 1.3.6.1.4.1.2352.2.28.1.4.1.16 | Counter32 | 0..4294967295 | Number of tunnel data errors reported by members of this group.

### 1.25.4 rbnL2tpTunnelCntTable

This table contains objects related to L2TP tunnel statistics.

`Index:` rbnL2tpMibTunnelID

Table 56 describes the objects in rbnL2tpTunnelCntTable.

Table 56 Objects in rbnL2tpTunnelCntTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnL2tpTCDataPktSent rbnL2tpTunnelCntEntry 1 1.3.6.1.4.1.2352.2.28.1.5.1.1 | Counter32 | 0..4294967295 | Number of data packets sent from this platform through this tunnel to its peer.
rbnL2tpTCDataPktRcvd rbnL2tpTunnelCntEntry 2 1.3.6.1.4.1.2352.2.28.1.5.1.2 | Counter32 | 0..4294967295 | Number of packets received from the L2TP peer for this tunnel.
rbnL2tpTCDataByteSent rbnL2tpTunnelCntEntry 3 1.3.6.1.4.1.2352.2.28.1.5.1.3 | Counter32 | 0..4294967295 | Number of data bytes sent from this platform through this tunnel to its peer.
rbnL2tpTCDataByteRcvd rbnL2tpTunnelCntEntry 4 1.3.6.1.4.1.2352.2.28.1.5.1.4 | Counter32 | 0..4294967295 | Number of data bytes received from the L2TP peer for this tunnel.
rbnL2tpTCCntrlPktSent rbnL2tpTunnelCntEntry 5 1.3.6.1.4.1.2352.2.28.1.5.1.5 | Counter32 | 0..4294967295 | Number of control packets sent from this platform through this tunnel to its L2TP peer.
rbnL2tpTCCntrlPktRcvd rbnL2tpTunnelCntEntry 6 1.3.6.1.4.1.2352.2.28.1.5.1.6 | Counter32 | 0..4294967295 | Number of control packets received from the L2TP peer for this tunnel.
rbnL2tpTCCntrlByteSent rbnL2tpTunnelCntEntry 7 1.3.6.1.4.1.2352.2.28.1.5.1.7 | Counter32 | 0..4294967295 | Number of control bytes sent from this platform through this tunnel to its L2TP peer.
rbnL2tpTCCntrlByteRcvd rbnL2tpTunnelCntEntry 8 1.3.6.1.4.1.2352.2.28.1.5.1.8 | Counter32 | 0..4294967295 | Number of control bytes received from the L2TP peer of this tunnel.
rbnL2tpTCPolicePktDrop rbnL2tpTunnelCntEntry 9 1.3.6.1.4.1.2352.2.28.1.5.1.9 | Counter32 | 0..4294967295 | Number of packets received from the L2TP peer of this tunnel that were dropped.
rbnL2tpTCRatePktDrop rbnL2tpTunnelCntEntry 10 1.3.6.1.4.1.2352.2.28.1.5.1.10 | Counter32 | 0..4294967295 | Number of packets transmitted from this platform through this tunnel that were dropped.
rbnL2tpTCCntrlErr rbnL2tpTunnelCntEntry 11 1.3.6.1.4.1.2352.2.28.1.5.1.11 | Unsigned32 | 0..4294967295 | Number of control errors that were detected.
rbnL2tpTCLastCtlErr rbnL2tpTunnelCntEntry 12 1.3.6.1.4.1.2352.2.28.1.5.1.12 | CtlErrType | Integer | The value of the last control error. See Section 1.43.7 CtlErrType for details.
rbnL2tpTCLastCtlErrTime rbnL2tpTunnelCntEntry 13 1.3.6.1.4.1.2352.2.28.1.5.1.13 | DateAndTime Octet String | SIZE (8) | The time that the last control error for this tunnel was detected.
rbnL2tpTCMaxResendQ rbnL2tpTunnelCntEntry 14 1.3.6.1.4.1.2352.2.28.1.5.1.14 | Gauge32 | 0..4294967295 | The maximum length of the resend queue.
rbnL2tpTCMaxUnsentQ rbnL2tpTunnelCntEntry 15 1.3.6.1.4.1.2352.2.28.1.5.1.15 | Gauge32 | 0..4294967295 | The maximum length of the unsent queue.
rbnL2tpTCCurResendQ rbnL2tpTunnelCntEntry 16 1.3.6.1.4.1.2352.2.28.1.5.1.16 | Gauge32 | 0..4294967295 | The current length of the resend queue.
rbnL2tpTCCurUnsentQ rbnL2tpTunnelCntEntry 17 1.3.6.1.4.1.2352.2.28.1.5.1.17 | Gauge32 | 0..4294967295 | The current length of the unsent queue.
rbnL2tpTCCurWindow rbnL2tpTunnelCntEntry 18 1.3.6.1.4.1.2352.2.28.1.5.1.18 | Gauge32 | 0..4294967295 | The current window size.

### 1.25.5 rbnL2tpSessionCntTable

This table contains objects related to L2TP Statistics.

`Index:` rbnL2tpMibTunnelID, rbnL2tpMibSessionID

Table 57 describes the objects in rbnL2tpSessionCntTable.

Table 57 Objects in rbnL2tpSessionCntTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnL2tpMibSessionID rbnL2tpSessionCntEntry 1 1.3.6.1.4.1.2352.2.28.1.6.1.1 | Unsigned32 | 0..65535 | Identifies the Session ID for a given L2TP session.
rbnL2tpSCPktSent rbnL2tpSessionCntEntry 2 1.3.6.1.4.1.2352.2.28.1.6.1.2 | Counter32 | 0..4294967295 | The number of packets sent by this platform in this session.
rbnL2tpSCPktRcvd rbnL2tpSessionCntEntry 3 1.3.6.1.4.1.2352.2.28.1.6.1.3 | Counter32 | 0..4294967295 | The number of packets received by this platform in this session.
rbnL2tpSCByteSent rbnL2tpSessionCntEntry 4 1.3.6.1.4.1.2352.2.28.1.6.1.4 | Counter32 | 0..4294967295 | The number of bytes sent by this platform in this session.
rbnL2tpSCByteRcvd rbnL2tpSessionCntEntry 5 1.3.6.1.4.1.2352.2.28.1.6.1.5 | Counter32 | 0..4294967295 | The number of bytes received by this platform in this session.
rbnL2tpSCMcastPktSent rbnL2tpSessionCntEntry 6 1.3.6.1.4.1.2352.2.28.1.6.1.6 | Counter64 | 0..18446744073709551615 | The number of multicast packets sent by this platform in this session.
rbnL2tpSCMcastPktRcvd rbnL2tpSessionCntEntry 7 1.3.6.1.4.1.2352.2.28.1.6.1.7 | Counter64 | 0..18446744073709551615 | The number of multicast packets received by this platform in this session.
rbnL2tpSCMcastByteSent rbnL2tpSessionCntEntry 8 1.3.6.1.4.1.2352.2.28.1.6.1.8 | Counter64 | 0..18446744073709551615 | The number of multicast bytes sent by this platform in this session.
rbnL2tpSCMcastByteRcvd rbnL2tpSessionCntEntry 9 1.3.6.1.4.1.2352.2.28.1.6.1.9 | Counter64 | 0..18446744073709551615 | The number of multicast bytes received by this platform in this session.

### 1.25.6 rbnL2tpPeerTunCfgTable

This table contains objects which identify L2TP peers and tunnels.

`Index:` rbnL2tpMibPeerName, rbnL2tpMibTunnelID

Table 58 describes the objects in rbnL2tpPeerTunCfgTable.

Table 58 Objects in rbnL2tpPeerTunCfgTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnL2tpPTCfgTunnelRemoteID rbnL2tpPeerTunCfgEntry 1 1.3.6.1.4.1.2352.2.28.1.8.1.1 | Unsigned32 | 0..65535 | The remote tunnel ID. A value of zero indicates that the remote tunnel ID could not be determined.
rbnL2tpPTCfgTunnelLocalNm rbnL2tpPeerTunCfgEntry 2 1.3.6.1.4.1.2352.2.28.1.8.1.2 | SnmpAdminString | 0..80 | The local name that was given to this tunnel. The length of the string is zero if no local name assigned to the tunnel.
rbnL2tpPTCfgTunnelRemoteNm rbnL2tpPeerTunCfgEntry 3 1.3.6.1.4.1.2352.2.28.1.8.1.3 | SnmpAdminString | 1..80 | The name that was given to the remote end of this tunnel. The length of the string is zero if no tunnel name can be obtained from the peer.
rbnL2tpPTCfgPeerLocalNm rbnL2tpPeerTunCfgEntry 4 1.3.6.1.4.1.2352.2.28.1.8.1.4 | SnmpAdminString | 0..80 | The local peer name. The empty peer name (zero length) indicates that the name could not be determined.
rbnL2tpPTCfgTunnelRemoteIPAddrType rbnL2tpPeerTunCfgEntry 5 1.3.6.1.4.1.2352.2.28.1.8.1.5 | InetAddressType Integer | 0—unknown 1—ipv4 2—ipv6 16—dns | The address type contained in the rbnL2tpPTCfgTunnelRemoteIPAddr object.
rbnL2tpPTCfgTunnelRemoteIPAddr rbnL2tpPeerTunCfgEntry 6 1.3.6.1.4.1.2352.2.28.1.8.1.6 | InetAddress Octet String | 0..255 | The remote IP address for this tunnel (utilized only with UDP).
rbnL2tpPTCfgTunnelState rbnL2tpPeerTunCfgEntry 7 1.3.6.1.4.1.2352.2.28.1.8.1.7 | TunStateType Integer | 0—invalid 1—deleted 2—idle 3—created 4—waitAAA 5—waitCtlReply 6—waitCtlConn 7—established 8—waitRouteUp | The current state of the tunnel.
rbnL2tpPTCfgTunnelContext rbnL2tpPeerTunCfgEntry 8 1.3.6.1.4.1.2352.2.28.1.8.1.8 | SnmpAdminString | 0..80 | The context of this tunnel. The empty context name (zero length) indicates that the context could not be determined. Any context name length greater than 80 is truncated.
rbnL2tpPTCfgSessionCount rbnL2tpPeerTunCfgEntry 9 1.3.6.1.4.1.2352.2.28.1.8.1.9 | Gauge32 | 0..4294967295 | The number of sessions belonging to this tunnel.
rbnL2tpPTCfgActSessCnt rbnL2tpPeerTunCfgEntry 10 1.3.6.1.4.1.2352.2.28.1.8.1.10 | Gauge32 | 0..4294967295 | The total number of sessions that are presently in the established state.
rbnL2tpPTCfgTotActSessions rbnL2tpPeerTunCfgEntry 11 1.3.6.1.4.1.2352.2.28.1.8.1.11 | Counter32 | 0..4294967295 | The total number of sessions that, at some time, reached the established state.
rbnL2tpPTCfgTotFailSessions rbnL2tpPeerTunCfgEntry 12 1.3.6.1.4.1.2352.2.28.1.8.1.12 | Counter32 | 0..4294967295 | The number of sessions that failed to reach the established state.

## 1.26 RBN-L2VPN-MIB

Provides data that matches the information displayed when entering the `show l2vpn` command (in any mode) using the `xc` option.

Table 59 describes the scalar object in static Layer 2 VPN circuits.

Table 59 Scalar Object in rbnMplsL2VpnStaticTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnMplsL2VpnNotificationEnable 1.3.6.4.1.2352.2.39.5.1 rbnMplsL2VpnMIBScalars | Integer | 1—true 2—false | Displays whether traps are SNMP traps are enabled on an L2VPN XC at the global level (in an L2VPN profile).

### 1.26.1 rbnMplsL2VpnStaticTable

This table contains objects that identify static Layer 2 VPN circuits. Rows in this table are created or deleted when the VPN circuit is configured.

`Index:` rbnMplsL2VpnStaticVpnLabel, rbnMplsL2VpnStaticPeerAddr

Table 60 describes the objects in rbnMplsL2VpnStaticTable.

Table 60 Objects in rbnMplsL2VpnStaticTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnMplsL2VpnStaticVpnLabel rbnMplsL2VpnStaticEntry 1 1.3.6.1.4.1.2352.2.39.3.3.1.1 | Unsigned32 | 4096..65535 | This object indicates the unique value assigned to a particular 548 static VPN circuit.
rbnMplsL2VpnStaticPeerAddr rbnMplsL2VpnStaticEntry 2 1.3.6.1.4.1.2352.2.39.3.3.1.2 | IpAddress Octet string | SIZE (4) | This object indicates the IP address of the VPN peer.
rbnMplsL2VpnStaticCctHandle rbnMplsL2VpnStaticEntry 3 1.3.6.1.4.1.2352.2.39.3.3.1.3 | RbnCircuitHandle Octet String | SIZE (8) | The internal representation of the physical circuit to which this VPN is connected. A hexidecimal value of ff ff ff ff ff ff ff ff indicates an invalid circuit.
rbnMplsL2VpnStaticVpnCctHandle rbnMplsL2VpnStaticEntry 4 1.3.6.1.4.1.2352.2.39.3.3.1.4 | RbnCircuitHandle Octet String | SIZE (8) | The internal representation of the VPN pseudo-circuit.
rbnMplsL2VpnStaticExpBits rbnMplsL2VpnStaticEntry 5 1.3.6.1.4.1.2352.2.39.3.3.1.5 | Unsigned32 | 0..4294967295 | The number of EXP bits configured for this VPN circuit.
rbnMplsL2VpnStaticInputCctUp rbnMplsL2VpnStaticEntry 6 1.3.6.1.4.1.2352.2.39.3.3.1.6 | TruthValue Integer | 1—true 2—false | The status of the VPN attachment circuit. A value of true indicates that the VPN attachment circuit is connected with its remote site. A value of false indicates that the remote site is not presently connected.
rbnMplsL2VpnStaticXcFlags rbnMplsL2VpnStaticEntry 7 1.3.6.1.4.1.2352.2.39.3.3.1.7 | RbnVpnXcFlagsType | Integer | Indicates more detailed information on the status of the VPN circuit. This object is a bit field, so it may contain one or more of these values. See Section 1.43.8 RbnVpnXcFlagsType and RbnVpnPwFlagsType for details.
rbnMplsL2VpnStaticIfIndexOrZero rbnMplsL2VpnStaticEntry 8 1.3.6.1.4.1.2352.2.39.3.3.1.8 | InterfaceIndexOrZero Integer32 | 0..2147483647 | Indicates whether there is a corresponding entry in ifTable. A nonzero value indicates the ifIndex of the entry in ifTable. A value of zero indicates that there is no entry.
rnbMplsL2VpnStaticPwFlags rbnMplsL2VpnStaticEntry 9 1.3.6.1.4.2352.2.39.3.3.1.9 | RbnVpnPwFlagsType | Integer | Provides more detailed information on the status of the VPN circuit. This object is a bit field so it may contain one or more of these values. See Section 1.43.8 RbnVpnXcFlagsType and RbnVpnPwFlagsType for details.
rbnMplsL2VpnStaticPwState rbnMplsL2VpnStaticEntry 10 1.3.6.1.4.1.2352.2.39.3.3.1.10 | RbnVpnPwStateType Integer | 0—unknown 1—up 2—down 3—standby | This object indicates the status of this UDP L2 VPN circuit. unknown (0) up (1) indicates that the VPN circuit is active i.e. connected with its remote site. down (2) indicates that the remote site is not presently connected. standby (3) indicates that the PW is in pending state to become active (i.e. up).
rbnMplsL2VpnStaticInLabel rbnMplsL2VpnStaticEntry 11 1.3.6.1.4.1.2352.2.39.3.3.1.11 | Unsigned 32 | 0..42949672 | The value used by the remote connection to identify this VPN circuit when communicating with the local manager.

### 1.26.2 rbnMplsL2VpnLdpTable

This table contains objects that identify Layer Distribution Protocol Layer 2 VPN circuits. Rows in this table are created or deleted when the VPN circuit is configured.

`Index:` rbnMplsL2VpnLdpPeerAddr, rbnMplsL2VpnLdpVcId

Table 61 describes the objects in rbnMplsL2VpnLdpTable.

Table 61 Objects in rbnMplsL2VpnLdpTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnMplsL2VpnLdpVcId rbnMplsL2VpnLdpEntry 1 1.3.6.1.4.1.2352.2.39.3.4.1.1 | Unsigned32 | 0..4294967295 | This object indicates the unique virtual VPN circuit id assigned 675 to this circuit.
rbnMplsL2VpnLdpPeerAddr rbnMplsL2VpnLdpEntry 2 1.3.6.1.4.1.2352.2.39.3.4.1.2 | IpAddress Octet String | SIZE (4) | This object indicates the IP address if the VPN peer.
rbnMplsL2VpnLdpCctHandle rbnMplsL2VpnLdpEntry 3 1.3.6.1.4.1.2352.2.39.3.4.1.3 | RbnCircuitHandle Octet String | SIZE (8) | The internal representation of the physical circuit to which this VPN is connected. A hexidecimal value of ff ff ff ff ff ff ff ff indicates an invalid circuit.
rbnMplsL2VpnLdpVpnCctHandle rbnMplsL2VpnLdpEntry 4 1.3.6.1.4.1.2352.2.39.3.4.1.4 | RbnCircuitHandle Octet String | SIZE (8) | The internal representation of the VPN pseudo-circuit.
rbnMplsL2VpnLdpInLabel rbnMplsL2VpnLdpEntry 5 1.3.6.1.4.1.2352.2.39.3.4.1.5 | Unsigned32 | 0..4294967295 | The value used by the remote connection to identify this VPN circuit when communicating with the local manager.
rbnMplsL2VpnLdpVpnLabel rbnMplsL2VpnLdpEntry 6 1.3.6.1.4.1.2352.2.39.3.4.1.6 | Unsigned32 | 0..4294967295 | The value setup in the local configuration to identify this VPN circuit.
rbnMplsL2VpnLdpRemGrpId rbnMplsL2VpnLdpEntry 7 1.3.6.1.4.1.2352.2.39.3.4.1.7 | Unsigned32 | 0..4294967295 | The remote group of which this VPN circuit is a part.
rbnMplsL2VpnLdpLocEncap rbnMplsL2VpnLdpEntry 8 1.3.6.1.4.1.2352.2.39.3.4.1.8 | SnmpAdminString | 0..80 | The local encapsulation type associated with this VPN circuit.
rbnMplsL2VpnLdpRemEncap rbnMplsL2VpnLdpEntry 9 1.3.6.1.4.1.2352.2.39.3.4.1.9 | SnmpAdminString | 0..80 | The remote encapsulation type associated with this VPN circuit.
rbnMplsL2VpnLdpLocVcType rbnMplsL2VpnLdpEntry 10 1.3.6.1.4.1.2352.2.39.3.4.1.10 | RbnVpnVcType Integer | 0—unknown 1—frame 2—aal5 3—atmTransCell 4—vlan 5—ethernet 6—hdlc 7—ppp 8—cem 9—atmVccCell 10—atmVpcCell | The type of virtual circuit on the local system.
rbnMplsL2VpnLdpRemVcType rbnMplsL2VpnLdpEntry 11 1.3.6.1.4.1.2352.2.39.3.4.1.11 | RbnVpnVcType Integer | 0—unknown 1—frame 2—aal5 3—atmTransCell 4—vlan 5—ethernet 6—hdlc 7—ppp 8—cem 9—atmVccCell 10—atmVpcCell | The type of virtual circuit on the remote system.
rbnMplsL2VpnLdpLocMtu rbnMplsL2VpnLdpEntry 12 1.3.6.1.4.1.2352.2.39.3.4.1.12 | Unsigned32 | 0..4294967295 | The maximum transmission unit of the local VPN circuit.
rbnMplsL2VpnLdpRemMtu rbnMplsL2VpnLdpEntry 13 1.3.6.1.4.1.2352.2.39.3.4.1.13 | Unsigned32 | 0..4294967295 | The maximum transmission unit of the remote connection.
rbnMplsL2VpnLdpXcCctUp rbnMplsL2VpnLdpEntry 14 1.3.6.1.4.1.2352.2.39.3.4.1.14 | TruthValue Integer | 1—true 2—false | The status of the VPN cross-connect circuit. A value of true indicates that the VPN circuit is connected with its remote site and attachment circuit is up (rbnMplsL2VpnLdpInputCctUp is true). A value of false indicates that the remote site is not connected; this mean that either the PSN is not reachable or the attachment circuit is down or signaling parameters mismatched.
rbnMplsL2VpnLdpExpBits rbnMplsL2VpnLdpEntry 15 1.3.6.1.4.1.2352.2.39.3.4.1.15 | Unsigned32 | 0..4294967295 | The number of EXP bits configured for this VPN circuit.
rbnMplsL2VpnLdpInputCctUp rbnMplsL2VpnLdpEntry 16 1.3.6.1.4.1.2352.2.39.3.4.1.16 | TruthValue Integer | 1—true 2—false | The status of the VPN attachment circuit. A value of true indicates that the VPN attachment circuit is up. A value of false indicates that the remote site is down.
rbnMplsL2VpnLdpXcFlags rbnMplsL2VpnLdpEntry 17 1.3.6.1.4.1.2352.2.39.3.4.1.17 | RbnVpnXcFlagsType | Integer | More detailed information on the status of the VPN circuit. This object is a bit field, so it may contain one or more of these values. See Section 1.43.8 RbnVpnXcFlagsType and RbnVpnPwFlagsType for details.
rbnMplsL2VpnLdpIfIndexOrZero rbnMplsL2VpnLdpEntry 18 1.3.6.1.4.1.2352.2.39.3.4.1.18 | InterfaceIndexOrZero Integer32 | 0..2147483647 | Indicates whether there is a corresponding entry in ifTable. A nonzero value indicates the ifIndex of the entry in ifTable. A value of zero indicates that there is no entry.
rbnMplsL2VpnLdpPwFlags rbnMplsL2VpnLdpEntry 19 1.3.6.1.4.1.2352.2.39.3.4.1.19 | RbnVpnPwFlagsType | Integer | Indicates more detailed information on the status of the VPN circuit. This object is a bit field so it may contain one or more of these values. See Section 1.43.8 RbnVpnXcFlagsType and RbnVpnPwFlagsType for details.
rbnMplsL2VpnLdpPwState rbnMplsL2VpnLdpEntry 20 1.3.6.4.1.2352.2.39.3.4.1.20 | RbnVpnPwStateType Integer | 0—unknown 1—up 2—down 3—standby | This object indicates the status of this UDP L2 VPN circuit. unknown (0) up (1) indicates that the VPN circuit is active i.e. connected with its remote site. down (2) indicates that the remote site is not presently connected. standby (3) indicates that the PW is in pending state to become active (i.e. up).

### 1.26.3 rbnUdpL2VpnStaticTable

This table contains objects which identify static UDP Layer 2 VPN circuits. With respect to creation and deletion of entries in this table, rows are created or deleted when the VPN circuit is configured.

`Index:` rbrbnUdpL2VpnStaticPeerPort, rbnUdpL2VpnStaticPeerAddressType, rbnUdpL2VpnStaticPeerAddress

Table 62 describes the objects in rbnUdpL2VpnStaticTable.

Table 62 Objects in rbnUdpL2VpnStaticTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnUdpL2VpnStaticPeerPort rbnUdpL2VpnStaticEntry 1 1.3.6.1.4.1.2352.2.39.6.1.1.1 | InetPortNumber Unsigned32 | 1..65535 | This object indicates the peer port number for this UDP L2 VPN circuit.
rbnUdpL2VpnStaticPeerAddressType rbnUdpL2VpnStaticEntry 2 1.3.6.1.4.1.2352.2.39.6.1.1.2 | InetAddressType Integer | 1—ipv4 | This object indicates the peer IP address type for this UDP L2 VPN circuit.
rbnUdpL2VpnStaticPeerAddress rbnUdpL2VpnStaticEntry 3 1.3.6.1.4.1.2352.2.39.6.1.1.3 | InetAddress OctetString | SIZE (4) | This object indicates the peer IP address for this UDP L2 VPN circuit. The peer address type is determined by the value of the corresponding rbnUdpL2VpnStaticPeerAddressType.
rbnUdpL2VpnStaticSourceAddressType rbnUdpL2VpnStaticEntry 4 1.3.6.1.4.1.2352.2.39.6.1.1.4 | InetAddressType Integer | 1—ipv4 | This object indicates the source IP address type for this UDP L2 VPN circuit.
rbnUdpL2VpnStaticSourceAddress rbnUdpL2VpnStaticEntry 5 1.3.6.1.4.1.2352.2.39.6.1.1.5 | InetAddress OctetString | SIZE (4) | This object indicates the source IP address for this UDP L2 VPN circuit. The source address type is determined by the value of the corresponding rbnUdpL2VpnStaticSourceAddressType.
rbnUdpL2VpnStaticSourcePort rbnUdpL2VpnStaticEntry 6 1.3.6.1.4.1.2352.2.39.6.1.1.6 | InetPortNumber Unsigned32 | 1024..65535 | This object indicates the source port number for this UDP L2 VPN circuit.
rbnUdpL2vpnStaticAccessCctHandle rbnUdpL2VpnStaticEntry 7 1.3.6.1.4.1.2352.2.39.6.1.1.7 | RbnCircuitHandle OctetString | SIZE (8) | This object indicates the internal representation of the access circuit for this UDP L2 VPN circuit.
rbnUdpL2VpnStaticVpnCctHandle rbnUdpL2VpnStaticEntry 8 1.3.6.1.4.1.2352.2.39.6.1.1.8 | RbnCircuitHandle OctetString | SIZE (8) | This object indicates the internal representation of this UDP L2 VPN circuit.
rbnUdpL2VpnStaticInputCctUp rbnUdpL2VpnStaticEntry 9 1.3.6.1.4.1.2352.2.39.6.1.1.9 | TruthValue Integer | 1—true 2—false | This object indicates the status of this UDP L2 VPN circuit. A value of true indicates that the VPN circuit is connected with its remote site. A value of false indicates that the remote site is not presently connected.
rbnUdpL2VpnStaticIfIndexOrZero rbnUdpL2VpnStaticEntry 10 1.3.6.1.4.1.2352.2.39.6.1.1.10 | InterfaceIndexOrZero Integer32 | 0..2147483647 | This object indicates whether there is a corresponding entry of this UDP L2 VPN access circuit in the ifTable. A non-zero value indicates the ifIndex of the entry in the ifTable. A value of zero indicates that there is no entry (for example, a pre-provisioned access circuit is used).
rbnUdpL2VpnStaticPwFlags rbnUdpL2VpnStaticEntry 11 1.3.6.1.4.1.2352.2.39.6.1.1.11 | RbnVpnPwFlagsType Bits | Integer | Provides more detailed information on the status of the VPN circuit. This object is a bit field so it may contain one or more of these values. See Section 1.43.8 RbnVpnXcFlagsType and RbnVpnPwFlagsType for details.
rbnUdpL2VpnStaticPwState rbnUdpL2VpnStaticEntry 12 1.3.6.1.4.1.2352.2.39.6.1.1.12 | Integer | Diffserver code for the CES over UDP PW. Default is Zero. The dscp code values are listed as follows: 0..63 Differentiated services codepoint value af11 Assured Forwarding - Class 1/Drop precedence 1 af12 Assured Forwarding - Class 1/Drop precedence 2 af13 Assured Forwarding - Class 1/Drop precedence 3 af21 Assured Forwarding - Class 2/Drop precedence 1 af22 Assured Forwarding - Class 2/Drop precedence 2 af23 Assured Forwarding - Class 2/Drop precedence 3 af31 Assured Forwarding - Class 3/Drop precedence 1 af32 Assured Forwarding - Class 3/Drop precedence 2 af33 Assured Forwarding - Class 3/Drop precedence 3 af41 Assured Forwarding - Class 4/Drop precedence 1 af42 Assured Forwarding - Class 4/Drop precedence 2 af43 Assured Forwarding - Class 4/Drop precedence 3
rbnUdpL2vpnStaticDscpCode rbnUdpL2VpnStaticEntry 13 1.3.6.1.4.1.2352.2.39.6.1.1.13 | RbnVpnPwStateType Integer | 0—unknown 1—up 2—down 3—standby | This object indicates the status of this UDP L2 VPN circuit. unknown (0) up (1) indicates that the VPN circuit is active i.e. connected with its remote site. down (2) indicates that the remote site is not presently connected. standby (3) indicates that the PW is in pending state to become active (i.e. up).
rbnUdpL2VpnStaticPsnType rbnUdpL2VpnStaticEntry 14 1.3.6.1.4.1.2352.2.39.6.1.1.14 | RbnVpnPsnType Integer | 0—unknown 1—ip 2—ipsec 3—mpls | This object indicates the packet switched networks (PSN) type for this UDP L2 VPN circuit.

## 1.27 RBN-MEDIA-GATEWAY-MIB

Defines the objects in monitoring media gateways using the rbnH248LinkStatusAlarm notification.

Table 63 describes the media gateway notification objects.

Table 63 Media Gateway Notification Objects
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnMGEventDateAndTime rbnMediaGatewayNotify 1 1.3.6.1.4.1.2352.2.52.1.1.1 | DateAndTime Octet string | SIZE (8) | Local date and time when the event was raised.
rbnMGEventSeverity rbnMediaGatewayNotify 2 1.3.6.1.4.1.2352.2.52.1.1.2 | Integer | 1—cleared 2—indeterminate 3—critical 4—major 5—minor 6—warning | Severity of the event.
rbnMGEventSender rbnMediaGatewayNotify 3 1.3.6.1.4.1.2352.2.52.1.1.3 | Octet string | 1..64 | Identifier of the entity sending the event.
rbnMGEventType rbnMediaGatewayNotify 4 1.3.6.1.4.1.2352.2.52.1.1.4 | IANAItuEventType | Integer | The type of event that triggered an alarm. See Section 1.43.5 IANAItuEventType for details.
rbnMGEventProbableCause rbnMediaGatewayNotify 5 1.3.6.1.4.1.2352.2.52.1.1.5 | rbnMGEventProbableCause | Integer | The probable cause for this alarm. See Section 1.43.4 IANAItuProbableCause for details.
rbnMGEventInformation rbnMediaGatewayNotify 6 1.3.6.1.4.1.2352.2.52.1.1.6 | Octet string | 0..256 | Additional information to describe the problem.

## 1.28 RBN-MEMORY-MIB

Manages system memory usage.

### 1.28.1 rbnMemoryTable

This table contains the objects that identify information about memory usage.

`Index:` rbnMemoryIndex

Table 64 describes the objects in rbnMemoryTable.

Table 64 Objects in rbnMemoryTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnMemoryIndex rbnMemoryEntry 1 1.3.6.1.4.1.2352.2.16.1.2.1.1 | Unsigned32 | 1..4294967295 | A unique identifier for an entry in this table.
rbnMemoryModule rbnMemoryEntry 2 1.3.6.1.4.1.2352.2.16.1.2.1.2 | SnmpAdminString | 0..32 | The name of the module on which this memory resides.
rbnMemoryFreeKBytes rbnMemoryEntry 3 1.3.6.1.4.1.2352.2.16.1.2.1.3 | RbnPercentage Integer32 | 0..100 | The size of unused memory in this entry.
rbnMemoryKBytesInUse rbnMemoryEntry 4 1.3.6.1.4.1.2352.2.16.1.2.1.4 | RbnPercentage Integer32 | 0..100 | The size of memory in use in this entry.
rbnMemoryBlocksInUse rbnMemoryEntry 5 1.3.6.1.4.1.2352.2.16.1.2.1.5 | Unsigned32 | 0..4294967295 | The number of blocks of memory on this module in use. You can use this statistic to check for memory leaks. For example, you can take note of the value, do some operations, undo the operations, then check the value again. The start and end values should match. If they do not, there may be a memory leak.
rbnMemoryCumulBlocks rbnMemoryEntry 6 1.3.6.1.4.1.2352.2.16.1.2.1.6 | Unsigned32 | 0..4294967295 | The cumulative blocks count for this entry. In some systems, this count indicates how many times the system called the memory allocation routine since the system booted. You can use this object to measure the how much memory an operation uses by measuring the number times the system calls the memory allocation routine.

## 1.29 RBN-MPLS-L3VPN-STD-EXT-MIB

This MIB contains managed object definitions for the Layer 3 MPLS VPNs.

### 1.29.1 rbnMplsL3VpnVrfRTTable

This table specifies per-VRF route target association. Each entry identifies a connectivity policy supported as part of a VPN. rbnMplsL3VpnVrfRTTable is equivalent to mplsL3VpnVrfRTTable in MPLS-L3VPN-STD-MIB except for lexicographical ordering. An entry in this table is created by an LSR for each route target configured for a VRF supporting an MPLS L3VPN instance. The indexing provides ordering per VRF instance. See RFC 4364, `BGP/MPLS IP Virtual Private Networks (VPNs)` for a complete definition of a route target.

`Index:` mplsL3VpnVrfName, rbnMplsL3VpnVrfRTAddrFamily, rbnMplsL3VpnVrfRTType, rbnMplsL3VpnVrfRTIndex

Table 65 describes the objects in rbnMplsL3VpnVrfRTTable. All objects in the table are not accessible unless stated otherwise.

Table 65 Objects in rbnMplsL3VpnVrfRTTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnMplsL3VpnVrfRTAddrFamily rbnMplsL3VpnVrfRTEntry 1 1.3.6.1.4.1.2352.2.51.1.1.1.1.1 | AddressFamilyNumbers Integer | 1—ipV4 2—ipV6 | The address family in which the route target is declared.
rbnMplsL3VpnVrfRTType rbnMplsL3VpnVrfRTEntry 2 1.3.6.1.4.1.2352.2.51.1.1.1.1.2 | MplsL3VpnRtType Integer | 1—import 2—export 3—both | Used to define the type of a route target usage (RTU). Route targets can be specified to be imported, exported, or both.
rbnMplsL3VpnVrfRTIndex rbnMplsL3VpnVrfRTEntry 3 1.3.6.1.4.1.2352.2.51.1.1.1.1.3 | Unsigned32 | 1...4294967295 | Auxiliary index for route targets configured for a particular VRF.
rbnMplsL3VpnVrfRT rbnMplsL3VpnVrfRTEntry 4 1.3.6.1.4.1.2352.2.51.1.1.1.1.4 | MplsL3VpnRouteDistinguisher Octet string | 0...256 | The route target distribution policy. This object is read-only.
rbnMplsL3VpnVrfRTDescr rbnMplsL3VpnVrfRTEntry 5 1.3.6.1.4.1.2352.2.51.1.1.1.1.5 | SnmpAdminString Octet string | 0...255 | Description of the route target. This object is read-only.

## 1.30 RBN-NOTIFY-ENHANCE-MIB

Enhances the notification objects on devices.

### 1.30.1 RBN-NOTIFY-ENHANCE-MIB Objects

Table 66 describes the general objects in RBN-NOTIFY-MIB. All objects in the table are accessible-for-notify.

Table 66 Objects in rbnL2tpTunnelCntTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnNESlot rbnNEGeneral 1 1.3.6.1.4.1.2352.2.36.1.1.1 | RbnSlot Unsigned32 | 0..255 | Represents the chassis slot number in which the entity associated with the notification is contained. A value of '0' indicates that the entity is not contained in a chassis slot.
rbnNECardName rbnNEGeneral 2 1.3.6.1.4.1.2352.2.36.1.1.2 | DisplayString | 0..255 | A textual description of the traffic card associated with the notification.
rbnNECardOp rbnNEGeneral 3 1.3.6.1.4.1.2352.2.36.1.1.3 | Integer | 1—insert 2—remove 3—other | Represents the operation performed on the traffic card associated with the notification.
rbnNECircuitId rbnNEGeneral 4 1.3.6.1.4.1.2352.2.36.1.1.4 | DisplayString | 0..255 | Represents a string that identifies the circuit associated with the notification. On the SmartEdge router, this string is formatted as `slot-port-channel-subchannel`, channel and subchannel are only included when appropriate.

## 1.31 RBN-PING-MIB

The RBN-PING-MIB defines additional objects in creating and monitoring ping tests according to the standard PING-MIB.

### 1.31.1 RBN-PING-MIB Global Object

Table 67 describes the global object in the RBN-PING-MIB.

Table 67 Objects in RBN-PING-MIB
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnPingNumTests rbnPingGlobals 1 1.3.6.1.4.1.2352.2.46.1.1.1 | Gauge32 | 0..4294967295 | The number of entries in the pingCtlTable.

### 1.31.2 rbnPingResultsTable

This table enhances the pingResultsTable, providing additional statistics for completing ping tests.

`Index:` pingCtlOwnerIndex, pingCtlTestName

Table 68 describes the objects in rbnPingResultsTable.

Table 68 Objects in rbnPingResultsTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnPingResultsJitter rbnPingResultsEntry 1 1.3.6.1.4.1.2352.2.46.1.2.1.1.1 | Gauge32 | 0..4294967295 | The calculated ping jitter value, which is the delta between the minimum round-trip-time (RTT) and the maximum RTT. If no RTT has been received, this object will have a value of zero (0). Value is identified in milliseconds.

### 1.31.3 rbnPingHistoryTable

This table provides details for storing ping test results. This table is a mirror of the pingResultsTable, with the addition of an index object. The number of entries in this table is limited per entry in the pingCtlTable by the value of the corresponding rbnPingCtlMaxHistoryRows object. An entry in this table is created when a ping test is completed. The initial 2 instance identifier index values identify the pingCtlEntry that these test results belong to. An entry is removed from the table when its corresponding pingCtlEntry is deleted. The oldest entry in this table for a corresponding entry in the pingCtlTable will be removed to allow the addition of a new entry once the number of rows in this table reaches the value specified by the rbnPingCtlMaxHistory for the corresponding entry in the rbnPingCtlTable.

`Index:` pingCtlOwnerIndex, pingCtlTestName, rbnPingHistoryIndex

Table 69 describes the objects in rbnPingHistoryTable. All objects in the table are read-only unless otherwise specified.

Table 69 Objects in rbnPingHistoryTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnPingHistoryIndex rbnPingHistoryEntry 1 1.3.6.1.4.1.2352.2.46.1.2.2.1.1 | Unsigned32 | 1..4294967295 | An entry in this table is created when a ping test completes. The initial two instance identifier index values identify the pingCtlEntry that these results belongs to.
rbnPingHistoryIpTargetAddressType rbnPingHistoryEntry 2 1.3.6.1.4.1.2352.2.46.1.2.2.1.2 | InetAddressType Integer | 0—unknown 1—ipv4 2—ipv6 | This object indicates the type of address stored in the corresponding pingResultsIpTargetAddress object.
rbnPingHistoryIpTargetAddress rbnPingHistoryEntry 3 1.3.6.1.4.1.2352.2.46.1.2.2.1.3 | InetAddress Octet string | 0..255 | The address type (InetAddressType) that relates to this object is specified by the corresponding value of pingResultsIpTargetAddressType.
rbnPingHistoryMinRtt rbnPingHistoryEntry 4 1.3.6.1.4.1.2352.2.46.1.2.2.1.4 | Unsigned32 | 0..4294967295 | The minimum ping round-trip-time (RTT) received. A value of 0 for this object implies that no RTT has been received. The value is identified in milliseconds.
rbnPingHistoryMaxRtt rbnPingHistoryEntry 5 1.3.6.1.4.1.2352.2.46.1.2.2.1.5 | Unsigned32 | 0..4294967295 | The maximum ping round-trip-time (RTT) received. A value of 0 for this object implies that no RTT has been received. The value is identified in milliseconds.
rbnPingHistoryAverageRtt rbnPingHistoryEntry 6 1.3.6.1.4.1.2352.2.46.1.2.2.1.6 | Unsigned32 | 0..4294967295 | The current average ping round-trip-time (RTT) in milliseconds.
rbnPingHistoryProbeResponses rbnPingHistoryEntry 7 1.3.6.1.4.1.2352.2.46.1.2.2.1.7 | Gauge32 | 0..4294967295 | Identifies the number of responses received for the corresponding pingCtlEntry and pingResultsEntry. The value of this object reports as zero (0) when no probe responses have been received. Value is identified in responses received.
rbnPingHistorySentProbes rbnPingHistoryEntry 8 1.3.6.1.4.1.2352.2.46.1.2.2.1.8 | Gauge32 | 0..4294967295 | The value of this object reflects the number of probes sent for the corresponding pingCtlEntry and pingResultsEntry. The value of this object reports as zero (0) when no probes have been sent.
rbnPingHistoryRttSumOfSquares rbnPingHistoryEntry 9 1.3.6.1.4.1.2352.2.46.1.2.2.1.9 | Gauge32 | 0..4294967295 | This object contains the sum of the squares for all ping responses received. Its purpose is to enable standard deviation calculation. The value of this object reports as zero (0) when no ping responses have been received. Value is milliseconds.
rbnPingHistoryLastGoodProbe rbnPingHistoryEntry 10 1.3.6.1.4.1.2352.2.46.1.2.2.1.10 | DateAndTime Octet string | SIZE (8) | Date and time when the last response was received for a probe.
rbnPingHistoryJitter rbnPingHistoryEntry 11 1.3.6.1.4.1.2352.2.46.1.2.2.1.11 | Gauge32 | 0..4294967295 | The calculated ping jitter value, which is the delta between the minimum round-trip-time (RTT) and the maximum RTT. If no RTT has been received, this object will have a value of 0. Value is milliseconds.

### 1.31.4 rbnPingCtlTable

This table enhances the pingCtlTable, providing additional options for all ping tests.

Table 70 describes the object in rbnPingCtlTable.

Table 70 Objects in rbnPingCtlTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnPingCtlMaxHistoryRows rbnPingCtlEntry 1 1.3.6.1.4.1.2352.2.46.1.3.1.1.1 | Unsigned32 | 0..12 | Indicates the maximum number of corresponding entries allowed in the rbnPingHistoryTable. The oldest corresponding entry in the rbnPingHistoryTable will be removed to allow the addition of a new entry once the number of corresponding rows in the rbnPingHistoryTable reaches this value. When a pingCtlTable entry is removed, all corresponding entries in the rbnPingHistoryTable will also be removed. A value of 0 for this object disables creation of rbnPingHistoryTable entries. Default value is 12.

### 1.31.5 rbnPingCtlIpTable

This table enhances the pingCtlTable, providing additional options for IPv4 ping tests.

These objects are ignored in conceptual rows where the pingCtlType instance does not equal pingIcmpEcho.

Table 71 describes the objects in rbnPingCtlIpTable.

Table 71 Objects in rbnPingCtlIpTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnPingCtlIpDontFragment rbnPingCtlIpEntry 1 1.3.6.1.4.1.2352.2.46.1.4.1.1.1 | TruthValue Integer | 1—true 2—false | Indicates whether the dont-fragment (DF) flag should be set in the probe packet IP header.
rbnPingCtlIpTtl rbnPingCtlIpEntry 2 1.3.6.1.4.1.2352.2.46.1.4.1.1.2 | Unsigned32 | 1..255 | Specifies a time-to-live (TTL) value to use in the probe packet IP header. Default value is 255.

## 1.32 RBN-PRODUCT-MIB

Contains the administrative assignments which are used to uniquely identify physical components.

### 1.32.1 RBN-PRODUCT-MIB Objects

Note:
  There are no types or values associated with these objects because they are nonLeaf objects.

Table 72 Product Assignments
Object and Object Identifier | Description
--- | ---
rbnSMS1000 rbnProducts 1 1.3.6.1.4.1.2352.1.1 | The definitive identifier for the SMS1000.
rbnSMS500 rbnProducts 2 1.3.6.1.4.1.2352.1.2 | The definitive identifier for the SMS500.
rbnSMS1800 rbnProducts 3 1.3.6.1.4.1.2352.1.3 | The definitive identifier for the SMS1800.
rbnSMS10000 rbnProducts 4 1.3.6.1.4.1.2352.1.4 | The definitive identifier for the SMS10000.
rbnSmartEdgeIDT rbnProducts 5 1.3.6.1.4.1.2352.1.5 | The definitive identifier for the SmartEdge (SE) IDT.
rbnEsp200 rbnProducts 6 1.3.6.1.4.1.2352.1.6 | The definitive identifier for the ESP200.
rbnEsp5000 rbnProducts 7 1.3.6.1.4.1.2352.1.7 | The definitive identifier for the ESP5000.
rbnEsp6000 rbnProducts 8 1.3.6.1.4.1.2352.1.8 | The definitive identifier for the ESP6000.
rbnSMS2800 rbnProducts 9 1.3.6.1.4.1.2352.1.9 | The definitive identifier for the SMS2800.
rbnSmartEdge800 rbnProducts 10 1.3.6.1.4.1.2352.1.10 | The definitive identifier for the SE800.
rbnSmartEdge400 rbnProducts 11 1.3.6.1.4.1.2352.1.11 | The definitive identifier for the SE400.
rbnSmartEdge100 rbnProducts 12 1.3.6.1.4.1.2352.1.12 | The definitive identifier for the SE100.
rbnSmartEdge1200 rbnProducts 13 1.3.6.1.4.1.2352.1.13 | The definitive identifier for the SE200.
rbnSM480 rbnProducts 14 1.3.6.1.4.1.2352.1.14 | The definitive identifier for the Smart Metro (SM) 480.
rbnSmartEdge600 rbnProducts 15 1.3.6.1.4.1.2352.1.15 | The definitive identifier for the SE600.
rbnSM240 rbnProducts 16 1.3.6.1.4.1.2352.1.16 | The definitive identifier for the SM240.

Table 73 Other Objects
Object and Object Identifier | Description
--- | ---
rbnEntityTypeOther rbnEntities 1 1.3.6.1.4.1.2352.6.1 | The top-level category identifier for entities that reside in the value of the PhysicalClass ENTITY-MIB object as other.

Table 74 Unknown Objects
Object and Object Identifier | Description
--- | ---
rbnEntityTypeUnknown rbnEntities 2 1.3.6.1.4.1.2352.6.2 | The top-level category identifier for entities that reside in the value of the PhysicalClass ENTITY-MIB object as unknown.

Table 75 Chassis Objects
Object and Object Identifier | Description
--- | ---
rbnEntityTypeChassis rbnEntities 3 1.3.6.1.4.1.2352.6.3 | The top-level category identifier for entities that reside in the value of the PhysicalClass ENTITY-MIB object as chassis.
rbnEntChassisSMS1000 rbnEntityTypeChassis 1 1.3.6.1.4.1.2352.6.3.1 | The definitive identifier for the SMS1000 chassis entity.
rbnEntChassisSMS500 rbnEntityTypeChassis 2 1.3.6.1.4.1.2352.6.3.2 | The definitive identifier for the SMS500 chassis entity.
rbnEntChassisSMS1800 rbnEntityTypeChassis 3 1.3.6.1.4.1.2352.6.3.3 | The definitive identifier for the SMS1800 chassis entity.
rbnEntChassisSMS10000 rbnEntityTypeChassis 4 1.3.6.1.4.1.2352.6.3.4 | The definitive identifier for the SMS10000 chassis entity.
rbnEntChassisSMS2800 rbnEntityTypeChassis 5 1.3.6.1.4.1.2352.6.3.5 | The definitive identifier for the SMS2800 chassis entity.
rbnEntChassisSE800 rbnEntityTypeChassis 6 1.3.6.1.4.1.2352.6.3.6 | The definitive identifier for the SE800 chassis entity.
rbnEntChassisSE400 rbnEntityTypeChassis 7 1.3.6.1.4.1.2352.6.3.7 | The definitive identifier for the SE400 chassis entity.
rbnEntChassisSE100 rbnEntityTypeChassis 8 1.3.6.1.4.1.2352.6.3.8 | The definitive identifier for the SE100 chassis entity.
rbnEntChassisSE1200 rbnEntityTypeChassis 9 1.3.6.1.4.1.2352.6.3.9 | The definitive identifier for the SE1200 chassis entity.
rbnEntChassisSM480 rbnEntityTypeChassis 10 1.3.6.1.4.1.2352.6.3.10 | The definitive identifier for the SMS10000 IO container (slot) entity.
rbnEntChassisSE600 rbnEntityTypeChassis 11 1.3.6.1.4.1.2352.6.3.11 | The definitive identifier for the SE600 chassis entity.
rbnEntChassisSM240 rbnEntityTypeChassis 12 1.3.6.1.4.1.2352.6.3.12 | The definitive identifier for the SM240 chassis entity.
rbnEntChassisSE1200H rbnEntityTypeChassis 13 1.3.6.1.4.1.2352.6.3.13 | The definitive identifier for the SE1200H chassis entity.

Table 76 Backplane Objects
Object and Object Identifier | Description
--- | ---
rbnEntityTypeBackplane rbnEntities 4 1.3.6.1.4.1.2352.6.4 | The top-level category identifier for entities that reside in the value of the PhysicalClass ENTITY-MIB object as backplane.
rbnEntBackplaneSMS1000Data rbnEntityTypeBackplane 1 1.3.6.1.4.1.2352.6.4.1 | The definitive identifier for the SMS1000 data backplane entity.
rbnEntBackplaneSMS1000Power rbnEntityTypeBackplane 2 1.3.6.1.4.1.2352.6.4.2 | The definitive identifier for the SMS1000 power backplane entity.
rbnEntBackplaneSMS500Data rbnEntityTypeBackplane 3 1.3.6.1.4.1.2352.6.4.3 | The definitive identifier for the SMS500 data backplane entity.
rbnEntBackplaneSMS500Power rbnEntityTypeBackplane 4 1.3.6.1.4.1.2352.6.4.4 | The definitive identifier for the SMS500 power backplane entity.
rbnEntBackplaneSMS1800Data rbnEntityTypeBackplane 5 1.3.6.1.4.1.2352.6.4.5 | The definitive identifier for the SMS1800 data backplane entity.
rbnEntBackplaneSMS1800Power rbnEntityTypeBackplane 6 1.3.6.1.4.1.2352.6.4.6 | The definitive identifier for the SMS1800 power backplane entity.
rbnEntBackplaneSMS10000Midplane rbnEntityTypeBackplane 7 1.3.6.1.4.1.2352.6.4.7 | The definitive identifier for the SMS10000 mid-plane entity.
rbnEntBackplaneSMS2800Data rbnEntityTypeBackplane 8 1.3.6.1.4.1.2352.6.4.8 | The definitive identifier for the SMS2800 data backplane entity.
rbnEntBackplaneSMS2800Power rbnEntityTypeBackplane 9 1.3.6.1.4.1.2352.6.4.9 | The definitive identifier for the SMS2800 power backplane entity.
rbnEntBackplaneSE800Data rbnEntityTypeBackplane 10 1.3.6.1.4.1.2352.6.4.10 | The definitive identifier for the SE800 data backplane entity.
rbnEntBackplaneSE400Data rbnEntityTypeBackplane 11 1.3.6.1.4.1.2352.6.4.11 | The definitive identifier for the SE400 data backplane entity.
rbnEntBackplaneSE100Data rbnEntityTypeBackplane 12 1.3.6.1.4.1.2352.6.4.12 | The definitive identifier for the SE100 data backplane entity.
rbnEntBackplaneSE1200Data rbnEntityTypeBackplane 13 1.3.6.1.4.1.2352.6.4.13 | The definitive identifier for the SE1200 data backplane entity.
rbnEntBackplaneSM480Data rbnEntityTypeBackplane 14 1.3.6.1.4.1.2352.6.4.14 | The definitive identifier for the SM480 data backplane entity.
rbnEntBackplaneSE600Data rbnEntityTypeBackplane 15 1.3.6.1.4.1.2352.6.4.15 | The definitive identifier for the SE600 data backplane entity.
rbnEntBackplaneSM240Data rbnEntityTypeBackplane 16 1.3.6.1.4.1.2352.6.4.16 | The definitive identifier for the SM240 data backplane entity.
rbnEntBackplaneSE1200HData rbnEntityTypeBackplane 17 1.3.6.1.4.1.2352.6.4.17 | The definitive identifier for the SE1200H data backplane entity.

Table 77 Data Container (slot) Entity Objects
Object and Object Identifier | Description
--- | ---
rbnEntityTypeContainer rbnEntities 5 1.3.6.1.4.1.2352.6.5 | The top-level category identifier for entities that reside in the value of the PhysicalClass ENTITY-MIB object as container.
rbnEntContainerSMS1000Data rbnEntityTypeContainer 1 1.3.6.1.4.1.2352.6.5.1 | The definitive identifier for the SMS1000 data container (slot) entity.
rbnEntContainerSMS1000Power rbnEntityTypeContainer 2 1.3.6.1.4.1.2352.6.5.2 | The definitive identifier for the SMS1000 power container (slot) entity.
rbnEntContainerSMS500Data rbnEntityTypeContainer 3 1.3.6.1.4.1.2352.6.5.3 | The definitive identifier for the SMS500 data container (slot) entity.
rbnEntContainerSMS500Power rbnEntityTypeContainer 4 1.3.6.1.4.1.2352.6.5.4 | The definitive identifier for the SMS500 power container (slot) entity.
rbnEntContainerSMS1800Data rbnEntityTypeContainer 5 1.3.6.1.4.1.2352.6.5.5 | The definitive identifier for the SMS1800 data container (slot) entity.
rbnEntContainerSMS1800Power rbnEntityTypeContainer 6 1.3.6.1.4.1.2352.6.5.6 | The definitive identifier for the SMS1800 power container (slot) entity.
rbnEntContainerSMS10000Fabric rbnEntityTypeContainer 7 1.3.6.1.4.1.2352.6.5.7 | The definitive identifier for the SMS10000 fabric container (slot) entity.
rbnEntContainerSMS10000Timing rbnEntityTypeContainer 8 1.3.6.1.4.1.2352.6.5.8 | The definitive identifier for the SMS10000 timing container (slot) entity.
rbnEntContainerSMS10000SMCM rbnEntityTypeContainer 9 1.3.6.1.4.1.2352.6.5.9 | The definitive identifier for the SMS10000 SM/CM container (slot) entity.
rbnEntContainerSMS10000IO rbnEntityTypeContainer 10 1.3.6.1.4.1.2352.6.5.10 | The definitive identifier for the SMS10000 IO container (slot) entity
rbnEntContainerSMS2800Power rbnEntityTypeContainer 11 1.3.6.1.4.1.2352.6.5.11 | The definitive identifier for the SMS2800 Power container (slot) entity.
rbnEntContainerSMS2800CSM rbnEntityTypeContainer 12 1.3.6.1.4.1.2352.6.5.12 | The definitive identifier for the SMS2800 CSM container (slot) entity.
rbnEntContainerSMS2800IO rbnEntityTypeContainer 13 1.3.6.1.4.1.2352.6.5.13 | The definitive identifier for the SMS2800 IO container (slot) entity.
rbnEntContainerSE800Data rbnEntityTypeContainer 14 1.3.6.1.4.1.2352.6.5.14 | The definitive identifier for the SE800 data container (slot) entity.
rbnEntContainerSE400Data rbnEntityTypeContainer 15 1.3.6.1.4.1.2352.6.5.15 | The definitive identifier for the SE400 data container (slot) entity.
rbnEntContainerSE100Data rbnEntityTypeContainer 16 1.3.6.1.4.1.2352.6.5.16 | The definitive identifier for the SE100 data container (slot) entity.
rbnEntContainerSE100Carrier rbnEntityTypeContainer 17 1.3.6.1.4.1.2352.6.5.17 | The definitive identifier for the SE100 carrier container (MIC-card holder) entity.
rbnEntContainerSE1200Data rbnEntityTypeContainer 18 1.3.6.1.4.1.2352.6.5.18 | The definitive identifier for the SE1200 data container (slot) entity.
rbnEntContainerSM480Data rbnEntityTypeContainer 19 1.3.6.1.4.1.2352.6.5.19 | The definitive identifier for the SM480 data container (slot) entity.
rbnEntContainerSE600Data rbnEntityTypeContainer 20 1.3.6.1.4.1.2352.6.5.20 | The definitive identifier for the SE600 data container (slot) entity.
rbnEntContainerSM240Data rbnEntityTypeContainer 21 1.3.6.1.4.1.2352.6.5.21 | The definitive identifier for the SM240 data container (slot) entity.
rbnEntContainerSE1200HData rbnEntityTypeContainer 22 1.3.6.1.4.1.2352.6.5.22 | The definitive identifier for the SE1200H data container (slot) entity.

Table 78 Power Supply Entity Objects
Object and Object Identifier | Description
--- | ---
rbnEntityTypePowerSupply rbnEntities 6 1.3.6.1.4.1.2352.6.6 | The top-level category identifier for entities that reside in the value of the PhysicalClass ENTITY-MIB object as powerSupply.
rbnEntPowerSupplyUnknown rbnEntityTypePowerSupply 1 1.3.6.1.4.1.2352.6.6.1 | The identifier used to represent any power supply that cannot be definitively identified, often because its configuration EEPROM is not valid.
rbnEntPowerSupplySMS1000AC rbnEntityTypePowerSupply 2 1.3.6.1.4.1.2352.6.6.2 | The definitive identifier for the SMS1000 AC power supply, model PS-1K-AC.
rbnEntPowerSupplySMS1000DC rbnEntityTypePowerSupply 3 1.3.6.1.4.1.2352.6.6.3 | The definitive identifier for the SMS1000 DC power supply, model PS-1K-DC.
rbnEntPowerSupplySMS500AC rbnEntityTypePowerSupply 4 1.3.6.1.4.1.2352.6.6.4 | The definitive identifier for the SMS500 AC power supply
rbnEntPowerSupplySMS500DC rbnEntityTypePowerSupply 5 1.3.6.1.4.1.2352.6.6.5 | The definitive identifier for the SMS500 DC power supply.
rbnEntPowerSupplySMS1800AC rbnEntityTypePowerSupply 6 1.3.6.1.4.1.2352.6.6.6 | The definitive identifier for the SMS1800 AC power supply.
rbnEntPowerSupplySMS1800DC rbnEntityTypePowerSupply 7 1.3.6.1.4.1.2352.6.6.7 | The definitive identifier for the SMS1800 DC power supply.
rbnEntPowerSupplySMS2800AC rbnEntityTypePowerSupply 8 1.3.6.1.4.1.2352.6.6.8 | The definitive identifier for the SMS2800 AC power supply.
rbnEntPowerSupplySMS2800DC rbnEntityTypePowerSupply 9 1.3.6.1.4.1.2352.6.6.9 | The definitive identifier for the SMS2800 DC power supply.

Table 79 Fan Entity Objects
Object and Object Identifier | Description
--- | ---
rbnEntityTypeFan rbnEntities 7 1.3.6.1.4.1.2352.6.7 | The top-level category identifier for entities that reside in the value of the PhysicalClass ENTITY-MIB object as fan.
rbnEntFanSE800 rbnEntityTypeFan 1 1.3.6.1.4.1.2352.6.7.1 | The definitive identifier for the SE800 fan tray.
rbnEntFanSE400 rbnEntityTypeFan 2 1.3.6.1.4.1.2352.6.7.2 | The definitive identifier for the SE400 fan tray.
rbnEntFanSE1200 rbnEntityTypeFan 3 1.3.6.1.4.1.2352.6.7.3 | The definitive identifier for the SE 1200 fan tray.
rbnEntFanSM480 rbnEntityTypeFan 4 1.3.6.1.4.1.2352.6.7.4 | The definitive identifier for the SM480 fan tray.
rbnEntFanSE600 rbnEntityTypeFan 5 1.3.6.1.4.1.2352.6.7.5 | The definitive identifier for the SE600 fan tray.
rbnEntFanSM240 rbnEntityTypeFan 6 1.3.6.1.4.1.2352.6.7.6 | The definitive identifier for the SM240 fan tray.
rbnEntFanSE1200H rbnEntityTypeFan 7 1.3.6.1.4.1.2352.6.7.7 | The definitive identifier for the SE1200H Fan Tray.

Table 80 Product Alarm Identifier Entity Objects
Object and Object Identifier | Description
--- | ---
rbnEntityTypeSensor rbnEntities 8 1.3.6.1.4.1.2352.6.8 | The top-level category identifier for entities which reside in the value of the PhysicalClass ENTITY-MIB object as sensor.
rbnEntSensorAlarmSE400 rbnEntityTypeSensor 1 1.3.6.1.4.1.2352.6.8.1 | The definitive identifier for the SE400 alarm card.
rbnEntSensorAlarmSE600 rbnEntityTypeSensor 2 1.3.6.1.4.1.2352.6.8.2 | The definitive identifier for the SE600 alarm card.
rbnEntSensorAlarmSM240 rbnEntityTypeSensor 3 1.3.6.1.4.1.2352.6.8.3 | The definitive identifier for the SM240 alarm card.

Table 81 Module Entity Objects
Object and Object Identifier | Description
--- | ---
rbnEntityTypeModule rbnEntities 9 1.3.6.1.4.1.2352.6.9 | The top-level category identifier for entities that reside in the value of the PhysicalClass ENTITY-MIB object as module.
rbnEntModuleUnknown rbnEntityTypeModule 1 1.3.6.1.4.1.2352.6.9.1 | The identifier used to represent any module that cannot be definitively identified, often because configuration EEPROM is not valid.
rbnEntModuleSMSAIMOC3 rbnEntityTypeModule 3 1.3.6.1.4.1.2352.6.9.3 | The definitive identifier for the SMS ATM OC-3 interface module.
rbnEntModuleSMSAIMDS3 rbnEntityTypeModule 4 1.3.6.1.4.1.2352.6.9.4 | The definitive identifier for the SMS ATM DS-3 interface module.
rbnEntModuleSMSAIME3 rbnEntityTypeModule 5 1.3.6.1.4.1.2352.6.9.5 | The definitive identifier for the SMS ATM E3 interface module.
rbnEntModuleSMSEIM rbnEntityTypeModule 6 1.3.6.1.4.1.2352.6.9.6 | The definitive identifier for the SMS 10/100BaseT Ethernet interface module.
rbnEntModuleSMSPIMDS3 rbnEntityTypeModule 7 1.3.6.1.4.1.2352.6.9.7 | The definitive identifier for the SMS Packet DS-3 interface module.
rbnEntModuleSMSPIME3 rbnEntityTypeModule 8 1.3.6.1.4.1.2352.6.9.8 | The definitive identifier for the SMS Packet E3 interface module.
rbnEntModuleSMSPIMHSSI rbnEntityTypeModule 9 1.3.6.1.4.1.2352.6.9.9 | The definitive identifier for the SMS Packet HSSI interface module.
rbnEntModuleSMSFE1 rbnEntityTypeModule 10 1.3.6.1.4.1.2352.6.9.10 | The definitive identifier for the SMS forwarding engine (FE) 1.
rbnEntModuleSMSFE2 rbnEntityTypeModule 12 1.3.6.1.4.1.2352.6.9.12 | The definitive identifier for the SMS FE 2.
rbnEntModuleSMSPIMDS1 rbnEntityTypeModule 14 1.3.6.1.4.1.2352.6.9.14 | The definitive identifier for the SMS Packet DS-1 interface module.
rbnEntModuleSMSPIMCDS3 rbnEntityTypeModule 15 1.3.6.1.4.1.2352.6.9.15 | The definitive identifier for the SMS Channelized DS-3 interface module.
rbnEntModuleSMSCE1 rbnEntityTypeModule 16 1.3.6.1.4.1.2352.6.9.16 | The definitive identifier for the SMS control engine (CE) 1.
rbnEntModuleSMSCE2 rbnEntityTypeModule 17 1.3.6.1.4.1.2352.6.9.17 | The definitive identifier for the SMS CE 2.
rbnEntModuleSMSCE3 rbnEntityTypeModule 18 1.3.6.1.4.1.2352.6.9.18 | The definitive identifier for the SMS CE 3.
rbnEntModuleSMSAIMT1 rbnEntityTypeModule 20 1.3.6.1.4.1.2352.6.9.20 | The definitive identifier for the SMS ATM T1 interface module.
rbnEntModuleSMSPIME1 rbnEntityTypeModule 22 1.3.6.1.4.1.2352.6.9.22 | The definitive identifier for the SMS Packet E1 interface module.
rbnEntModuleSMSAIME1 rbnEntityTypeModule 23 1.3.6.1.4.1.2352.6.9.23 | The definitive identifier for the SMS ATM E1 interface module.
rbnEntModuleSMSPOSOC3 rbnEntityTypeModule 24 1.3.6.1.4.1.2352.6.9.24 | The definitive identifier for the SMS POS OC-3 interface module.
rbnEntModuleSMSPOSOC12 rbnEntityTypeModule 25 1.3.6.1.4.1.2352.6.9.25 | The definitive identifier for the SMS POS OC-12 interface module.
rbnEntModuleSMSGIGEIM rbnEntityTypeModule 26 1.3.6.1.4.1.2352.6.9.26 | The definitive identifier for the SMS Gigabit Ethernet interface module.
rbnEntModuleSMSAIMOC12 rbnEntityTypeModule 27 1.3.6.1.4.1.2352.6.9.27 | The definitive identifier for the SMS ATM OC-12 interface module.
rbnEntModuleSMSIPSEC rbnEntityTypeModule 28 1.3.6.1.4.1.2352.6.9.28 | The definitive identifier for the SMS IPsec interface module.
rbnEntModuleSMSFABRIC rbnEntityTypeModule 29 1.3.6.1.4.1.2352.6.9.29 | The definitive identifier for the SMS switch fabric module.
rbnEntModuleSMSCM rbnEntityTypeModule 30 1.3.6.1.4.1.2352.6.9.30 | The definitive identifier for the SMS connection manager module.
rbnEntModuleSMSTIMING rbnEntityTypeModule 31 1.3.6.1.4.1.2352.6.9.31 | The definitive identifier for the SMS timing module.
rbnEntModuleSMSSM rbnEntityTypeModule 32 1.3.6.1.4.1.2352.6.9.32 | The definitive identifier for the SMS system manager module.
rbnEntModuleSMSFE3 rbnEntityTypeModule 35 1.3.6.1.4.1.2352.6.9.35 | The definitive identifier for the SMS FE 3.
rbnEntModuleSMSCSM rbnEntityTypeModule 36 1.3.6.1.4.1.2352.6.9.36 | The definitive identifier for the connection system manager (CSM) module.
rbnEntModuleSMSXFE rbnEntityTypeModule 40 1.3.6.1.4.1.2352.6.9.40 | The definitive identifier for the SMS extended FE.
rbnEntModuleSEXC rbnEntityTypeModule 41 1.3.6.1.4.1.2352.6.9.41 | The definitive identifier for the SE cross-connect module.
rbnEntModuleSEEIM rbnEntityTypeModule 42 1.3.6.1.4.1.2352.6.9.42 | The definitive identifier for the SE 10/100BaseT Ethernet interface module.
rbnEntModuleSEGIGEIM rbnEntityTypeModule 43 1.3.6.1.4.1.2352.6.9.43 | The definitive identifier for the SE Gigabit Ethernet interface module.
rbnEntModuleSEPOSOC12 rbnEntityTypeModule 44 1.3.6.1.4.1.2352.6.9.44 | The definitive identifier for the SE POS OC-12 interface module.
rbnEntModuleSEPOSOC48 rbnEntityTypeModule 45 1.3.6.1.4.1.2352.6.9.45 | The definitive identifier for the SE POS OC-48 interface module.
rbnEntModuleSEPOSOC3 rbnEntityTypeModule 46 1.3.6.1.4.1.2352.6.9.46 | The definitive identifier for the SE POS OC3 interface module.
rbnEntModuleSECHOC12DS1 rbnEntityTypeModule 47 1.3.6.1.4.1.2352.6.9.47 | The definitive identifier for the SE Channelized OC12 DS1 interface module.
rbnEntModuleSECHOC12DS3 rbnEntityTypeModule 48 1.3.6.1.4.1.2352.6.9.48 | The definitive identifier for the SE Channelized OC12 DS3 interface module.
rbnEntModuleSEAIMOC3 rbnEntityTypeModule 49 1.3.6.1.4.1.2352.6.9.49 | The definitive identifier for the SE ATM OC3 interface module.
rbnEntModuleSEAIMOC12 rbnEntityTypeModule 50 1.3.6.1.4.1.2352.6.9.50 | The definitive identifier for the SE ATM OC12 interface module.
rbnEntModuleSECHDS3 rbnEntityTypeModule 51 1.3.6.1.4.1.2352.6.9.51 | The definitive identifier for the SE Channelized DS3 interface module.
rbnEntModuleSEDS3 rbnEntityTypeModule 52 1.3.6.1.4.1.2352.6.9.52 | The definitive identifier for the SE DS3 interface module.
rbnEntModuleSEAIMDS3 rbnEntityTypeModule 53 1.3.6.1.4.1.2352.6.9.53 | The definitive identifier for the SE ATM DS3 interface module.
rbnEntModuleSECHSTM1E1 rbnEntityTypeModule 54 1.3.6.1.4.1.2352.6.9.54 | The definitive identifier for the SE Channelized STM-1 to E1 interface module.
rbnEntModuleSEE1 rbnEntityTypeModule 55 1.3.6.1.4.1.2352.6.9.55 | The definitive identifier for the SE E1 interface module.
rbnEntModuleSEXC3 rbnEntityTypeModule 56 1.3.6.1.4.1.2352.6.9.56 | The definitive identifier for the SmartEdge cross-connect module version 3.
rbnEntModuleSEAIMOC12E rbnEntityTypeModule 58 1.3.6.1.4.1.2352.6.9.58 | The definitive identifier for the ATM OC-12 enhanced interface module.
rbnEntModuleSEGIGETM rbnEntityTypeModule 59 1.3.6.1.4.1.2352.6.9.59 | The definitive identifier for the SE Gigabit Ethernet with traffic management module.
rbnEntModuleSE10GIGEIM rbnEntityTypeModule 60 1.3.6.1.4.1.2352.6.9.60 | The definitive identifier for the SE 10 Gigabit Ethernet interface module.
rbnEntModuleSE100XC rbnEntityTypeModule 61 1.3.6.1.4.1.2352.6.9.61 | The definitive identifier for the SE100 cross-connect module.
rbnEntModuleSE100EMIC rbnEntityTypeModule 62 1.3.6.1.4.1.2352.6.9.62 | The definitive identifier for the SE100 10/100BaseT Ethernet media interface connect module.
rbnEntModuleSE100FXMIC rbnEntityTypeModule 63 1.3.6.1.4.1.2352.6.9.63 | The definitive identifier for the SE100 FX-100 Ethernet media interface connect module.
rbnEntModuleSE100GERJMIC rbnEntityTypeModule 64 1.3.6.1.4.1.2352.6.9.64 | The definitive identifier for the SE100 Gigabit Ethernet media interface connect module.
rbnEntModuleSE100GEFXMIC rbnEntityTypeModule 65 1.3.6.1.4.1.2352.6.9.65 | The definitive identifier for the SE100 FX-1000 Ethernet media interface connect module.
rbnEntModuleSEXC4 rbnEntityTypeModule 66 1.3.6.1.4.1.2352.6.9.66 | The definitive identifier for the SE cross-connect module version 4.
rbnEntModuleSE100AIMOC3MIC rbnEntityTypeModule 67 1.3.6.1.4.1.2352.6.9.67 | The definitive identifier for the SE100 2-port ATM OC-3 media interfaceconnect module.
rbnEntModuleSEASE rbnEntityTypeModule 68 1.3.6.1.4.1.2352.6.9.68 | The definitive identifier for the SE Advanced Services Engine (ASE) module.
rbnEntModuleSEFE60GE2 rbnEntityTypeModule 69 1.3.6.1.4.1.2352.6.9.69 | The definitive identifier for the SE FE60GE2 Ethernet interface module.
rbnEntModuleSEPOSOC192 rbnEntityTypeModule 70 1.3.6.1.4.1.2352.6.9.70 | The definitive identifier for the SE POS OC-192 interface module.
rbnEntModuleSE5PortGIGE rbnEntityTypeModule 71 1.3.6.1.4.1.2352.6.9.71 | The definitive identifier for the SE 5-port PPA2 based Gigabit Ethernet interface module.
rbnEntModuleSE20PortGIGE rbnEntityTypeModule 72 1.3.6.1.4.1.2352.6.9.72 | The definitive identifier for the 20-port PPA3- or PMA3-based Gigabit Ethernet interface module.
rbnEntModuleSE4Port10GIGE rbnEntityTypeModule 73 1.3.6.1.4.1.2352.6.9.73 | The definitive identifier for the 4-port PPA3- or PMA3-based 10 Gigabit Ethernet interface module.
rbnEntModuleSE10GIGETM rbnEntityTypeModule 74 1.3.6.1.4.1.2352.6.9.74 | The definitive identifier for the 10 Gigabit Ethernet Traffic Management interface module.
rbnEntModuleSESSE rbnEntityTypeModule 75 1.3.6.1.4.1.2352.6.9.75 | The definitive identifier for the SmartEdge Server Engine (SSE).
rbnEntModuleSE10PortGIGEDDR2 rbnEntityTypeModule 76 1.3.6.1.4.1.2352.6.9.76 | The definitive identifier for the SE 10 Gigabit Ethernet with DDR Upgrade.
rbnEntModuleSE4PortOC48 rbnEntityTypeModule 77 1.3.6.1.4.1.2352.6.9.77 | The definitive identifier for the SE 4-port OC-48 POS interface module.
rbnEntModuleSE8PortOC3 rbnEntityTypeModule 78 1.3.6.1.4.1.2352.6.9.78 | The definitive identifier for the SE 8-port OC-3 ATM interface module.
rbnEntModuleSE8OR2PORTCHOC3OC12 rbnEntityTypeModule 79 1.3.6.1.4.1.2352.6.9.79 | The definitive identifier for the SE Channelized OC3/STM1 or OC12/STM4 8 or 2 Port Interface Module.
rbnEntModuleSE1Port10GEOC192 rbnEntityTypeModule 81 1.3.6.1.4.1.2352.6.9.81 | The definitive identifier for the SE version of a line card supporting either 10GE (Gigabit Ethernet) or OC192 but not both.
rbnEntModuleSEPos8xOC3 rbnEntityTypeModule 82 1.3.6.1.4.1.2352.6.9.82 | The definitive identifier for the SE 8-port OC-3 POS PPA2 interface module.
rbnEntModuleSEPos4xOC12 rbnEntityTypeModule 83 1.3.6.1.4.1.2352.6.9.83 | The definitive identifier for the SE 4 port OC-12 POS PPA2 interface module.
rbnEntModuleSEAtm2xOC12 rbnEntityTypeModule 84 1.3.6.1.4.1.2352.6.9.84 | The definitive identifier for the SE 2 port OC-12 ATM PPA2 interface module.
rbnEntModuleSM8OR2PORTCHOC3OC12 rbnEntityTypeModule 112 1.3.6.1.4.1.2352.6.9.112 | The definitive identifier for the Channelized OC3/STM1 or OC12/STM4 8 or 2 Port interface module.

Table 82 Port Entity Objects
Object and Object Identifier | Description
--- | ---
rbnEntityTypePort rbnEntities 10 1.3.6.1.4.1.2352.6.10 | The top-level category identifier for entities that reside in PhysicalClass ENTITY-MIB object as port.
rbnEntPortUnknown rbnEntityTypePort 1 1.3.6.1.4.1.2352.6.10.1 | The identifier used to represent any module that cannot be definitively identified, often because configuration EEPROM is not valid.
rbnEntPortSMSAIMOC3 rbnEntityTypePort 3 1.3.6.1.4.1.2352.6.10.3 | The definitive identifier for the SMS ATM OC-3 interface port.
rbnEntPortSMSAIMDS3 rbnEntityTypePort 4 1.3.6.1.4.1.2352.6.10.4 | The definitive identifier for the SMS ATM DS-3 interface port.
rbnEntPortSMSAIME3 rbnEntityTypePort 5 1.3.6.1.4.1.2352.6.10.5 | The definitive identifier for the SMS ATM E3 interface port.
rbnEntPortSMSEIM rbnEntityTypePort 6 1.3.6.1.4.1.2352.6.10.6 | The definitive identifier for the SMS 10/100BaseT Ethernet interface port.
rbnEntPortSMSPIMDS3 rbnEntityTypePort 7 1.3.6.1.4.1.2352.6.10.7 | The definitive identifier for the SMS Packet DS-3 interface port.
rbnEntPortSMSPIME3 rbnEntityTypePort 8 1.3.6.1.4.1.2352.6.10.8 | The definitive identifier for the SMS Packet E3 interface port.
rbnEntPortSMSPIMHSSI rbnEntityTypePort 9 1.3.6.1.4.1.2352.6.10.9 | The definitive identifier for the SMS Packet HSSI interface port.
rbnEntPortSMSPIMDS1 rbnEntityTypePort 14 1.3.6.1.4.1.2352.6.10.14 | The definitive identifier for the SMS Packet DS-1 interface port.
rbnEntPortSMSPIMCDS3 rbnEntityTypePort 15 1.3.6.1.4.1.2352.6.10.15 | The definitive identifier for the SMS Channelized DS-3 interface port.
rbnEntPortSMSCE1MGMT rbnEntityTypePort 16 1.3.6.1.4.1.2352.6.10.16 | The definitive identifier for the SMS Control Engine 1, local management port.
rbnEntPortSMSCE2MGMT rbnEntityTypePort 17 1.3.6.1.4.1.2352.6.10.17 | The definitive identifier for the SMS Control Engine 2, local management port.
rbnEntPortSMSCE3MGMT rbnEntityTypePort 18 1.3.6.1.4.1.2352.6.10.18 | The definitive identifier for the SMS Control Engine 3, local management port.
rbnEntPortSMSAIMT1 rbnEntityTypePort 20 1.3.6.1.4.1.2352.6.10.20 | The definitive identifier for the SMS ATM T1 interface port.
rbnEntPortSMSPIME1 rbnEntityTypePort 22 1.3.6.1.4.1.2352.6.10.22 | The definitive identifier for the SMS Packet E1 interface port.
rbnEntPortSMSAIME1 rbnEntityTypePort 23 1.3.6.1.4.1.2352.6.10.23 | The definitive identifier for the SMS ATM E1 interface port.
rbnEntPortSMSPOSOC3 rbnEntityTypePort 24 1.3.6.1.4.1.2352.6.10.24 | The definitive identifier for the SMS POS OC-3 interface port.
rbnEntPortSMSPOSOC12 rbnEntityTypePort 25 1.3.6.1.4.1.2352.6.10.25 | The definitive identifier for the SMS POS OC-12 interface port.
rbnEntPortSMSGIGEIM rbnEntityTypePort 26 1.3.6.1.4.1.2352.6.10.26 | The definitive identifier for the SMS Gigabit Ethernet interface port.
rbnEntPortSMSAIMOC12 rbnEntityTypePort 27 1.3.6.1.4.1.2352.6.10.27 | The definitive identifier for the SMS ATM OC-12 interface port.
rbnEntPortSMSCSMMGMT rbnEntityTypePort 36 1.3.6.1.4.1.2352.6.10.36 | The definitive identifier for the Connection System Manager (CSM), Local management port.
rbnEntPortSEXCMGMT rbnEntityTypePort 41 1.3.6.1.4.1.2352.6.10.41 | The definitive identifier for the SE Cross Connect, local management port.
rbnEntPortSEEIM rbnEntityTypePort 42 1.3.6.1.4.1.2352.6.10.42 | The definitive identifier for the SE 10/100BaseT Ethernet interface port.
rbnEntPortSEGIGEIM rbnEntityTypePort 43 1.3.6.1.4.1.2352.6.10.43 | The definitive identifier for the SE Gigabit Ethernet interface port.
rbnEntPortSEPOSOC12 rbnEntityTypePort 44 1.3.6.1.4.1.2352.6.10.44 | The definitive identifier for the SE POS OC-12 interface port.
rbnEntPortSEPOSOC48 rbnEntityTypePort 45 1.3.6.1.4.1.2352.6.10.45 | The definitive identifier for the SE POS OC-48 interface port.
rbnEntPortSEPOSOC3 rbnEntityTypePort 46 1.3.6.1.4.1.2352.6.10.46 | The definitive identifier for the SE POS OC3 interface port.
rbnEntPortSECHOC12DS1 rbnEntityTypePort 47 1.3.6.1.4.1.2352.6.10.47 | The definitive identifier for the SE Channelized OC12 DS1 interface port.
rbnEntPortSECHOC12DS3 rbnEntityTypePort 48 1.3.6.1.4.1.2352.6.10.48 | The definitive identifier for the SE Channelized OC12 DS3 interface port.
rbnEntPortSEAIMOC3 rbnEntityTypePort 49 1.3.6.1.4.1.2352.6.10.49 | The definitive identifier for the SE ATM OC3 interface port.
rbnEntPortSEAIMOC12 rbnEntityTypePort 50 1.3.6.1.4.1.2352.6.10.50 | The definitive identifier for the SE ATM OC12 interface port.
rbnEntPortSECHDS3 rbnEntityTypePort 51 1.3.6.1.4.1.2352.6.10.51 | The definitive identifier for the SE Channelized DS3 interface port.
rbnEntPortSEDS3 rbnEntityTypePort 52 1.3.6.1.4.1.2352.6.10.52 | The definitive identifier for the SE DS3 interface port.
rbnEntPortSEAIMDS3 rbnEntityTypePort 53 1.3.6.1.4.1.2352.6.10.53 | The definitive identifier for the SE ATM DS3 interface port.
rbnEntPortSECHSTM1E1 rbnEntityTypePort 54 1.3.6.1.4.1.2352.6.10.54 | The definitive identifier for the SE Channelized STM-1 to E1 interface port.
rbnEntPortSEE1 rbnEntityTypePort 55 1.3.6.1.4.1.2352.6.10.55 | The definitive identifier for the SE E1 interface port.
rbnEntPortSEXC3MGMT rbnEntityTypePort 56 1.3.6.1.4.1.2352.6.10.56 | The definitive identifier for the SE Cross Connect 3, local management port.
rbnEntPortSEE3 rbnEntityTypePort 57 1.3.6.1.4.1.2352.6.10.57 | The definitive identifier for the SE E3 interface port.
rbnEntPortSEAIMOC12E rbnEntityTypePort 58 1.3.6.1.4.1.2352.6.10.58 | The definitive identifier for the SE ATM OC12 Enhanced interface port.
rbnEntPortSEGIGETM rbnEntityTypePort 59 1.3.6.1.4.1.2352.6.10.59 | The definitive identifier for the SE Gigabit Ethernet with Traffic Management interface port.
rbnEntPortSE10GIGEIM rbnEntityTypePort 60 1.3.6.1.4.1.2352.6.10.60 | The definitive identifier for the SE 10 Gigabit Ethernet Interface Management port.
rbnEntPortSE100XCMGMT rbnEntityTypePort 61 1.3.6.1.4.1.2352.6.10.61 | The definitive identifier for the SE 100 Cross Connect, local management port.
rbnEntPortSE100EIM rbnEntityTypePort 62 1.3.6.1.4.1.2352.6.10.62 | The definitive identifier for the SE 100 10/100BaseT Ethernet Interface Management port.
rbnEntPortSE100FXIM rbnEntityTypePort 63 1.3.6.1.4.1.2352.6.10.63 | The definitive identifier for the SE 100 FX-100 Ethernet interface port.
rbnEntModuleSE100GERJMIC rbnEntityTypePort 64 1.3.6.1.4.1.2352.6.10.64 | The definitive identifier for the SE 100 Gigabit Ethernet interface port.
rbnEntModuleSE100GEFXMIC rbnEntityTypePort 65 1.3.6.1.4.1.2352.6.10.65 | The definitive identifier for the SE 100 FX-1000 Ethernet interface port.
rbnEntPortSEXC4MGMT rbnEntityTypePort 66 1.3.6.1.4.1.2352.6.10.66 | The definitive identifier for the SE Cross Connect 4, local management port.
rbnEntPortSE100AIMOC3 rbnEntityTypePort 67 1.3.6.1.4.1.2352.6.10.67 | The definitive identifier for the SE 100 ATM OC-3 interface port.
rbnEntPortSEPOSOC192 rbnEntityTypePort 68 1.3.6.1.4.1.2352.6.10.68 | The definitive identifier for the SE POS OC-192 interface port.
rbnEntPortSE10GIGETM rbnEntityTypePort 69 1.3.6.1.4.1.2352.6.10.69 | The definitive identifier for the SE 10 Gigabit Ethernet Traffic Management interface port.
rbnEntPortSM10GIGEIM rbnEntityTypePort 101 1.3.6.1.4.1.2352.6.10.101 | The definitive identifier for the SM 10 Gigabit Ethernet interface port.
rbnEntPortSMRPMGMT rbnEntityTypePort 103 1.3.6.1.4.1.2352.6.10.103 | The definitive identifier for the SMRP local management port.
rbnEntPortSMGIGEIM rbnEntityTypePort 104 1.3.6.1.4.1.2352.6.10.104 | The definitive identifier for the SM Gigabit Ethernet interface port.
rbnEntPortSMGIGETM rbnEntityTypePort 105 1.3.6.1.4.1.2352.6.10.105 | The definitive identifier for the SM Gigabit Ethernet with Traffic Management interface port.
rbnEntPortSM10GIGETM rbnEntityTypePort 106 1.3.6.1.4.1.2352.6.10.106 | The definitive identifier for the SM 10 Gigabit Ethernet with Traffic Management port.
rbnEntPortSMEIM rbnEntityTypePort 107 1.3.6.1.4.1.2352.6.10.107 | The definitive identifier for the SM 10/100BaseT Ethernet interface port.
rbnEntPortSMCHOC3OC12 rbnEntityTypePort 108 1.3.6.1.4.1.2352.6.10.108 | The definitive identifier for the SM Channelized 3/STM1 or OC12/STM4 Interface Port.
rbnEntPortSMCHOC3 rbnEntityTypePort 109 1.3.6.1.4.1.2352.6.10.109 | The definitive identifier for the SM Channelized C3/STM1 Interface Port.

Table 83 Stack Objects
Object and Object Identifier | Description
--- | ---
rbnEntityTypeStack rbnEntities 11 1.3.6.1.4.1.2352.6.11 | The top-level category identifier for entities which reside in the ENTITY-MIB PhysicalClass module.

Table 84 CPU Objects
Object and Object Identifier | Description
--- | ---
rbnEntityTypeCPU rbnEntities 12 1.3.6.1.4.1.2352.6.12 | The top-level category identifier for entities which reside in the ENTITY-MIB PhysicalClass module.

Table 85 Disk Objects
Object and Object Identifier | Description
--- | ---
rbnEntityTypeDisk rbnEntities 13 1.3.6.1.4.1.2352.6.13 | The top-level category identifier for entities which reside in the ENTITY-MIB PhysicalClass module.
rbnEntDiskUnknown rbnEntityTypeDisk 1 1.3.6.1.4.1.2352.6.13.1 | The identifier use to represent any disk which cannot be definitively identified.
rbnEntDiskSSE rbnEntityTypeDisk 2 1.3.6.1.4.1.2352.6.13.2 | The definitive identifier for the removable disks on SSE card.

Table 86 Memory Objects
Object and Object Identifier | Description
--- | ---
rbnEntityTypeMemory rbnEntities 14 1.3.6.1.4.1.2352.6.14 | The top-level category identifier for entities which reside in the ENTITY-MIB PhysicalClass module.

## 1.33 RBN-PVC-MIB

Defines the objects used to support the creation, deletion, and management of ATM and Ethernet 802.1Q PVCs.

### 1.33.1 rbnAtmPvcConfigTable

This table contains the objects that identify and configure ATM PVCs.

`Index:` rbnAtmPvcSlot, rbnAtmPvcPort, rbnAtmPvcVpi, rbnAtmPvcVci

Table 87 describes the objects in rbnAtmPvcConfigTable. All objects in the table are read-only unless otherwise specified.

Table 87 Objects in rbnAtmPvcConfigTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnAtmPvcSlot rbnAtmPvcConfigEntry 1.3.6.1.4.1.2352.2.7.1.1.1.1 | RbnSlot Unsigned32 | 0..255 | The chassis slot number.
rbnAtmPvcPort rbnAtmPvcConfigEntry 2 1.3.6.1.4.1.2352.2.7.1.1.1.2 | RbnSlot Unsigned32 | 0..255 | The port number.
rbnAtmPvcVpi rbnAtmPvcConfigEntry 3 1.3.6.1.4.1.2352.2.7.1.1.1.3 | Unsigned32 | 0..255 | The Virtual Path Identifier for the PVC
rbnAtmPvcVci rbnAtmPvcConfigEntry 4 1.3.6.1.4.1.2352.2.7.1.1.1.4 | Unsigned32 | 0..65535 | The Virtual Channel Identifier for the PVC.
rbnAtmPvcProfileName rbnAtmPvcConfigEntry 5 1.3.6.1.4.1.2352.2.7.1.1.1.5 | SnmpAdminString | 1..63 | The profile name to use with the PVC.
rbnAtmPvcEncapsulation rbnAtmPvcConfigEntry 6 1.3.6.1.4.1.2352.2.7.1.1.1.6 | RbnAtmEncapsulation Integer | 0—unknown 2—bridge1483 3—multi1483 4—route1483 7—ppp 9—pppOverEthernet 14—raw | The encapsulation to use with the PVC.
rbnAtmPvcRowStatus rbnAtmPvcConfigEntry 8 1.3.6.1.4.1.2352.2.7.1.1.1.8 | RowStatus Integer | 1—active | Indicates the active row.
rbnAtmPvcCircuitType rbnAtmPvcConfigEntry 9 1.3.6.1.4.1.2352.2.7.1.1.1.9 | RbnPvcCircuitType Integer | 1—explicit 2—explicitRange 3—onDemandRange | The PVC circuit type. For this MIB object, only those entries with an rbnAtmPvcCircuitType object that has a value 'explicit' can be removed by setting the rbnAtmPvcRowStatus object equal to 'destroy'.
rbnAtmPvcCircuitHandle rbnAtmPvcConfigEntry 10 1.3.6.1.4.1.2352.2.7.1.1.1.1 | RbnCircuitHandle Octet String | SIZE (8) | Used internally to uniquely identify a circuit. The value of this object can be used to correlate entries with those in rbnBindTable defined in the RBN-BIND-MIB.
rbnAtmPvcClearCircuit rbnAtmPvcConfigEntry 11 1.3.6.1.4.1.2352.2.7.1.1.1.11 | TruthValue Integer | 1—true 2—false | When this object is true, the system clears active subscriber sessions on the specified circuit. When false, there is no action taken.

### 1.33.2 rbnFrameRelayPvcConfigTable

This table contains the objects that identify and configure Frame Relay PVCs.

`Index:` rbnFrameRelayPvcSlot, rbnFrameRelayPvcPort, rbnFrameRelayPvcChannel, rbnFrameRelayPvcDLCI

Table 88 describes the objects in rbnFrameRelayPvcConfigTable. All objects in the table are read-only unless otherwise specified.

Table 88 Objects in rbnFrameRelayPvcConfigTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnFrameRelayPvcSlot rbnFrameRelayPvcConfigEntry 1 1.3.6.1.4.1.2352.2.7.1.2.1.1 | RbnSlot Unsigned32 | 0..255 | The chassis slot number.
rbnFrameRelayPvcPort rbnFrameRelayPvcConfigEntry 2 1.3.6.1.4.1.2352.2.7.1.2.1.2 | RbnPort Unsigned32 | 0..255 | The port number.
rbnFrameRelayPvcChannel rbnFrameRelayPvcConfigEntry 3 1.3.6.1.4.1.2352.2.7.1.2.1.3 | Unsigned32 | 0..255 | The channel number
rbnFrameRelayPvcDLCI rbnFrameRelayPvcConfigEntry 4 1.3.6.1.4.1.2352.2.7.1.2.1.4 | Unsigned32 | 0..65535 | The Data Link Connection Identifier.
rbnFrameRelayPvcProfileName rbnFrameRelayPvcConfigEntry 5 1.3.6.1.4.1.2352.2.7.1.2.1.5 | SnmpAdminString | 1..63 | The profile name to use with the PVC. This object is read-create.
rbnFrameRelayPvcEncapsulation rbnFrameRelayPvcConfigEntry 6 1.3.6.1.4.1.2352.2.7.1.2.1.6 | RbnFrameRelayEncapsulation Integer | 1—auto1490 2—bridge1490 3—multi1490 4—route1490 5—l2tp 6—l2tpVcMuxed 7—ppp 8—pppAuto 9—pppOverEthernet 10—dot1a1490 11—clips1490 12—pppAutoNopoe | The encapsulation to use with the PVC. This object is read-create.
rbnFrameRelayPvcRowStatus rbnFrameRelayPvcConfigEntry 8 1.3.6.1.4.1.2352.2.7.1.2.1.8 | RowStatus Integer | 1—active 2—notInService 3—notReady 4— createAndGo 5— createAndWait 6—destroy | The row status for creating, modifying, or deleting an entry in the table. This object is read-create.
rbnFrameRelayPvcCircuitType rbnFrameRelayPvcConfigEntry 9 1.3.6.1.4.1.2352.2.7.1.2.1.9 | RbnPvcCircuitType Integer | 1—explicit 2— explicitRange 3— onDemandRange 4—protection | The PVC circuit type. For this MIB object, only those entries with an rbnFrameRelayPvcCircuitType object that has a value of explicit can be removed by setting the rbnFrameRelayPvcRowStatus object equal to destroy. This object is read-create.
rbnFrameRelayPvcCircuitHandle rbnFrameRelayPvcConfigEntry 10 1.3.6.1.4.1.2352.2.7.1.2.1.10 | RbnCircuitHandle Octet String | SIZE (8) | Used internally to uniquely identify a circuit. The value of this object can be used to correlate entries with those in rbnBindTable defined in the RBN-BIND-MIB.
rbnFrameRelayPvcClearCircuit rbnFrameRelayPvcConfigEntry 11 1.3.6.1.4.1.2352.2.7.1.2.1.11 | TruthValue Integer | 1—true 2—false | When this object is true, the system clears active subscriber sessions on the specified circuit. When false, there is no action taken. This object can only be written when the conceptual row exists. When this object is set to true and the encapsulation of the circuit is bridged or routed (for example, bridge1490 or route1490), subscribers reauthenticate after being cleared. This object is read-create.

### 1.33.3 rbnDot1qPvcOnEthConfigTable

This table contains the objects that identify and configure IEEE 802.1Q PVCs on Ethernet ports.

`Index:` rbnDot1qPvcOnEthSlot, rbnDot1qPvcOnEthPort, rbnDot1qPvcOnEthVlanId

Table 89 describes the objects in rbnDot1qPvcOnEthConfigTable. All objects in the table are read-only unless otherwise specified.

Table 89 Objects in rbnDot1qPvcOnEthConfigTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnDot1qPvcOnEthSlot rbnDot1qPvcOnEthConfigEntry 1 1.3.6.1.4.1.2352.2.7.1.3.1.1 | Unsigned32 | 0..255 | The chassis slot number.
rbnDot1qPvcOnEthPort rbnDot1qPvcOnEthConfigEntry 2 1.3.6.1.4.1.2352.2.7.1.3.1.2 | Unsigned32 | 0..255 | The port number.
rbnDot1qPvcOnEthVlanId rbnDot1qPvcOnEthConfigEntry 3 1.3.6.1.4.1.2352.2.7.1.3.1.3 | Integer | 1..4095 | IEEE 802.1Q Virtual LAN (VLAN) tag value.
rbnDot1qPvcOnEthRowStatus rbnDot1qPvcOnEthConfigEntry 4 1.3.6.1.4.1.2352.2.7.1.3.1.4 | RowStatus Integer | 1—active | Indicates the active row.
rbnDot1qPvcOnEthProfileName rbnDot1qPvcOnEthConfigEntry 5 1.3.6.1.4.1.2352.2.7.1.3.1.5 | SnmpAdminString | 1..63 | The profile name to use with the PVC.
rbnDot1qPvcOnEthEncapsulation rbnDot1qPvcOnEthConfigEntry 6 1.3.6.1.4.1.2352.2.7.1.3.1.6 | RbnDot1qEncap- sulation Integer | 0—unknown 1—ipOverEthernet 2—dot1qMulti 3—pppOverEthernet 4—dot1qRaw | The encapsulation to use with the PVC.
rbnDot1qPvcOnEthCircuitType rbnDot1qPvcOnEthConfigEntry 7 1.3.6.1.4.1.2352.2.7.1.3.1.7 | RbnPvcCircuit Type Integer | 1—explicit 3—onDemandRange | The PVC circuit type. For this MIB object, only those entries with an rbnDot1qPvcOnEthCircuitType object that has a value of explicit can be removed by setting the rbnDot1qPvcOnEthRowStatus object equal to destroy.
rbnDot1qPvcOnEthCircuitHandle rbnDot1qPvcOnEthConfigEntry 8 1.3.6.1.4.1.2352.2.7.1.3.1.8 | RbnCircuitHandle Octet String | SIZE (8) | Used internally to uniquely identify a circuit. The value of this object can be used to correlate entries with those in the rbnBindTable object defined in the RBN-BIND-MIB.
rbnDot1qPvcOnEthClearCircuit rbnDot1qPvcOnEthConfigEntry 9 1.3.6.1.4.1.2352.2.7.1.3.1.9 | TruthValue | 1—true 2—false | When this object is true , the system clears active subscriber sessions on the specified circuit. When false, there is no action taken. This object can be written only when the conceptual row exists. This object is read-create.

### 1.33.4 rbnDot1qPvcOnAtmConfigTable

This table contains the objects that identify and configure IEEE 802.1Q PVCs on ATM circuits.

`Index:` rbnDot1qPvcOnAtmSlot, rbnDot1qPvcOnAtmPort, rbnDot1qPvcOnAtmVpi, rbnDot1qPvcOnAtmVci, rbnDot1qPvcOnAtmVlanId

Table 90 describes the objects in rbnDot1qPvcOnAtmConfigTable.

Table 90 Objects in rbnDot1qPvcOnAtmConfigTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnDot1qPvcOnAtmSlot rbnDot1qPvcOnAtmConfigEntry 1 1.3.6.1.4.1.2352.2.7.1.4.1.1 | RbnSlot Unsigned32 | 0..255 | The chassis slot number.
rbnDot1qPvcOnAtmPort rbnDot1qPvcOnAtmConfigEntry 2 1.3.6.1.4.1.2352.2.7.1.4.1.2 | RbnPort Unsigned32 | 0..255 | The port number.
rbnDot1qPvcOnAtmVpi rbnDot1qPvcOnAtmConfigEntry 3 1.3.6.1.4.1.2352.2.7.1.4.1.3 | Unsigned32 | 0..255 | The Virtual Path Identifier for the PVC.
rbnDot1qPvcOnAtmVci rbnDot1qPvcOnAtmConfigEntry 4 1.3.6.1.4.1.2352.2.7.1.4.1.4 | Unsigned32 | 0..65535 | The Virtual Channel Identifier for the PVC.
rbnDot1qPvcOnAtmVlanId rbnDot1qPvcOnAtmConfigEntry 5 1.3.6.1.4.1.2352.2.7.1.4.1.5 | RbnVidOrUntagged Integer32 | 1..4096 | IEEE 802.1Q Virtual LAN (VLAN) tag value.
rbnDot1qPvcOnAtmRowStatus rbnDot1qPvcOnAtmConfigEntry 6 1.3.6.1.4.1.2352.2.7.1.4.1.6 | RowStatus Integer | 1—active 2—notInService 3—notReady 4—createAndGo 5—createAndWait 6—destroy | The row status for creating, modifying, or deleting an entry in the table.
rbnDot1qPvcOnAtmProfileName rbnDot1qPvcOnAtmConfigEntry 7 1.3.6.1.4.1.2352.2.7.1.4.1.7 | SnmpAdminString | 1..63 | The profile name to use with the PVC.
rbnDot1qPvcOnAtmEncapsulation rbnDot1qPvcOnAtmConfigEntry 8 1.3.6.1.4.1.2352.2.7.1.4.1.8 | RbnDot1qEncapsulation Integer | 0—unknown 1—ipOverEthernet 2—dot1qMulti 3—pppOverEthernet 4—dot1qRaw 5—dot1qClips 6—dot1qTunnelMulti 7—dot1qTunnelPppOverEthernet 8—dot1qTunnelRaw 9—dot1qTunnelClips | The encapsulation to use with the PVC.
rbnDot1qPvcOnAtmCircuitType rbnDot1qPvcOnAtmConfigEntry 9 1.3.6.1.4.1.2352.2.7.1.4.1.9 | RbnPvcCircuitType Integer | 1—explicit 2—explicitRange 3—onDemandRange 4—protection | The PVC circuit type. For this object, only entries of the rbnDot1qPvcOnAtmCircuit Type object with the value 'explicit' may be removed by setting the rbnDot1qPvcOnAtmRow Status object equal to 'destroy'.
rbnDot1qPvcOnAtmCircuitHandle rbnDot1qPvcOnAtmConfigEntry 10 1.3.6.1.4.1.2352.2.7.1.4.1.10 | RbnCircuitHandle Octet String | SIZE (8) | Used internally to uniquely identify a circuit. The value of this object can be used to correlate entries with those in the rbnBindTable object defined in the RBN-BIND-MIB.
rbnDot1qPvcOnAtmClearCircuit rbnDot1qPvcOnAtmConfigEntry 11 1.3.6.1.4.1.2352.2.7.1.4.1.11 | TruthValue | 1—true 2—false | When this object is true, the system clears active subscriber sessions on the specified circuit. When false, there is no action taken. This object can be written only when the conceptual row exists. This object is read-create.

### 1.33.5 rbnDot1qPvcOnFrConfigTable

This table contains the objects that identify and configure IEEE 802.1Q PVCs on Frame Relay ports.

`Index:` rbnDot1qPvcOnFrSlot, rbnDot1qPvcOnFrPort, rbnDot1qPvcOnFrChannel, rbnDot1qPvcOnFrDLCI, rbnDot1qPvcOnFrVlanId

Table 91 describes the objects in rbnDot1qPvcOnFrConfigTable. All objects in the table are read-only unless otherwise specified.

Table 91 Objects in rbnDot1qPvcOnFrConfigTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnDot1qPvcOnFrSlot rbnDot1qPvcOnFrConfigEntry 1 1.3.6.1.4.1.2352.2.7.1.5.1.1 | RbnSlot Unsigned32 | 0..255 | The chassis slot number.
rbnDot1qPvcOnFrPort rbnDot1qPvcOnFrConfigEntry 2 1.3.6.1.4.1.2352.2.7.1.5.1.2 | RbnPort Unsigned32 | 0..255 | The port number.
rbnDot1qPvcOnFrChannel rbnDot1qPvcOnFrConfigEntry 3 1.3.6.1.4.1.2352.2.7.1.5.1.3 | Unsigned32 | 0..65535 | The channel number.
rbnDot1qPvcOnFrDLCI rbnDot1qPvcOnFrConfigEntry 4 1.3.6.1.4.1.2352.2.7.1.5.1.4 | Unsigned32 | 0..65535 | The Data Link Connection Identifier.
rbnDot1qPvcOnFrVlanId rbnDot1qPvcOnFrConfigEntry 5 1.3.6.1.4.1.2352.2.7.1.5.1.5 | RbnVidOrUntagged Integer32 | 1..4096 | IEEE 802.1Q Virtual LAN (VLAN) tag value.
rbnDot1qPvcOnFrRowStatus rbnDot1qPvcOnFrConfigEntry 6 1.3.6.1.4.1.2352.2.7.1.5.1.6 | RowStatus Integer | 1—active 2—notInService 3—notReady 4—createAndGo 5—createAndWait 6—destroy | The row status for creating, modifying, or deleting an entry in the table.
rbnDot1qPvcOnFrProfileName rbnDot1qPvcOnFrConfigEntry 7 1.3.6.1.4.1.2352.2.7.1.5.1.7 | SnmpAdminString | 1..63 | The profile name to use with the PVC.
rbnDot1qPvcOnFrEncapsulation rbnDot1qPvcOnFrConfigEntry 8 1.3.6.1.4.1.2352.2.7.1.5.1.8 | RbnDot1qEncapsulation Integer | 0—unknown 1—ipOverEthernet 2—dot1qMulti 3—pppOverEthernet 4—dot1qRaw 5—dot1qClips 6—dot1qTunnelMulti 7—dot1qTunnelPppOverEthernet 8—dot1qTunnelRaw 9—dot1qTunnelClips | The encapsulation to use with the PVC.
rbnDot1qPvcOnFrCircuitType rbnDot1qPvcOnFrConfigEntry 9 1.3.6.1.4.1.2352.2.7.1.5.1.9 | RbnPvcCircuitType Integer | 1—explicit 2—explicitRange 3—onDemandRange 4—protection | The PVC circuit type. For this object, only entries of the rbnDot1qPvcOnFrCircuitType object with the value 'explicit' may be removed by setting the rbnDot1qPvcOnFrRowStatus object equal to 'destroy'.
rbnDot1qPvcOnFrCircuitHandle rbnDot1qPvcOnFrConfigEntry 10 1.3.6.1.4.1.2352.2.7.1.5.1.10 | RbnCircuitHandle Octet String | SIZE (8) | Used internally to uniquely identify a circuit. The value of this object can be used to correlate entries with those in the rbnBindTable object defined in the RBN-BIND-MIB.
rbnDot1qPvcOnFrClearCircuit rbnDot1qPvcOnFrConfigEntry 11 1.3.6.1.4.1.2352.2.7.1.5.1.11 | TruthValue Integer | 1—true 2—false | When true, the system clears active subscriber sessions on the specified circuit. When false, there is no action taken. This object can be written only when the conceptual row exists. This object is read-create.

## 1.34 RBN-QOS-MIB

This table contains the objects that manage interfaces that have quality of service (QoS) enabled. These objects also monitor the QoS queue statistics on the subscriber circuits (CLIPS and PPPoE), with traffic management (TM) based priority weighted fair queuing (PWFQ).

Note:
  The interface MIB tables include MIB objects only if the corresponding QoS configurations exist.

Table 92 describes the parallelism between MIB tables and objects for non-subscriber (bind interface) and subscriber (bind subscriber or auth subscriber) circuits.

Table 92 RBN-QOS-MIB Circuits
Non-subscriber circuits | Subscriber circuits
--- | ---
IF-MIB:: ifTable / ifXTable | RBN-SUBSCRIBER-ACTIVE-MIB:: rbnSubsActiveTable/rbnSubsStatsTable
RBN-QOS-MIB:: rbnQosInterfaceTable | N/A
RBN-QOS-MIB:: rbnQosInterfaceQueueStatsTable | RBN-QOS-MIB:: rbnQosSubscriberQueueStatsTable
RBN-QOS-MIB:: rbnQosIntfRLClassStatsTable | RBN-QOS-MIB:: rbnQosSubscriberRLClassStatsTable
RBN-QOS-MIB:: rbnQosHierarchicalPolicyStatsTable | N/A
RBN-QOSMIB:: rbnQosHierarchicalPClassStatsTable | N/A

### 1.34.1 rbnQosInterfaceTable

This table contains entries for every packet-oriented IF-MIB layer for which QoS is enabled.

`Index:` ifIndex

Table 93 describes the objects in rbnQosInterfaceTable.

Table 93 Objects in rbnQosInterfaceTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnQosIfInOctets rbnQosInterfaceEntry 1 1.3.6.1.4.1.2352.2.22.1.1.1.1 | Counter32 | 0..4294967295 | The total number of post-limited octets received on the interface, including framing characters. Discontinuities in the value of this counter can occur at reinitialization of the management system and at other times as indicated by the value of the ifCounterDiscontinuityTime object.
rbnQosIfHCInOctets rbnQosInterfaceEntry 2 1.3.6.1.4.1.2352.2.22.1.1.1.2 | Counter64 | 0..18446744073709551615 | The total number of post-limited octets received on the interface, including framing characters. This object is 64-bit version of the rbnQosIfInOctets object. Discontinuities in the value of this counter can occur at reinitialization of the management system and at other times as indicated by the value of the ifCounterDiscontinuityTime object.
rbnQosIfOutOctets rbnQosInterfaceEntry 3 1.3.6.1.4.1.2352.2.22.1.1.1.3 | Counter32 | 0..4294967295 | The total number of prelimited octets transmitted out of the interface, including framing characters. Discontinuities in the value of this counter can occur at reinitialization of the management system and at other times as indicated by the value of the ifCounterDiscontinuityTime object.
rbnQosIfHCOutOctets rbnQosInterfaceEntry 4 1.3.6.1.4.1.2352.2.22.1.1.1.4 | Counter64 | 0..18446744073709551615 | The total number of prelimited octets transmitted out of the interface, including framing characters. This object is a 64-bit version of the rbnQosIfOutOctets object. Discontinuities in the value of this counter can occur at reinitialization of the management system and at other times as indicated by the value of the ifCounterDiscontinuityTime object.
rbnQosIfInDroppedOctets rbnQosInterfaceEntry 5 1.3.6.1.4.1.2352.2.22.1.1.1.5 | Counter32 | 0..4294967295 | The total number of received octets that were dropped on the interface, including but not limited to octets dropped due to limiting. Discontinuities in the value of this counter can occur at reinitialization of the management system and at other times as indicated by the value of the ifCounterDiscontinuityTime object. NOTE: This object is not supported for ATM cards using PortMaker II (PM2) SAR, e.g. atm-ds3-12-port, atm-oc3-4-port, atm-oc12e-1-port, etc.
rbnQosIfHCInDroppedOctets rbnQosInterfaceEntry 6 1.3.6.1.4.1.2352.2.22.1.1.1.6 | Counter64 | 0..18446744073709551615 | The total number of received octets that were dropped on the interface, including but not limited to octets dropped due to limiting. This object is a 64-bit version of the rbnQosIfInDroppedOctets object. Discontinuities in the value of this counter can occur at reinitialization of the management system and at other times as indicated by the value of the ifCounterDiscontinuityTime object. NOTE: This object is not supported for ATM cards using PortMaker II (PM2) SAR, e.g. atm-ds3-12-port, atm-oc3-4-port, atm-oc12e-1-port, etc.
rbnQosIfOutDroppedOctets rbnQosInterfaceEntry 7 1.3.6.1.4.1.2352.2.22.1.1.1.7 | Counter32 | 0..4294967295 | The total number of outbound octets that were dropped on the interface, including but not limited to octets dropped due to limiting. Discontinuities in the value of this counter can occur at reinitialization of the management system and at other times as indicated by the value of the ifCounterDiscontinuityTime object. NOTE: This object is not supported for ATM cards using PortMaker II (PM2) SAR, e.g. atm-ds3-12-port, atm-oc3-4-port, atm-oc12e-1-port, etc.
rbnQosIfHCOutDroppedOctets rbnQosInterfaceEntry 8 1.3.6.1.4.1.2352.2.22.1.1.1.8 | Counter64 | 0..18446744073709551615 | The total number of outbound octets that were dropped on the interface, including but not limited to octets dropped due to limiting. This object is a 64-bit version of the rbnQosIfOutDroppedOctets object. Discontinuities in the value of this counter can occur at reinitialization of the management system and at other times as indicated by the value of the ifCounterDiscontinuityTime object. NOTE: This object is not supported for ATM cards using PortMaker II (PM2) SAR, e.g. atm-ds3-12-port, atm-oc3-4-port, atm-oc12e-1-port, etc.

### 1.34.2 rbnQosInterfaceQueueStatsTable

This table specifies statistical information for each transmit queue. It contains the transmit queue octet counts for each packet-oriented IF-MIB layer for which QoS is enabled.

`Index:` ifIndex, rbnQosIfQueueId

Table 94 describes the objects in rbnQosInterfaceQueueStatsTable.

Table 94 Objects in rbnQosInterfaceQueueStatsTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnQosIfQueueId rbnQosInterfaceQueueStatsEntry 1 1.3.6.1.4.1.2352.2.22.1.2.1.1 | Unsigned32 | 0..4294967295 | A unique identifier for a transmit queue within an interface.
rbnQosIfQueueOutOctets rbnQosInterfaceQueueStatsEntry 2 1.3.6.1.4.1.2352.2.22.1.2.1.2 | Counter32 | 0..4294967295 | The number of octets transmitted out of this queue. Discontinuities in the value of this counter can occur at reinitialization of the management system and at other times as indicated by the value of the ifCounterDiscontinuityTime object.
rbnQosIfQueueOutPkts rbnQosInterfaceQueueStatsEntry 3 1.3.6.1.4.1.2352.2.22.1.2.1.3 | Counter32 | 0..4294967295 | The number of packets transmitted out of this queue. Discontinuities in the value of this counter can occur at reinitialization of the management system and at other times as indicated by the value of the ifCounterDiscontinuityTime object.
rbnQosIfQueueWredDroppedOctets rbnQosInterfaceQueueStatsEntry 4 1.3.6.1.4.1.2352.2.22.1.2.1.4 | Counter32 | 0..4294967295 | The number of octets dropped due to the application of a WRED algorithm. Discontinuities in the value of this counter can occur at reinitialization of the management system and at other times as indicated by the value of the ifCounterDiscontinuityTime object. NOTE: This object is not supported for ATM cards using PortMaker II (PM2) SAR, e.g. atm-ds3-12-port, atm-oc3-4-port, atm-oc12e-1-port, etc.
rbnQosIfQueueWredDroppedPkts rbnQosInterfaceQueueStatsEntry 5 1.3.6.1.4.1.2352.2.22.1.2.1.5 | Counter32 | 0..4294967295 | The number of packets dropped due to the application of a WRED algorithm. Discontinuities in the value of this counter can occur at reinitialization of the management system and at other times as indicated by the value of the ifCounterDiscontinuityTime object.
rbnQosIfQueueTailDroppedOctets rbnQosInterfaceQueueStatsEntry 6 1.3.6.1.4.1.2352.2.22.1.2.1.6 | Counter32 | 0..4294967295 | The number of octets dropped when the total number of packets in this queue was greater than the maximum threshold. Discontinuities in the value of this counter can occur at reinitialization of the management system and at other times as indicated by the value of the ifCounterDiscontinuityTime object. NOTE: This object is not supported for ATM cards using PortMaker II (PM2) SAR, e.g. atm-ds3-12-port, atm-oc3-4-port, atm-oc12e-1-port, etc.
rbnQosIfQueueTailDroppedPkts rbnQosInterfaceQueueStatsEntry 7 1.3.6.1.4.1.2352.2.22.1.2.1.7 | Counter32 | 0..4294967295 | The number of packets dropped when the total number of packets in this queue was greater than the maximum threshold. Discontinuities in the value of this counter can occur at reinitialization of the management system and at other times as indicated by the value of the ifCounterDiscontinuityTime object.
rbnQosIfQueueHCOutOctets rbnQosInterfaceQueueStatsEntry 8 1.3.6.1.4.1.2352.2.22.1.2.1.8 | Counter64 | 0..18446744073709551615 | The number of octets transmitted out of this queue. This object is a 64-bit version of the rbnQosIfQueueOutOctets object. Discontinuities in the value of this counter can occur at reinitialization of the management system and at other times as indicated by the value of the ifCounterDiscontinuityTime object.
rbnQosIfQueueHCOutPkts rbnQosInterfaceQueueStatsEntry 9 1.3.6.1.4.1.2352.2.22.1.2.1.9 | Counter64 | 0..18446744073709551615 | The number of packets transmitted out of this queue. This object is a 64-bit version of the rbnQosIfQueueOutPkts object. Discontinuities in the value of this counter can occur at reinitialization of the management system and at other times as indicated by the value of the ifCounterDiscontinuityTime object.
rbnQosIfQueueHCWredDroppedOctets rbnQosInterfaceQueueStatsEntry 10 1.3.6.1.4.1.2352.2.22.1.2.1.10 | Counter64 | 0..18446744073709551615 | The number of octets dropped due to the application of a WRED algorithm. This object is a 64-bit version of the rbnQosIfQueueWredDroppedOctets object. Discontinuities in the value of this counter can occur at reinitialization of the management system and at other times as indicated by the value of the ifCounterDiscontinuityTime object. NOTE: This object is not supported for ATM cards using PortMaker II (PM2) SAR, e.g. atm-ds3-12-port, atm-oc3-4-port, atm-oc12e-1-port, etc.
rbnQosIfQueueHCWredDroppedPkts rbnQosInterfaceQueueStatsEntry 11 1.3.6.1.4.1.2352.2.22.1.2.1.11 | Counter64 | 0..18446744073709551615 | The number of packets dropped due to the application of a WRED algorithm. This object is a 64-bit version of the rbnQosIfQueueWredDroppedPkts object. Discontinuities in the value of this counter can occur at reinitialization of the management system and at other times as indicated by the value of the ifCounterDiscontinuityTime object.
rbnQosIfQueueHCTailDroppedOctets rbnQosInterfaceQueueStatsEntry 12 1.3.6.1.4.1.2352.2.22.1.2.1.12 | Counter64 | 0..18446744073709551615 | The number of octets dropped when the total number of packets in this queue was greater than the maximum threshold. This object is a 64-bit version of the rbnQosIfQueueTailDroppedOctets object. Discontinuities in the value of this counter can occur at reinitialization of the management system and at other times as indicated by the value of the ifCounterDiscontinuityTime object. NOTE: This object is not supported for ATM cards using PortMaker II (PM2) SAR, e.g. atm-ds3-12-port, atm-oc3-4-port, atm-oc12e-1-port, etc.
rbnQosIfQueueHCTailDroppedPkts rbnQosInterfaceQueueStatsEntry 13 1.3.6.1.4.1.2352.2.22.1.2.1.13 | Counter64 | 0..18446744073709551615 | The number of packets dropped when the total number of packets in this queue was greater than the maximum threshold. This object is a 64-bit version of the rbnQosIfQueueTailDroppedPkts object. Discontinuities in the value of this counter can occur at reinitialization of the management system and at other times as indicated by the value of the ifCounterDiscontinuityTime object.

### 1.34.3 rbnQosSubscriberQueueStatsTable

This table specifies per-transmit queue statistical information. It contains the transmit queue octet counts for each active subscriber session for which QoS queuing policy is enabled.

`Index:` rbnSubsActiveName, rbnSubsActiveSessionId, rbnQosSubsQueueId

Table 95 describes the objects in rbnQosSubscriberQueueStatsTable.

Table 95 Objects in rbnQosSubscriberQueueStatsTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnQosSubsQueueId rbnQosSubscriberQueueStatsEntry 1 1.3.6.1.4.1.2352.2.22.1.3.1.1 | Unsigned32 | 0..7 | A unique identifier for a transmit queue used by the circuit.
rbnQosSubsQueuePolicyName rbnQosSubscriberQueueStatsEntry 2 1.3.6.1.4.1.2352.2.22.1.3.1.2 | SnmpAdminString | 1..39 | The name of the queuing policy the subscriber circuit is using.
rbnQosSubsQueueOutOctets rbnQosSubscriberQueueStatsEntry 3 1.3.6.1.4.1.2352.2.22.1.3.1.3 | Counter32 | 0..4294967295 | The number of octets transmitted out of this queue. Discontinuities in the value of this counter can occur at reinitialization of the management system.
rbnQosSubsQueueOutPkts rbnQosSubscriberQueueStatsEntry 4 1.3.6.1.4.1.2352.2.22.1.3.1.4 | Counter32 | 0..4294967295 | The number of packets transmitted out of this queue. Discontinuities in the value of this counter can occur at reinitialization of the management system.
rbnQosSubsQueueWredDroppedOctets rbnQosSubscriberQueueStatsEntry 5 1.3.6.1.4.1.2352.2.22.1.3.1.5 | Counter32 | 0..4294967295 | The number of octets dropped due to the application of a WRED algorithm. Discontinuities in the value of this counter can occur at reinitialization of the management system.
rbnQosSubsQueueWredDroppedPkts rbnQosSubscriberQueueStatsEntry 6 1.3.6.1.4.1.2352.2.22.1.3.1.6 | Counter32 | 0..4294967295 | The number of packets dropped due to the application of a WRED algorithm. Discontinuities in the value of this counter can occur at reinitialization of the management system.
rbnQosSubsQueueTailDroppedOctets rbnQosSubscriberQueueStatsEntry 7 1.3.6.1.4.1.2352.2.22.1.3.1. | Counter32 | 0..4294967295 | The number of octets dropped when the total number of packets in this queue was greater than the maximum threshold. Discontinuities in the value of this counter can occur at reinitialization of the management system.
rbnQosSubsQueueTailDroppedPkts rbnQosSubscriberQueueStatsEntry 8 1.3.6.1.4.1.2352.2.22.1.3.1.8 | Counter32 | 0..4294967295 | The number of packets dropped when the total number of packets in this queue was greater than the maximum threshold. Discontinuities in the value of this counter can occur at reinitialization of the management system.
rbnQosSubsQueueHCOutOctets rbnQosSubscriberQueueStatsEntry 9 1.3.6.1.4.1.2352.2.22.1.3.1.9 | Counter64 | 0..18446744073709551615 | The number of octets transmitted out of this queue. This object is a 64-bit version of the rbnQosSubsQueueOutOctets object. Discontinuities in the value of this counter can occur at reinitialization of the management system.
rbnQosSubsQueueHCOutPkts rbnQosSubscriberQueueStatsEntry 10 1.3.6.1.4.1.2352.2.22.1.3.1.10 | Counter64 | 0..18446744073709551615 | The number of packets transmitted out of this queue. This object is a 64-bit version of the rbnQosSubsQueueOutPkts object. Discontinuities in the value of this counter can occur at reinitialization of the management system.
rbnQosSubsQueueHCWredDroppedOctets rbnQosSubscriberQueueStatsEntry 11 1.3.6.1.4.1.2352.2.22.1.3.1.11 | Counter64 | 0..18446744073709551615 | The number of octets dropped due to the application of a WRED algorithm. This object is a 64-bit version of the rbnQosSubsQueueWredDroppedOctets object. Discontinuities in the value of this counter can occur at reinitialization of the management system.
rbnQosSubsQueueHCWredDroppedPkts rbnQosSubscriberQueueStatsEntry 12 1.3.6.1.4.1.2352.2.22.1.3.1.12 | Counter64 | 0..18446744073709551615 | The number of packets dropped due to the application of a WRED algorithm. This object is a 64-bit version of the rbnQosSubsQueueWredDroppedPkts object. Discontinuities in the value of this counter can occur at reinitialization of the management system.
rbnQosSubsQueueHCTailDroppedOctets rbnQosSubscriberQueueStatsEntry 13 1.3.6.1.4.1.2352.2.22.1.3.1.13 | Counter64 | 0..18446744073709551615 | The number of octets dropped when the total number of packets in this queue was greater than the maximum threshold. This object is a 64-bit version of the rbnQosSubsQueueTailDroppedOctets object. Discontinuities in the value of this counter can occur at reinitialization of the management system.
rbnQosSubsQueueHCTailDroppedPkts rbnQosSubscriberQueueStatsEntry 14 1.3.6.1.4.1.2352.2.22.1.3.1.14 | Counter64 | 0..18446744073709551615 | The number of packets dropped when the total number of packets in this queue was greater than the maximum threshold. This object is a 64-bit version of the rbnQosSubsQueueTailDroppedPkts object. Discontinuities in the value of this counter can occur at reinitialization of the management system.

### 1.34.4 rbnQosIntfRLClassStatsTable

This table specifies per-class statistical information. It contains the class octet counts for each packet-oriented IF-MIB layer to which the class-based policing and metering policy is applied.

`Index:` ifIndex, rbnQosIfRLPolicyType, rbnQosIfRLClassId

Table 96 describes the objects in rbnQosIntfRLClassStatsTable.

Table 96 Objects in rbnQosIntfRLClassStatsTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnQosIfRLPolicyType rbnQosIntfRLClassStatsEntry 1 1.3.6.1.4.1.2352.2.22.1.4.1.1 | RbnQosPolicyType Integer | 1—policing 2—metering | The type of the rate-limit policy which is applied to the interface. policing (1): Indicates inbound policing is applied. metering (2): Indicates outbound policy is applied.
rbnQosIfRLClassId rbnQosIntfRLClassStatsEntry 2 1.3.6.1.4.1.2352.2.22.1.4.1.2 | RbnQosClassId Unsigned32 | 1..8 | A value that uniquely identifies a class defined in the rate-limit policy access list.
rbnQosIfRLPolicyName rbnQosIntfRLClassStatsEntry 3 1.3.6.1.4.1.2352.2.22.1.4.1.3 | SnmpAdminString OctetString | 1..39 | Name of the rate-limit policy.
rbnQosIfRLClassName rbnQosIntfRLClassStatsEntry 4 1.3.6.1.4.1.2352.2.22.1.4.1.4 | SnmpAdminString OctetString | 1..39 | Name of the class in the rate-limit policy access list.
rbnQosIfRLClassConformOctets rbnQosIntfRLClassStatsEntry 5 1.3.6.1.4.1.2352.2.22.1.4.1.5 | Counter64 | 0..18446744073709551615 | The number of octets that conform to the rate limit set on the interface for which class counters are enabled.
rbnQosIfRLClassConformPkts rbnQosIntfRLClassStatsEntry 6 1.3.6.1.4.1.2352.2.22.1.4.1.6 | Counter64 | 0..18446744073709551615 | The number of packets that conform to the rate limit set on the interface for which class counters are enabled.
rbnQosIfRLClassConformDroppedOctets rbnQosIntfRLClassStatsEntry 7 1.3.6.1.4.1.2352.2.22.1.4.1.7 | Counter64 | 0..18446744073709551615 | The number of octets dropped due to the application of a conform action on packets that conform to the rate limit set on the interface for which class counters are enabled.
rbnQosIfRLClassConformDroppedPkts rbnQosIntfRLClassStatsEntry 8 1.3.6.1.4.1.2352.2.22.1.4.1.8 | Counter64 | 0..18446744073709551615 | The number of packets dropped due to the application of a conform action on packets that conform to the rate limit set on the interface for which class counters are enabled.
rbnQosIfRLClassExceedOctets rbnQosIntfRLClassStatsEntry 9 1.3.6.1.4.1.2352.2.22.1.4.1.9 | Counter64 | 0..18446744073709551615 | The number of octets that exceed the rate limit set on the interface for which class counters are enabled.
rbnQosIfRLClassExceedPkts rbnQosIntfRLClassStatsEntry 10 1.3.6.1.4.1.2352.2.22.1.4.1.10 | Counter64 | 0..18446744073709551615 | The number of packets that exceed the rate limit set on the interface.
rbnQosIfRLClassExceedDroppedOctets rbnQosIntfRLClassStatsEntry 11 1.3.6.1.4.1.2352.2.22.1.4.1.11 | Counter64 | 0..18446744073709551615 | The number of octets dropped due to the application of an exceed action on packets that exceed the rate limit set on the interface for which class counters are enabled.
rbnQosIfRLClassExceedDroppedPkts rbnQosIntfRLClassStatsEntry 12 1.3.6.1.4.1.2352.2.22.1.4.1.12 | Counter64 | 0..18446744073709551615 | The number of packets dropped due to the application of an exceed action on packets that exceed the rate limit set on the interface for which class counters are enabled.
rbnQosIfRLClassViolateOctets rbnQosIntfRLClassStatsEntry 13 1.3.6.1.4.1.2352.2.22.1.4.1.13 | Counter64 | 0..18446744073709551615 | The number of octets that violate the normal and maximum burst sizes on the interface for which class counters are enabled.
rbnQosIfRLClassViolatePkts rbnQosIntfRLClassStatsEntry 14 1.3.6.1.4.1.2352.2.22.1.4.1.14 | Counter64 | 0..18446744073709551615 | The number of packets that violate the normal and maximum burst sizes on the interface for which class counters are enabled.
rbnQosIfRLClassViolateDroppedOctets rbnQosIntfRLClassStatsEntry 15 1.3.6.1.4.1.2352.2.22.1.4.1.15 | Counter64 | 0..18446744073709551615 | The number of octets dropped due to the application of a violate action on packets that violate the normal and maximum burst sizes on the interface for which class counters are enabled.
rbnQosIfRLClassViolateDroppedPkts rbnQosIntfRLClassStatsEntry 16 1.3.6.1.4.1.2352.2.22.1.4.1.16 | Counter64 | 0..18446744073709551615 | The number of packets dropped due to the application of a violate action on packets that violate the normal and maximum burst sizes on the interface for which class counters are enabled.

### 1.34.5 rbnQosSubscriberRLClassStatsTable

This table specifies per-class statistical information on the subscriber circuits. It contains the class octet counts for each active subscriber session to which the class-based policing and metering policy is applied when the counters are enabled for the class.

All MIB objects defined in the table are viewed within the context identified in the SNMP protocol (that is, the community string in SNMPv1 or SNMPv2 or the contextName in SNMPv3)

`Index:` rbnSubsActiveName, rbnSubsActiveSessionId, rbnQosSubsRLPolicyType, rbnQosSubsRLClassId

Table 97 describes the objects in rbnQosSubscriberRLClassStatsTable.

Table 97 Objects in rbnQosSubscriberRLClassStatsTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnQosSubsRLPolicyType rbnQosSubscriberRLClassStatsEntry 1 1.3.6.1.4.1.2352.2.22.1.5.1.1 | RbnQosPolicyType Integer | 1—policing 2—metering | The type of the rate-limit policy which is applied to the circuit. policing (1): Indicates inbound policing is applied. metering (2): Indicates outbound policy is applied.
rbnQosSubsRLClassId rbnQosSubscriberRLClassStatsEntry 2 1.3.6.1.4.1.2352.2.22.1.5.1.2 | RbnQosClassId Unsigned32 | 1..8 | A value that uniquely identifies a class defined in the rate-limit policy access list.
rbnQosSubsRLPolicyName rbnQosSubscriberRLClassStatsEntry 3 1.3.6.1.4.1.2352.2.22.1.5.1.3 | SnmpAdminString | 1..39 | Name of the rate-limit policy.
rbnQosSubsRLClassName rbnQosSubscriberRLClassStatsEntry 4 1.3.6.1.4.1.2352.2.22.1.5.1.4 | SnmpAdminString | 1..39 | Name of the class in the rate-limit policy access list.
rbnQosSubsRLClassConformOctets rbnQosSubscriberRLClassStatsEntry 5 1.3.6.1.4.1.2352.2.22.1.5.1.5 | Counter64 | 0..18446744073709551615 | The number of octets that conform to the rate limit set on the subscriber circuit.
rbnQosSubsRLClassConformPkts rbnQosSubscriberRLClassStatsEntry 6 1.3.6.1.4.1.2352.2.22.1.5.1.6 | Counter64 | 0..18446744073709551615 | The number of packets that conform to the rate limit set on the subscriber circuit.
rbnQosSubsRLClassConformDroppedOctets rbnQosSubscriberRLClassStatsEntry 7 1.3.6.1.4.1.2352.2.22.1.5.1.7 | Counter64 | 0..18446744073709551615 | The number of octets dropped due to the application of a conform action on packets that conform to the rate limit set on the subscriber circuit.
rbnQosSubsRLClassConformDroppedPkts rbnQosSubscriberRLClassStatsEntry 8 1.3.6.1.4.1.2352.2.22.1.5.1.8 | Counter64 | 0..18446744073709551615 | The number of packets dropped due to the application of a conform action on packets that conform to the rate limit set on the subscriber circuit.
rbnQosSubsRLClassExceedOctets rbnQosSubscriberRLClassStatsEntry 9 1.3.6.1.4.1.2352.2.22.1.5.1.9 | Counter64 | 0..18446744073709551615 | The number of octets that exceed the rate limit set on the subscriber circuit.
rbnQosSubsRLClassExceedPkts rbnQosSubscriberRLClassStatsEntry 10 1.3.6.1.4.1.2352.2.22.1.5.1.10 | Counter64 | 0..18446744073709551615 | The number of packets that exceed the rate limit set on the subscriber circuit.
rbnQosSubsRLClassExceedDroppedOctets rbnQosSubscriberRLClassStatsEntry 11 1.3.6.1.4.1.2352.2.22.1.5.1.11 | Counter64 | 0..18446744073709551615 | The number of octets dropped due to the application of an exceed action on packets that exceed the rate limit set on the subscriber circuit.
rbnQosSubsRLClassExceedDroppedPkts rbnQosSubscriberRLClassStatsEntry 12 1.3.6.1.4.1.2352.2.22.1.5.1.12 | Counter64 | 0..18446744073709551615 | The number of packets dropped due to the application of an exceed action on packets that exceed the rate limit set on the subscriber circuit.
rbnQosSubsRLClassViolateOctets rbnQosSubscriberRLClassStatsEntry 13 1.3.6.1.4.1.2352.2.22.1.5.1.13 | Counter64 | 0..18446744073709551615 | The number of octets that violate the normal and maximum burst sizes on the subscriber circuit.
rbnQosSubsRLClassViolatePkts rbnQosSubscriberRLClassStatsEntry 14 1.3.6.1.4.1.2352.2.22.1.5.1.14 | Counter64 | 0..18446744073709551615 | The number of packets that violate the normal and maximum burst sizes on the subscriber circuit.
rbnQosSubsRLClassViolateDroppedOctets rbnQosSubscriberRLClassStatsEntry 15 1.3.6.1.4.1.2352.2.22.1.5.1.15 | Counter64 | 0..18446744073709551615 | The number of octets dropped due to the application of a violate action on packets that violate the normal and maximum burst sizes on the subscriber circuit.
rbnQosSubsRLClassViolateDroppedPkts rbnQosSubscriberRLClassStatsEntry 16 1.3.6.1.4.1.2352.2.22.1.5.1.16 | Counter64 | 0..18446744073709551615 | The number of packets dropped due to the application of a violate action on packets that violate the normal and maximum burst sizes on the subscriber circuit.

### 1.34.6 rbnQosHierarchicalPolicyStatsTable

This table lists the drop counters for child circuits of hierarchical QOS policies applied to the child.

`Index:` ifIndex, rbnQosHierarchicalPolicyType

Table 98 describes the objects in rbnQosHierarchicalPolicyStatsTable.

Table 98 Objects in rbnQosHierarchicalPolicyStatsTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnQosHierarchicalPolicyType rbnQosHierarchicalPolicyStatsEntry 1 1.3.6.1.4.1.2352.2.22.1.6.1.1 | RbnQosPolicyType Integer | 1—policing 2—metering | The type of the hierarchical parent rate-limit policy which is applied to the child circuit. policing (1): Indicates inbound policing is applied. metering (2): Indicates outbound policy is applied.
rbnQosHierarchicalPolicyName rbnQosHierarchicalPolicyStatsEntry 2 1.3.6.1.4.1.2352.2.22.1.6.1.2 | SnmpAdminString | 1..39 | Name of the hierarchical parent policy applied to the child circuit.
rbnQosHierarchicalPolicyDroppedOctets rbnQosHierarchicalPolicyStatsEntry 3 1.3.6.1.4.1.2352.2.22.1.6.1.3 | Counter64 | 0..18446744073709551615 | The number of octets dropped due to the hierarchical parent's policy applied to the child circuit.
rbnQosHierarchicalPolicyDroppedPkts rbnQosHierarchicalPolicyStatsEntry 4 1.3.6.1.4.1.2352.2.22.1.6.1.4 | Counter64 | 0..18446744073709551615 | The number of packets dropped due to the hierarchical parent's policy applied to the child circuit.

### 1.34.7 rbnQosHierarchicalPClassStatsTable

This table lists the drop counters for child circuits of hierarchical QOS policy classes applied to the child.

`Index:` ifIndex, rbnQosHierarchicalPolicyType, rbnQosHierarchicalPClassId

Table 99 describes the objects in rbnQosHierarchicalPClassStatsTable.

Table 99 Objects in rbnQosHierarchicalPClassStatsTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnQosHierarchicalPClassId rbnQosHierarchicalPClassStatsEntry 1 1.3.6.1.4.1.2352.2.22.1.7.1.1 | RbnQosClassId Unsigned32 | 1..8 | The class id of the hierarchical parent policy class which is applied to the child circuit.
rbnQosHierarchicalPClassName rbnQosHierarchicalPClassStatsEntry 2 1.3.6.1.4.1.2352.2.22.1.7.1.2 | SnmpAdminString | 1..39 | Name of the hierarchical parent policy class that is applied to the child circuit.
rbnQosHierarchicalPClassDroppedOctets rbnQosHierarchicalPClassStatsEntry 3 1.3.6.1.4.1.2352.2.22.1.7.1.3 | Counter64 | 0..18446744073709551615 | The number of octets dropped due to the hierarchical parent's policy class applied to the child circuit.
rbnQosHierarchicalPClassDroppedPkts rbnQosHierarchicalPClassStatsEntry 4 1.3.6.1.4.1.2352.2.22.1.7.1.4 | Counter64 | 0..18446744073709551615 | The number of packets dropped due to the hierarchical parent's policy class applied to the child circuit.

## 1.35 RBN-RADIUS-MIB

Defines additional objects and notifications for managing the Remote Authentication Dial-In User Service (RADIUS) authentication and accounting servers in use by the SmartEdge router.

The following sections describe objects in RBN-RADIUS-MIB.

### 1.35.1 RADIUS Authorization Objects

Table 100 describes the RADIUS authorization objects in RBN-RADIUS-MIB.

Table 100 RADIUS Authorization Objects
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnRadiusAuthPktTimeout rbnRadiusAuthObjects 1 1.3.6.1.4.1.2352.2.32.1.1.1 | Unsigned32 | 1..2147483647 | The maximum amount of time to wait for a response from a RADIUS authorization server before assuming the packet was lost.
rbnRadiusAuthSrvTimeout rbnRadiusAuthObjects 2 1.3.6.1.4.1.2352.2.32.1.1.2 | Unsigned32 | 0..2147483647 | The maximum amount of time to wait for any response from a RADIUS authorization server before assuming the server is unreachable. A value of '0' indicates that there is no timeout value. In this case, a server is considered to be unreachable when no response is received within the rbnRadiusAuthPktTimeout object window.
rbnRadiusAuthDeadtime rbnRadiusAuthObjects 3 1.3.6.1.4.1.2352.2.32.1.1.3 | Unsigned32 | 0..65535 | After a RADIUS authorization server has been transitioned to 'down,' it is assumed to be unreachable for this interval. After that point, the system can start sending requests to the server again. A value of '0' indicates the system can start sending requests to the server immediately.
rbnRadiusAuthTries rbnRadiusAuthObjects 4 1.3.6.1.4.1.2352.2.32.1.1.4 | Unsigned32 | 1..2147483647 | The number of times the system attempts to transmit an authorization request to a RADIUS server. If multiple RADIUS authorization servers have been configured, retransmissions cycle through the other servers before being retransmitted to the server that originally failed to respond.
rbnRadiusAuthStripDomain rbnRadiusAuthObjects 6 1.3.6.1.4.1.2352.2.32.1.1.6 | TruthValue Integer | 1—true 2—false | If this object is false, the entire username, including the domain name, is sent to the RADIUS server. If true, the domain portion of a structured username is stripped before relaying a request to a RADIUS server.

### 1.35.2 RADIUS Accounting Objects

Table 101 describes the RADIUS accounting objects for RBN-RADIUS-MIB.

Table 101 RADIUS Accounting Objects
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnRadiusAcctPktTimeout rbnRadiusAcctObjects 1 1.3.6.1.4.1.2352.2.32.1.2.1 | Unsigned32 | 1..2147483647 | The maximum amount of time to wait for a response from a RADIUS accounting server before assuming the packet was lost. Note: If the system is using a RADIUS server for both authorization and accounting, this object's value is ignored for that server. Instead, the value of the rbnRadiusAuthPktTimeout object is used for all requests going to that server.
rbnRadiusAcctSrvTimeout rbnRadiusAcctObjects 2 1.3.6.1.4.1.2352.2.32.1.2.2 | Unsigned32 | 0..2147483647 | The maximum amount of time to wait for any response from a RADIUS accounting server before assuming the server is unreachable. A value of '0' indicates that there is no timeout value. In this case, a server is considered to be unreachable when no response is received within the rbnRadiusAcctPktTimeout object window. Note: If the system is using a RADIUS server for both authorization and accounting, this object's value is ignored for that server. Instead the value of the rbnRadiusAuthSrvTimeout object will be used for that server.
rbnRadiusAcctDeadtime rbnRadiusAcctObjects 3 1.3.6.1.4.1.2352.2.32.1.2.3 | Unsigned32 | 0..65535 | After a RADIUS accounting server has been transitioned to 'down,' it is assumed to be unreachable for this interval. After that point, the system can start sending accounting records to the server again. A value of zero indicates the system can start sending records to the server immediately. If the system is using a RADIUS server for both authorization and accounting, this object's value is ignored for that server. Instead, the value of the rbnRadiusAuthDeadtime object is used for that server.
rbnRadiusAcctTries rbnRadiusAcctObjects 4 1.3.6.1.4.1.2352.2.32.1.2.4 | Unsigned32 | 1..2147483647 | The number of times the system attempts to transmit an accounting record to a RADIUS server. If multiple RADIUS accounting servers have been configured, retransmissions cycle through the other servers before being retransmitted to the server that originally failed to respond. If the system is using a RADIUS server for both authorization and accounting, this object's value is ignored for that server. Instead, the value of the rbnRadiusAuthTries object is used for that server.
rbnRadiusAcctStripDomain rbnRadiusAcctObjects 6 1.3.6.1.4.1.2352.2.32.1.2.6 | TruthValue Integer | 1—true 2—false | If this object is false, the entire username, including the domain name, is sent to the RADIUS server. If true, the domain portion of a structured username is stripped before relaying a request to a RADIUS server.

### 1.35.3 RADIUS Notification Objects

Table 102 describes the RADIUS notification objects for RBN-RADIUS-MIB. All objects in the table are accessible-for-notify.

Table 102 RADIUS Notification Objects
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnRadiusClientPort rbnRadiusNotifyObjects 1 1.3.6.1.4.1.2352.2.32.1.3.1 | Unsigned32 | 1024..65535 | A system can be configured to use a range of source TCP/IP ports when sending requests to a RADIUS server. When a server transitions to up or down and a state-change notification is generated, an instance of this object is included to indicate which source port was used when the server changed state.
rbnRadiusContext rbnRadiusNotifyObjects 2 1.3.6.1.4.1.2352.2.32.1.3.2 | SnmpAdminString | 1..63 | The name of the context in which this server is configured.
rbnRadiusReason rbnRadiusNotifyObjects 3 1.3.6.1.4.1.2352.2.32.1.3.3 | RbnRadiusServerReason Integer | 1—responding 2—packetTimeout 3—serverTimeout 4—portDown | The reason for the last state change of the server.
rbnRadiusUsername rbnRadiusNotifyObjects 4 1.3.6.1.4.1.2352.2.32.1.3.4 | SnmpAdminString | 0..128 | The name of the user the system was trying to authenticate or send accounting information for when the RADIUS server transitioned to 'down'. NOTE: The 'username' is only valid when transitioning due to a packet-level timeout. When transitioning due to any other reason, the value for this object is a string of zero (0) length.

### 1.35.4 rbnRadiusAuthSrvTable

This table augments the radiusAuthServerTable. All entries that exist in that table have a corresponding entry in this table.

`Index`: radiusAuthServerIndex

Table 103 describes the objects in rbnRadiusAuthSrvTable.

Table 103 Objects in rbnRadiusAuthSrvTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnRadiusAuthSrvState rbnRadiusAuthSrvEntry 1 1.3.6.1.4.1.2352.2.32.1.1.5.1.1 | RbnRadiusServerState Integer | 1—unknown 2—up 3—down | The current state of the RADIUS server.
rbnRadiusAuthSrvLastChange rbnRadiusAuthSrvEntry 2 1.3.6.1.4.1.2352.2.32.1.1.5.1.2 | TimeStamp TimeTicks | 0..4294967295 | The value of sysUpTime when this server last changed state. If rbnRadiusAuthSrvState is 'unknown,' this is effectively the value of the sysUpTime object when this server was initially configured.
rbnRadiusAuthSrvCounterResetTime rbnRadiusAuthSrvEntry 3 1.3.6.1.4.1.2352.2.32.1.1.5.1.3 | TimeStamp TimeTicks | 0..4294967295 | The value of sysUpTime on the most recent occasion when any of the counters for this RADIUS server experienced a discontinuity. This includes counters in this table as well as those in the radiusAuthServerTable object.
rbnRadiusAuthSrvSendErrors rbnRadiusAuthSrvEntry 4 1.3.6.1.4.1.2352.2.32.1.1.5.1.4 | Counter32 | 0..4294967295 | The number of packets destined to this RADIUS server that could not be transmitted due to an error. Discontinuities in the value of this counter are indicated by the value of the rbnRadiusAuthSrvCounterResetTime object.

### 1.35.5 rbnRadiusAcctSrvTable

This table augments the radiusAccServerTable. All entries that exist in that table have a corresponding entry in this table.

`Index`: radiusAccServerIndex

Table 104 describes the objects in rbnRadiusAcctSrvTable.

Table 104 Objects in rbnRadiusAcctSrvTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnRadiusAcctSrvState rbnRadiusAcctSrvEntry 1 1.3.6.1.4.1.2352.2.32.1.2.5.1.1 | RbnRadiusServerState Integer | 1—unknown 2—up 3—down | The current state of the RADIUS server.
rbnRadiusAcctSrvLastChange rbnRadiusAcctSrvEntry 2 1.3.6.1.4.1.2352.2.32.1.2.5.1.2 | TimeStamp TimeTicks | 0..4294967295 | The value of the sysUpTime object when this server last changed state. If the rbnRadiusAcctSrvState object is 'unknown,‘ this is effectively the value of the sysUpTime object when this server was initially configured.
rbnRadiusAcctSrvCounterResetTime rbnRadiusAcctSrvEntry 3 1.3.6.1.4.1.2352.2.32.1.2.5.1.3 | TimeStamp TimeTicks | 0..4294967295 | The value of the sysUpTime object on the most recent occasion when any of the counters for this RADIUS server experienced a discontinuity. Note: This value includes counters in this table as well as those in the radiusAccServerTable object.
rbnRadiusAcctSrvSendErrors rbnRadiusAcctSrvEntry 4 1.3.6.1.4.1.2352.2.32.1.2.5.1.4 | Counter32 | 0..4294967295 | The number of packets destined to this RADIUS server which could not be transmitted due to an error. Discontinuities in the value of this counter are indicated by the value of the rbnRadiusAcctSrvCounterResetTime object.

## 1.36 RBN-SFP-MIB

Defines objects for managing the Small Form-Factor Pluggable (SFP) transceivers.

### 1.36.1 rbnSfpAlarmActiveTable

This table contains the SFP alarms currently active on the SFP.

`Index:` rbnSfpActiveAlarmIndex

Table 105 describes the objects in rbnSfpAlarmActiveTable.

Table 105 Objects in rbnStackedVlanAggrStatsTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnSfpActiveAlarmIndex rbnSfpAlarmActiveEntry 1 1.3.6.1.4.1.2352.2.49.1.1.1.1 | Unsigned32 | 1..4294967295 | A monotonically increasing integer index. It wraps back to 1 after it reaches its maximum value.
rbnSfpAlarmCardSlot rbnSfpAlarmActiveEntry 2 1.3.6.1.4.1.2352.2.49.1.1.1.2 | RbnSlot Unsigned32 | 0..255 | The chassis slot number in which the card is present where the SFP plugged in.
rbnSfpAlarmPort rbnSfpAlarmActiveEntry 3 1.3.6.1.4.1.2352.2.49.1.1.1.3 | RbnSlot Unsigned32 | 0..255 | The port number where the SFP plugged in.
rbnSfpAlarmId rbnSfpAlarmActiveEntry 4 1.3.6.1.4.1.2352.2.49.1.1.1.4 | RbnAlarmId | Integer | An identifier for the alarm. See Section 1.43.1 RbnAlarmId for details.
rbnSfpAlarmSeverity rbnSfpAlarmActiveEntry 5 1.3.6.1.4.1.2352.2.49.1.1.1.5 | ItuPerceivedSeverity | Integer | The current severity of the alarm. See Section 1.43.6 ItuPerceivedSeverity for details.
rbnSfpAlarmType rbnSfpAlarmActiveEntry 6 1.3.6.1.4.1.2352.2.49.1.1.1.6 | IANAItuEventType | Integer | The type of alarm. See Section 1.43.5 IANAItuEventType for details.
rbnSfpAlarmDateAndTime rbnSfpAlarmActiveEntry 7 1.3.6.1.4.1.2352.2.49.1.1.1.7 | DateAndTime Octet String | SIZE (8) | The local date and time when the alarm was raised
rbnSfpAlarmDescription rbnSfpAlarmActiveEntry 8 1.3.6.1.4.1.2352.2.49.1.1.1.8 | SnmpAdminString Octet String | 0..64 | A text string which conveys additional information about the alarm.
rbnSfpAlarmProbableCause rbnSfpAlarmActiveEntry 9 1.3.6.1.4.1.2352.2.49.1.1.1.9 | IANAItuProbableCause | Integer | The probable cause for this alarm. See Section 1.43.4 IANAItuProbableCause for details.
rbnSfpAlarmServiceAffecting rbnSfpAlarmActiveEntry 10 1.3.6.1.4.1.2352.2.49.1.1.1.10 | Integer | 1—yes 2—no | Indicates whether the alarm is perceived to be service impacting.

## 1.37 RBN-SSE-MIB

Defines objects necessary to support the management of SmartEdge Storage Engine (SSE) file server groups, partitions and corresponding alarms.

### 1.37.1 rbnFSGroupTable

This table provides details for a file-server group, which is a logical abstraction of a physical file server. This table lists the file server groups that have been configured on the system.

`Index:` rbnFSGroupName

Table 106 describes the objects in rbnFSGroupTable.

Table 106 Objects in rbnFSGroupTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnFSGroupName rbnFSGroupEntry 1 1.3.6.1.4.1.2352.2.48.1.1.1.1 | SnmpAdminString | 1..16 | A textual name for the File Server Group.
rbnFSGroupState rbnFSGroupEntry 2 1.3.6.1.4.1.2352.2.48.1.1.1.2 | Integer | 0—unknown 1—up 2—down 3—partial 4—stale 5— noCard 6—unassigned | Service state of the File Server Group.
rbnFSGroupMode rbnFSGroupEntry 3 1.3.6.1.4.1.2352.2.48.1.1.1.3 | Integer | 1—diskRedundancy 2— networkRedundancy 3—nonRedundant | The operational mode. DiskRedundancy is where each hard disk on a single file-server card mirrors the other and when one fails the other takes over automatically. NetworkRedundancy is a one file-server mirroring the other in the same chassis. One of the file-servers will be in active state while the other is standby or backup. NonRedundant is when one or two hard disks serve as a generic disk.
rbnFSGroupRaidMode rbnFSGroupEntry 4 1.3.6.1.4.1.2352.2.48.1.1.1.4 | Integer | 0—unknown 1—raid0 2—raid1 3—independent | Operational mode of the disks. The option RAID0 is where the operational mode must use 2 disks. RAID1 implies using 2 disks, although 1 could be un-plugged. Independent (standalone) is either 1 or 2 disks.
rbnFSGroupRevert rbnFSGroupEntry 5 1.3.6.1.4.1.2352.2.48.1.1.1.5 | TruthValue Integer | 1—true 2—false | The reverting mode of the File Server Group. Revert back to original primary/secondary relationship if in reverted mode (that is this object has the value true(1)).
rbnFSPrimarySlot rbnFSGroupEntry 6 1.3.6.1.4.1.2352.2.48.1.1.1.6 | RbnSlot Unsigned32 | 0..255 | The chassis slot number in which the primary SSE card is present.
rbnFSSecondarySlot rbnFSGroupEntry 7 1.3.6.1.4.1.2352.2.48.1.1.1.7 | RbnSlot Unsigned32 | 0..255 | The chassis slot number in which the secondary SSE card is present.
rbnFSActiveSlot rbnFSGroupEntry 8 1.3.6.1.4.1.2352.2.48.1.1.1.8 | RbnSlot Unsigned32 | 0..255 | The slot number in which the active SSE card is present.

### 1.37.2 rbnFSPartitionTable

This table lists the partitions that have been 212 configured on the system.

`Index:` rbnFSGroupName, rbnFSPartitionName

Table 107 describes the objects in rbnFSPartitionTable.

Table 107 Objects in rbnFSPartitionTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnFSPartitionName rbnFSPartitionEntry 1 1.3.6.1.4.1.2352.2.48.1.2.1.1 | SnmpAdminString | 1..16 | A textual name for the Partition.
rbnFSPartitionState rbnFSPartitionEntry 2 1.3.6.1.4.1.2352.2.48.1.2.1.2 | Integer | 1—up 2—down 3—stale | Operational status of the partition.
rbnFSPartitionSize rbnFSPartitionEntry 3 1.3.6.1.4.1.2352.2.48.1.2.1.3 | Unsigned32 | 1..4294967295 | Size of the partition in GBytes.
rbnFSPartitionDisk rbnFSPartitionEntry 4 1.3.6.1.4.1.2352.2.48.1.2.1.4 | Unsigned32 | 1..10 | Disk ID of the disk (disk num) where the partition is located. For SSE, 0 for DISK_1, 1 for DISK_2 and 2 for DISK_ALL will be used.
rbnFSPartitionMirrored rbnFSPartitionEntry 5 1.3.6.1.4.1.2352.2.48.1.2.1.5 | Integer | 1—enabled 2—disabled 3—notApplicable | Mirror data to standby disk, if network redundancy is configured.
rbnFSPartitionRaiseTriggerPercentage rbnFSPartitionEntry 6 1.3.6.1.4.1.2352.2.48.1.2.1.6 | RbnPercentage | 50..100 | Partition capacity used in percentage to trigger alarm. Raise percentage of 100 indicates alarm is triggered when the partition is completely full. The default value is 80.
rbnFSPartitionClearTriggerPercentage rbnFSPartitionEntry 7 1.3.6.1.4.1.2352.2.48.1.2.1.7 | RbnPercentage | 10..100 | Specifies the capacity percentage for when the alarm is cleared. Clear percentage of 10 indicates alarm is triggered when partition is at 10% below raise percentage. The default value is 70.

### 1.37.3 RBN-SSE-MIB Objects

Table 109 the general objects for RBN-SSE-MIB.

Table 108 RBN-SSE-MIB Objects
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnSseAlarmDateAndTime rbnSseMIBObjects 3 1.3.6.1.4.1.2352.2.48.1.3 | DateAndTime Octet String | SIZE (8) | The local date and time when the alarm was raised
rbnSseAlarmSeverity rbnSseMIBObjects 4 1.3.6.1.4.1.2352.2.48.1.4 | ItuPerceivedSeverity | Integer | The current severity of the alarm. See Section 1.43.6 ItuPerceivedSeverity for details.
rbnSseAlarmProbableCause rbnSseMIBObjects 5 1.3.6.1.4.1.2352.2.48.1.5 | IANAItuProbableCause | Integer | The probable cause for this alarm. See Section 1.43.4 IANAItuProbableCause for details.
rbnSseEventType rbnSseMIBObjects 6 1.3.6.1.4.1.2352.2.48.1.6 | IANAItuEventType | Integer | The type of alarm. See Section 1.43.5 IANAItuEventType for details.
rbnSseAlarmDescription rbnSseMIBObjects 7 1.3.6.1.4.1.2352.2.48.1.7 | SnmpAdminString | 0..64 | A text string which conveys additional information about the alarm.

## 1.38 RBN-STACKEDVLAN-MIB

Defines objects for managing the interfaces in the stacked VLAN.

### 1.38.1 rbnStackedVlanAggrStatsTable

This table contains aggregated statistics of inner VLAN related to an outer VLAN.

`Index:` rbnStackedVlanIndex

Table 109 describes the objects in rbnStackedVlanAggrStatsTable.

Table 109 Objects in rbnStackedVlanAggrStatsTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnStackedVlanIndex rbnStackedVlanAggrStatsEntry 2 1.3.6.1.4.1.2352.2.40.1.1.1.2 | InterfaceIndex Integer32 | 1..2147483647 | An index value that uniquely identifies an interface to an ethernet-like medium. The interface identified by a particular value of this index is the same interface as identified by the same value of ifIndex.
rbnStackedVlanHCInOctets rbnStackedVlanAggrStatsEntry 2 1.3.6.1.4.1.2352.2.40.1.1.1.2 | Counter64 | 0..18446744073709551615 | The aggregate of the total number of octets received on each outer VLAN and its inner VLANs, including framing characters.
rbnStackedVlanHCInUcastPkts rbnStackedVlanAggrStatsEntry 3 1.3.6.1.4.1.2352.2.40.1.1.1.3 | Counter64 | 0..18446744073709551615 | The aggregate of the number of packets, delivered by this sublayer to a higher layer or sublayer, which were not addressed to a multicast or broadcast address at this sublayer for each outer VLAN and its inner VLANs.
rbnStackedVlanHCInMulticastPkts rbnStackedVlanAggrStatsEntry 4 1.3.6.1.4.1.2352.2.40.1.1.1.4 | Counter64 | 0..18446744073709551615 | The aggregate number of packets, delivered by this sublayer to a higher layer or sublayer, that were addressed to a multicast address at this sublayer for each outer VLAN and its inner VLANs. For a MAC layer protocol, this includes both Group and Functional addresses.
rbnStackedVlanHCInBroadcastPkts rbnStackedVlanAggrStatsEntry 5 1.3.6.1.4.1.2352.2.40.1.1.1.5 | Counter64 | 0..18446744073709551615 | The aggregate number of packets, delivered by this sublayer to a higher layer or sublayer, that were addressed to a broadcast address at this sublayer for each outer VLAN and its inner VLANs.
rbnStackedVlanHCOutOctets rbnStackedVlanAggrStatsEntry 6 1.3.6.1.4.1.2352.2.40.1.1.1.6 | Counter64 | 0..18446744073709551615 | The aggregate of the total number of octets transmitted out of the interface, including framing characters for each outer VLAN and its inner VLANs.
rbnStackedVlanHCOutUcastPkts rbnStackedVlanAggrStatsEntry 7 1.3.6.1.4.1.2352.2.40.1.1.1.7 | Counter64 | 0..18446744073709551615 | The aggregate of the total number of packets that higher-level protocols requested be transmitted, and that were not addressed to a multicast or broadcast address at this sublayer, including those that were discarded or not sent for each outer VLAN and its inner VLANs.
rbnStackedVlanHCOutMulticastPkts rbnStackedVlanAggrStatsEntry 8 1.3.6.1.4.1.2352.2.40.1.1.1.8 | Counter64 | 0..18446744073709551615 | The aggregate of the total number of packets that higher-level protocols requested be transmitted, and that were addressed to a multicast address at this sublayer, including those that were discarded or not sent for each outer VLAN and its inner VLANs. For a MAC layer protocol, this includes both Group and Functional addresses.
rbnStackedVlanHCOutBroadcastPkts rbnStackedVlanAggrStatsEntry 9 1.3.6.1.4.1.2352.2.40.1.1.1.9 | Counter64 | 0..18446744073709551615 | The aggregate of the total number of packets that higher-level protocols requested be transmitted, and that were addressed to a broadcast address at this sublayer, including those that were discarded or not sent for each outer VLAN and its inner VLANs.

## 1.39 RBN-SUBSCRIBER-ACTIVE-MIB

Defines the objects for monitoring active subscribers in the SmartEdge product family. Related commands include the `subscriber` and `show subscriber` commands.

The following sections contain object information for RBN-SUBSCRIBER-ACTIVE-MIB.

### 1.39.1 Subscriber Licensing Objects

Table 110 describes the subscriber licensing objects in RBN-SUBSCRIBER-ACTIVE-MIB.

Table 110 Subscriber Licensing
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnSubsMaxSupportedSessions rbnSubsLicense 1 11.3.6.1.4.1.2352.2.27.1.2.5.1 | Gauge32 | 0..4294967295 | The maximum number of active subscriber sessions on the SmartEdge router.
rbnSubsLicensedSessions rbnSubsLicense 2 21.3.6.1.4.1.2352.2.27.1.2.5.2 | Gauge32 | 0..4294967295 | The number of licensed subscriber sessions on the SmartEdge router.
rbnSubsActiveSessions rbnSubsLicense 3 31.3.6.1.4.1.2352.2.27.1.2.5.3 | Gauge32 | 0..4294967295 | The number of active subscriber sessions on the SmartEdge router.
rbnSubsCapacityPercentageUsed rbnSubsLicense 4 41.3.6.1.4.1.2352.2.27.1.2.5.4 | RbnPercentage Integer32 | 0..100 | The percentage of licensed subscriber sessions out of all active sessions in use on the SmartEdge router.

### 1.39.2 Clear Subscriber Objects

Table 111 describes the clear subscribers objects in RBN-SUBSCRIBER-ACTIVE-MIB.

Table 111 Clearing Subscribers
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnSubsClearSubscriberName rbnSubsClear 1 1.3.6.1.4.1.2352.2.27.1.1.3.1 | SnmpAdminString | 1..80 | Setting this object to the subscriber name clears all sessions associated with the subscriber. In the case of a PPP circuit, the SmartEdge OS attempts to renegotiate and reauthenticate a new session with the remote peer on the circuit. In the case of RFC 1483 and RFC 1490 encapsulated circuits the circuit is brought down and then back up and an attempt is made to reauthenticate the subscriber bound to the circuit. This object returns a string of zero (0) length when queried.
rbnSubsClearSessionId rbnSubsClear 2 1.3.6.1.4.1.2352.2.27.1.1.3.2 | SnmpAdminString | 0..32 | Clears the subscriber session identified by this value. In the case of a PPP circuit, the SmartEdge OS attempts to renegotiate and reauthenticate a new session with the remote peer on the circuit. In the case of RFC 1483 and RFC 1490 encapsulated circuits the circuit is brought down and then back up and an attempt is made to reauthenticate the subscriber bound to the circuit. This object returns a string of zero (0) length when queried.

### 1.39.3 Bounce Objects

Table 112 describes the bounce objects in RBN-SUBSCRIBER-ACTIVE-MIB. Bounce objects remove a subscriber session and reauthorize or reset the session. For example, you can use these objects to reauthorize a subscriber during a subscription change. The objects in the table are read-write.

Table 112 Bounce Objects
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnSubsBounceName rbnSubsClear 3 1.3.6.1.4.1.2352.2.27.1.1.3.3 | SnmpAdminString | 0..80 | Each circuit using CLIPS encapsulation used by the named subscriber is brought down and immediately recreated using the RADIUS Access Accept attributes. Any other circuit encapsulation type is cleared. This object returns a string of zero (0) length when queried.
rbnSubsBounceSessionId rbnSubsClear 4 1.3.6.1.4.1.2352.2.27.1.1.3.4 | SnmpAdminString | 0..32 | The circuit using CLIPS encapsulation identified by the RADIUS Acct-Session-Id is brought down and immediately recreated using the RADIUS Access-Accept attributes. Any other circuit encapsulation type is cleared. This object returns a string of zero (0) length when queried.

### 1.39.4 Reauthorization Objects

Table 113 describes the reauthorization objects in RBN-SUBSCRIBER-ACTIVE-MIB. All objects in the table are read-write.

Table 113 Reauthorization Objects
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnSubsReauthName rbnSubsClear 7 1.3.6.1.4.1.2352.2.27.1.1.3.7 | SnmpAdminString | 0..80 | Reauthorize all of the active sessions associated with the given subscriber in the context identified in the SNMP protocol (the community string in SNMPv1 or SNMPv2 or the contextName in SNMPv3). This object returns a string of zero (0) length when queried.
rbnSubsReauthSessionId rbnSubsClear 8 1.3.6.1.4.1.2352.2.27.1.1.3.8 | SnmpAdminString | 0..32 | Reauthorize the active session identified by the value of this object and the context identified in the SNMP protocol (the community string in SNMPv1 or SNMPv2 or the contextName object in SNMPv3). This object returns a string of zero (0) length when queried.
rbnSubsClearReason rbnSubsClear 9 1.3.6.1.4.1.2352.2.27.1.1.3.9 | Unsigned32 | 0..4294967295 | An unsigned integer value that may be included in the set request for the rbnSubsClearSubscriberName object, rbnSubsClearSessionId object, rbnSubsBounceName object, rbnSubsBounceSessionId object, or any other objects defines under the rbnSubsClear OID node. The use of this object value is implementation dependent. This object returns 0 when queried.

### 1.39.5 Notification Object

Table 114 describes the notification object in RBN-SUBSCRIBER-ACTIVE-MIB.

Table 114 Notification Objects
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnSubsNotifyEnable rbnSubsNotify 1 1.3.6.1.4.1.2352.2.27.1.3.1 | TruthValue Integer | 1—true 2—false | Provides a mechanism for enabling and disabling subscriber notifications. A value of true, indicates that subscriber notifications are enabled. A value of false, indicates that subscriber notifications are disabled. This object is read-write.

### 1.39.6 rbnSubsActiveTable

This table contains subscriber sessions that have been authenticated on a circuit.

`Index:`rbnSubsActiveSessionId

Table 115 describes the objects in rbnSubsActiveTable.

Table 115 Objects in rbnSubsActiveTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnSubsActiveName rbnSubsActiveEntry 1 1.3.6.1.4.1.2352.2.27.1.1.1.1.1 | SnmpAdminString | 1..80 | Active subscriber entry name. A subscriber name configured by other means may have been given a length greater than 80. Names which exceed this length are not accessible via SNMP operations.
rbnSubsActiveSessionId rbnSubsActiveEntry 2 1.3.6.1.4.1.2352.2.27.1.1.1.1.2 | SnmpAdminString OctetString | 1..32 | A value that uniquely identifies an active subscriber session. If RADIUS is being used to configure/authenticate subscribers, this value will appear in the RADIUS Acct-Session-Id attribute.
rbnSubsActiveCircuitDescr rbnSubsActiveEntry 3 1.3.6.1.4.1.2352.2.27.1.1.1.1.3 | SnmpAdminString | 1..64 | A string that provides identifying information (such as slot or port) of the circuit the subscriber is using.
rbnSubsActiveCircuitHandle rbnSubsActiveEntry 4 1.3.6.1.4.1.2352.2.27.1.1.1.1.4 | RbnCircuitHandle Octet String | 8 | A value for identifying circuits.
rbnSubsActiveStartTime rbnSubsActiveEntry 5 1.3.6.1.4.1.2352.2.27.1.1.1.1.5 | DateAndTime | SIZE (8) | The time when the subscriber became active.
rbnSubsActiveClear rbnSubsActiveEntry 6 1.3.6.1.4.1.2352.2.27.1.1.1.1.6 | TruthValue Integer | 1—true 2—false | Setting this value to true clears the active subscriber session. In a PPP session, the PPP process attempts to renegotiate and reauthenticate a new session with the remote peer on the circuit. In RFC 1483 encapsulated circuits, the session is brought down and then back up and an attempt is made to reauthenticate the subscriber. An SNMP get operation always returns the value false.
rbnSubsActiveResend rbnSubsActiveEntry 7 1.3.6.1.4.1.2352.2.27.1.1.1.1.7 | TruthValue Integer | 1—true 2—false | Setting this value to true configures the SmartEdge OS to resend the RADIUS acct-start-packet message for services associated with the subscriber session. An SNMP get operation always returns false.
rbnSubsActiveNasPortType rbnSubsActiveEntry 8 1.3.6.1.4.1.2352.2.27.1.1.1.1.8 | Unsigned32 | 0..4294967295 | The RADIUS attribute NAS-Port-Type; type of physical port that is authenticating the user.
rbnSubsActiveMediumType rbnSubsActiveEntry 9 1.3.6.1.4.1.2352.2.27.1.1.1.1.9 | RbnPortMediumType Integer | 0—unknown 11—dsl 12—cable 13—wireless 14—satellite | The medium type of the NAS-Port.
rbnSubsActiveResendSvcAcct rbnSubsActiveEntry 10 1.3.6.1.4.1.2352.2.27.1.1.1.1.10 | TruthValue Integer | 1—true 2—false | Setting this value to true configures the SmartEdge OS to resend the RADIUS acct-start-packet message for services associated with the subscriber session. An SNMP get operation always returns false.

### 1.39.7 rbnSubsActiveSessionTable

This table contains active subscriber sessions which have been authenticated on a circuit.

Index: rbnSubsActiveSessionId

Table 116 describes the objects in rbnSubsActiveSessionTable.

Table 116 Objects in rbnSubsActiveSessionTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnSubsActiveSubscriberName rbnSubsActiveSessionEntry 1 1.3.6.1.4.1.2352.2.27.1.1.6.1.1 | SnmpAdminString | 1..256 | The subscriber name associated with the session.
rbnSubsActiveSessionPointer rbnSubsActiveSessionEntry 2 1.3.6.1.4.1.2352.2.27.1.1.6.1.2 | Object ID | N/A | Pointer to the row in the rbnSubsActiveTable row associated with this subscriber.

### 1.39.8 rbnSubsActiveIpTable

This table contains IP addresses used by active subscribers.

`Index:` rbnSubsActiveName, rbnSubsActiveSessionId, rbnSubsActiveAddrType, rbnSubsActiveAddr

Table 117 describes the objects in rbnSubsActiveIpTable.

Table 117 Objects in rbnSubsActiveIpTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnSubsActiveAddrType rbnSubsActiveIpEntry 1 1.3.6.1.4.1.2352.2.27.1.1.2.1.1 | InetAddressType Integer | 0—unknown 1—ipv4 2—ipv6 3—ipv4z 4—ipv6z 16—dns | The address type of rbnSubsActiveAddr.
rbnSubsActiveAddr rbnSubsActiveIpEntry 2 1.3.6.1.4.1.2352.2.27.1.1.2.1.2 | InetAddress String | 4 | 16 | 20 | The host IP address of the active subscriber.

### 1.39.9 rbnSubsActiveIpAddrTable

This table contains the IPv4 and IPv6 addresses used by active subscribers.

Index: rbnSubsActiveSessionId, rbnSubsActiveIpAddrType, rbnSubsActiveIpAddr, rbnSubsActiveIpPfxLen

Table 118 describes the objects in rbnSubsActiveIpAddrTable.

Table 118 Objects in rbnSubsActiveIpAddrTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnSubsActiveIpAddrType rbnSubsActiveIpAddrEntry 1 1.3.6.1.4.1.2352.2.27.1.1.7.1.1 | InetAddressType Integer | 1—IPv4 2—IPv6 | IP address type for the active subscriber.
rbnSubsActiveIpAddr rbnSubsActiveIpAddrEntry 2 1.3.6.1.4.1.2352.2.27.1.1.7.1.2 | InetAddress | 4 | 16 | Host IP address of the active subscriber.
rbnSubsActiveIpPfxLen rbnSubsActiveIpAddrEntry 3 1.3.6.1.4.1.2352.2.27.1.1.7.1.3 | InetAddressPrefixLength Unsigned32 | 0 ..128 | The prefix length associated with this prefix. For IPv4 active subscriber sessions, the prefix length is always 32.
rbnSubsActiveIpAddrDesc rbnSubsActiveIpAddrEntry 4 1.3.6.1.4.1.2352.2.27.1.1.7.1.4 | SnmpAdminString Octet string | 0 ..255 | Human readable IP address.

### 1.39.10 rbnSubsCntxtCountTable

This table contains counts of active subscribers by context name. Unlike any of the other tables in this MIB module, all rows in this table are accessible when the local context is specified in the SNMP message, unless restricted by entries in vacmAccessTable. SNMP requests that use other contexts return only the row that matches the context.

`Index:` vacmContextName

Table 119 describes the objects in rbnSubsCntxtCountTable.

Table 119 Objects in rbnSubsCntxtCountTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnSubsCntxtCount rbnSubsCntxtCountEntry 1 1.3.6.1.4.1.2352.2.27.1.2.1.1.1 | Gauge32 | 0..4294967295 | The count of active subscribers for the context.
rbnSubsCntxtIp4OnlyCount rbnSubsCntxtCountEntry 2 1.3.6.1.4.1.2352.2.27.1.2.1.1.2 | Gauge32 | 0..4294967295 | The count of active subscribers authorized for IPv4 only, for the current context.
rbnSubsCntxtIp6OnlyCount rbnSubsCntxtCountEntry 3 1.3.6.1.4.1.2352.2.27.1.2.1.1.3 | Gauge32 | 0..4294967295 | The count of active subscribers authorized for IPv6 only, for the current context.
rbnSubsCntxtDualCount rbnSubsCntxtCountEntry 4 1.3.6.1.4.1.2352.2.27.1.2.1.1.4 | Gauge32 | 0..4294967295 | The count of active subscribers authorized for both IPv4 and IPv6, for the current context.
rbnSubsCntxtLacCount rbnSubsCntxtCountEntry 5 1.3.6.1.4.1.2352.2.27.1.2.1.1.5 | Gauge32 | 0..4294967295 | The count of active LAC subscribers for the context.

### 1.39.11 rbnSubsEncapsCountTable

This table contains counts of active subscribers by encapsulation type.

Table 120 describes the objects in rbnSubsEncapsCountTable.

Table 120 Objects in rbnSubsEncapsCountTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnSubsEncapsulationType rbnSubsEncapsCountEntry 1 1.3.6.1.4.1.2352.2.27.1.2.2.1.1 | Integer | 1—ppp 2—pppoe 3—bridged1483 4—routed1483 5—multi1483 6—dot1q1483 7—dot1qEnet 8—bridged1490 9—routed1490 10—multi1490 11—dot1q1490 12—clips 255—other | Encapsulation type the active subscriber is using. PPP includes all types of PPP encapsulations except PPPoE.
rbnSubsEncapsCount rbnSubsEncapsCountEntry 2 1.3.6.1.4.1.2352.2.27.1.2.2.1.2 | Gauge32 | 0..4294967295 | The count of active subscribers for the encapsulation type.

### 1.39.12 rbnSubsStatsTable

This table contains counters for individual circuits.

`Index:` rbnSubsActiveName, rbnSubsActiveSessionId

Table 121 describes the objects in rbnSubsStatsTable.

Table 121 Objects in rbnSubsStatsTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnSubsOctetsSent rbnSubsStatsEntry 1 1.3.6.1.4.1.2352.2.27.1.2.3.1.1 | Counter64 | 0..18446744073709551615 | The number of octets sent by the circuit. This counter includes multicast activity.
rbnSubsOctetsReceived rbnSubsStatsEntry 2 1.3.6.1.4.1.2352.2.27.1.2.3.1.2 | Counter64 | 0..18446744073709551615 | The number of octets received by the circuit. This counter includes multicast activity.
rbnSubsPktsSent rbnSubsStatsEntry 3 1.3.6.1.4.1.2352.2.27.1.2.3.1.3 | Counter64 | 0..18446744073709551615 | The number of packets sent by the circuit. This counter includes multicast activity.
rbnSubsPktsReceived rbnSubsStatsEntry 4 1.3.6.1.4.1.2352.2.27.1.2.3.1.4 | Counter64 | 0..18446744073709551615 | The number of packets received by the circuit. This counter includes multicast activity.
rbnSubsXmitOctetsDropped rbnSubsStatsEntry 5 1.3.6.1.4.1.2352.2.27.1.2.3.1.5 | Counter32 | 0..4294967295 | The number of octets dropped by the circuit before transmission.
rbnSubsXmitPktsDropped rbnSubsStatsEntry 6 1.3.6.1.4.1.2352.2.27.1.2.3.1.6 | Counter32 | 0..4294967295 | The number of packets dropped by the circuit before transmission.
rbnSubsMcastOctetsSent rbnSubsStatsEntry 7 1.3.6.1.4.1.2352.2.27.1.2.3.1.7 | Counter64 | 0..18446744073709551615 | The number of multicast octets sent by the circuit.
rbnSubsMcastOctetsReceived rbnSubsStatsEntry 8 1.3.6.1.4.1.2352.2.27.1.2.3.1.8 | Counter64 | 0..18446744073709551615 | The number of multicast octets received by the circuit.
rbnSubsMcastPktsSent rbnSubsStatsEntry 9 1.3.6.1.4.1.2352.2.27.1.2.3.1.9 | Counter64 | 0..18446744073709551615 | The number of multicast packets sent by the circuit.
rbnSubsMcastPktsReceived rbnSubsStatsEntry 10 1.3.6.1.4.1.2352.2.27.1.2.3.1.10 | Counter64 | 0..18446744073709551615 | The number of multicast packets received by the circuit.

### 1.39.13 rbnSubsProfileCountTable

This table contains counts of active subscribers by profile name.

Table 122 describes the objects in rbnSubsProfileCountTable.

Table 122 Objects in rbnSubsProfileCountTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnSubsProfileName rbnSubsProfileCountEntry 1 1.3.6.1.4.1.2352.2.27.1.2.4.1.1 | SnmpAdminString | 1..80 | Name of a profile assigned to a set of subscribers.
rbnSubsProfileCount rbnSubsProfileCountEntry 2 1.3.6.1.4.1.2352.2.27.1.2.4.1.2 | Gauge32 | 0..4294967295 | The count of active subscribers assigned this profile.

### 1.39.14 rbnSubsServiceVolumeTable

This table specifies service volume information on the subscriber circuits. It contains the volume octet counts for each active subscriber session for which the service is active.

All MIB objects defined in the table are viewed within the context identified in the SNMP protocol (the community string in SNMPv1 or SNMPv2, or the contextName in SNMPv3.)

`Index:` rbnSubsActiveName, rbnSubsActiveSessionId, rbnSubsServiceIndex

Table 123 describes the objects in rbnSubsServiceVolumeTable.

Table 123 Objects in rbnSubsServiceVolumeTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnSubsServiceVolumeLimitIn rbnSubsServiceVolumeEntry 1 1.3.6.1.4.1.2352.2.27.1.1.4.1.1 | Unsigned32 | 0..4294967295 | The volume limit in kilobytes (KB) allowed for the subscriber service to input (or receive) for this subscriber. If the value is 0, then there is no limit.
rbnSubsServiceVolumeLimitOut rbnSubsServiceVolumeEntry 2 1.3.6.1.4.1.2352.2.27.1.1.4.1.2 | Unsigned32 | 0..4294967295 | The volume limit in kilobytes (KB) allowed for the subscriber service to output (or transmit) for this subscriber. If the value is 0, then there is no limit.
rbnSubsServiceActiveTime rbnSubsServiceVolumeEntry 3 1.3.6.1.4.1.2352.2.27.1.1.4.1.3 | TimeStamp TimeTicks | 0..4294967295 | The value of sysUpTime when the service became active for this subscriber. If sysUpTime is reset to zero as a result of a reinitialization of the network management system or subsystem, the values of all TimeStamp objects are also reset.
rbnSubsServiceVolumeOctetsIn rbnSubsServiceVolumeEntry 4 1.3.6.1.4.1.2352.2.27.1.1.4.1.4 | Counter64 | 0..18446744073709551615 | The subscriber session volume octets in count.
rbnSubsServiceVolumeOctetsOut rbnSubsServiceVolumeEntry 5 1.3.6.1.4.1.2352.2.27.1.1.4.1.5 | Counter64 | 0..18446744073709551615 | The subscriber session volume octets out count.
rbnSubsServiceVolumePktsIn rbnSubsServiceVolumeEntry 6 1.3.6.1.4.1.2352.2.27.1.1.4.1.6 | Counter64 | 0..18446744073709551615 | The subscriber session volume packet in count.
rbnSubsServiceVolumePktsOut rbnSubsServiceVolumeEntry 7 1.3.6.1.4.1.2352.2.27.1.1.4.1.7 | Counter64 | 0..18446744073709551615 | The subscriber session volume packet out count.

### 1.39.15 rbnSubsServicesTable

This table contains services available to subscribers. To perform a MIB walk for this table, you must first perform a MIB walk of the rbnSubsServiceVolumeTable.

`Index:` rbnSubsServiceIndex

Table 124 describes the objects in rbnSubsServicesTable.

Table 124 Objects in rbnSubsServicesTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnSubsServiceName rbnSubsServicesEntry 2 1.3.6.1.4.1.2352.2.27.1.1.5.1.2 | SnmpAdminString | 1..128 | The name identifying the service.
rbnSubsServiceTag rbnSubsServicesEntry 3 1.3.6.1.4.1.2352.2.27.1.1.5.1.3 | SnmpAdminString | 0..32 | A tag associated with the service name, which may provide additional qualification to the name.

### 1.39.16 Example: Obtaining the Active Subscriber Circuit Description

RBN-SUBSCRIBER-ACTIVE-MIB can be used to interpret the index number of a subscriber in ASCII string format. To query the circuit description value of an active subscriber named, client-v10@test1, you can run the following SNMP query:

    getnext -v2c qcup.lab public@ctx1

    rbnSubsActiveCircuitDescr.16.99.108.105.101.110.116.45.118.49.48.64.116.
    101.115.116.49

    getone -v2c qcup.lab public@ctx1

    rbnSubsActiveCircuitDescr.16.99.108.105.101.110.116.45.118.49.48.64.
    116.101.115.116.49.25.70.70.49.48.70.70.70.70.53.56.65.49.69.69.49.
    53.45.52.52.50.66.51.52.51.65

The value of rbnsubsActiveCircuitDescr contains the information about the subscriber name length, subscriber name, and session ID. The OID returns values in this way: rbnSubsActiveCircuitDescr.[`subscriber name length`].[`subscriber name`].`[session id length]`.[`session id`]. The value of rbnsubsActiveCircuitDescr is L2TP LNS 10612245. Broken down, this means that the length of subscriber name is 16 (decimal). The subscriber name is 99.108.105.101.110.116.45.118.49.48.64.116.101.115.116.49 or, in text form, client-v10@test1, and the session ID has a length of 25 with a value 25.70.70.49.48.70.70.70.70.53.56.65.49.69.69.49.53.45.52.52.50.66.51.52.51.65 or, in text form, FF10FFFF58A1EE15-442B343A.

Use the subscriber name in the rbnSubscriberActiveMib object to display the information in the CLI and show the SNMP information about the subscriber. In this example, the CLI displays this output:

    [local]#show sub all

    TYPE   CIRCUIT          SUBSCRIBER   CONTEXT    START TIME
    ----------------------------------------------------------------------

    ppp L2TP LNS 10612245 client-v10@test1 ctx1 Mar 29 18:28:26

    ppp L2TP LNS 10612246 client-v11@test1 ctx1 Mar 29 18:28:26

    ppp L2TP LNS 10612247 client-v12@test1 ctx1 Mar 29 18:28:27

    ppp L2TP LNS 10612248 client-v13@test1 ctx1 Mar 29 18:28:27

    ppp L2TP LNS 10612249 client-v14@test1 ctx1 Mar 29 18:28:27

    ppp L2TP LNS 10612250 client-v15@test2 ctx2 Mar 29 18:28:27

    ppp L2TP LNS 10612251 client-v16@test2 ctx2 Mar 29 18:28:27

    ppp L2TP LNS 10612252 client-v17@test2 ctx2 Mar 29 18:28:27

    ppp L2TP LNS 10612253 client-v18@test2 ctx2 Mar 29 18:28:27

    ppp L2TP LNS 10612254 client-v19@test2 ctx2 Mar 29 18:28:27

    ---------------------------------------------------------------------

    Total=10

## 1.40 RBN-SYS-RESOURCES-MIB

Manages system resources, such as process events, disk utilization, and switchovers.

When using this MIB, there are differences in the usage of memory and CPU usage. This MIB can also help to generate a SNMP trap.

### 1.40.1 Notification Objects

Table 125 describes the notification objects for RBN-SYS-RESOURCES-MIB. All objects in the table are read-only unless otherwise specified.

Table 125 Notification Objects
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnSRProcessNotifyLastUpdate rbnSRProcess 1 1.3.6.1.4.1.2352.2.24.1.1.1 | TimeTicks Integer | 0..4294967295 | The value of sysUpTime when an entry in rbnSRProcessNotifyTable was last added. Because this table can contain many entries, polling of this object allows a management station to determine when redownloading of the table might be useful.
rbnSRProcessEventNotifyEnable rbnSRProcess 2 1.3.6.1.4.1.2352.2.24.1.1.2 | Integer | 1—enabled 2—disabled | Indicates whether the rbnSRProcessEvent notification should be generated for this system. This object is read-write.

### 1.40.2 System Group Objects

Table 126 describes the objects in system group objects. All objects in the table are read-only unless otherwise specified.

Table 126 System Group Objects
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnSRSystemUptime rbnSRSystem 1 1.3.6.1.4.1.2352.2.24.1.3.1 | TimeTicks Integer | 0..4294967295 | The amount of time since this system was last initialized. This is different from sysUpTime in the SNMPv2-MIB [RFC1907] because sysUpTime is the uptime of the network management portion of the system.
rbnSRSystemDate rbnSRSystem 2 1.3.6.1.4.1.2352.2.24.1.3.2 | DateAndTime Octet string | SIZE (8) | The local date and time of day on the host.
rbnSRPowerExceededStatus rbnPowerExceeded 1 1.3.6.1.4.1.2352.2.24.1.4.1 | Integer | 1—normal 2—failed | The status of alarm when a controller card is inserted and results in more power being drawn than recommended. If an instance of this object has the value normal, then the chassis power has not been exceeded. If an instance of this object has the value failed, the chassis power was exceeded when a controller card was inserted. This object is accessible-for-notify.

### 1.40.3 rbnSRProcessNotifyTable

This table provides a list of process event notifications since an agent was last reinitialized. If no process event has ever been generated, this table is empty, for example, has zero entries.

`Index:` rbnSRProcessNotifyProcName

Table 127 describes the objects in rbnSRProcessNotifyTable.

Table 127 Objects in rbnSRProcessNotifyTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnSRProcessNotifyProcName rbnSRProcessNotifyEntry 1 1.3.6.1.4.1.2352.2.24.1.1.3.1.1 | SnmpAdminString | 1..64 | A human readable name identifying a particular process in the system.
rbnSRProcessNotifyPID rbnSRProcessNotifyEntry 2 1.3.6.1.4.1.2352.2.24.1.1.3.1.2 | Unsigned32 | 0..214748364 | A decimal number uniquely identifies the process. The value 0 indicates the process has not been started.
rbnSRProcessNotifyEventCause rbnSRProcessNotifyEntry 3 1.3.6.1.4.1.2352.2.24.1.1.3.1.3 | Integer | Identifies the cause of a process death or birth event. The value firstStart (1) indicates that the process has been started the first time. The other values identify the process exit status recorded on the last process death event. On the SmartEdge router, these values correspond 1-to-1 with the values displayed by the 'show process crash-info' CLI command.
| 1—firstStart 2—hangup 3—interrupt 4—quit 5—illegalInstruction 6—traceTrap 7—abort 8—emt 9—floatingPointException 10—kill 11—busError 12—segmentFault 13—systemCallError 14—pipeError 15—alarmClock 16—softwareTermination 17—urgentConditionOnIOChannel 18—stopNotFromTty 19—stopFromTty
| Integer (continued) | 20—continueStopped 21—childExit 22—ttyInput 23—ttyOutput 24—inputOutput 25—exceededCpuTime 26—exceededFileSize 27—virtualAlarm 28—profilingAlarm 29—windowResize 30—infoRequest 31—userDefined1 32—userDefined2 33—powerFailRestart 34—unknown
rbnSRProcessNotifyEventType rbnSRProcessNotifyEntry 4 1.3.6.1.4.1.2352.2.24.1.1.3.1.4 | Integer | 1—death 2—birth | The type of event notification sent on the process described by this row of the table. The process event type death, indicates that the agent has been informed that the process is not available for any use. The event type birth, indicates that the agent has been informed that the process has started.
rbnSRProcessNumOfSpawn rbnSRProcessNotifyEntry 5 1.3.6.1.4.1.2352.2.24.1.1.3.1.5 | Unsigned32 | 0..2147483647 | The number of times the process has been spawned since the system was last initialized. Note that this is different from the restart of the network management portion of the system.
rbnSRProcessNotifyLastTimeSent rbnSRProcessNotifyEntry 6 1.3.6.1.4.1.2352.2.24.1.1.3.1.6 | TimeTicks Integer | 0..4294967295 | The value of the sysUpTime object at the time this notification was last generated on the process.

### 1.40.4 rbnSRStorageTable

This is a table of long-term storage devices contained by the system. Disk devices accessed remotely over a network are not included.

`Index:` rbnSRStorageIndex

Table 128 describes the objects in rbnSRStorageTable. All objects in the table are read-only unless otherwise specified.

Table 128 Objects in rbnSRStorageTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnSRStorageIndex rbnSRStorageEntry 1 1.3.6.1.4.1.2352.2.24.1.2.1.1.1 | Integer32 | 1..2147483647 | A unique value for each long-term storage device contained by the system. The value for each physical storage device must remain constant at least from one reinitialization of the agent to the next reinitialization.
rbnSRStorageDescr rbnSRStorageEntry 2 1.3.6.1.4.1.2352.2.24.1.2.1.1.2 | SnmpAdminString | 0..64 | A textual description of this storage device, optionally including the device manufacturer, revision, and serial number.
rbnSRStorageMedia rbnSRStorageEntry 3 1.3.6.1.4.1.2352.2.24.1.2.1.1.3 | Integer | 1—other 2—hardDisk 3—flashMemory | The type of media used in this long-term storage device.
rbnSRStorageRemovable rbnSRStorageEntry 4 1.3.6.1.4.1.2352.2.24.1.2.1.1.4 | TruthValue Integer | 1—true 2—false | Denotes whether the storage media can be removed from the slot.
rbnSRStorageSize rbnSRStorageEntry 5 1.3.6.1.4.1.2352.2.24.1.2.1.1.5 | RbnKBytes Integer32 | 0..2147483647 | The total size for this long-term storage device. If the media is removable and is currently removed, this value should be zero.
rbnSRStorageUtilization rbnSRStorageEntry 6 1.3.6.1.4.1.2352.2.24.1.2.1.1.6 | RbnPercentage Integer32 | 0..100 | The percent (%) utilization of the storage space on a scale of 0 to 100%. The formula used to calculate the Utilization is as follows. Used blocks * 100 Utilization = free blocks avail to the user + used blocks. Note that the divisor is the total number of blocks available to the user, which is a subset of the total storage size on the device in the rbnSRStorageSize object.
rbnSRStorageSlot rbnSRStorageEntry 7 1.3.6.1.4.1.2352.2.24.1.2.1.1.7 | RbnSlot Unsigned32 | 0..255 | The chassis slot number in which the controller card containing this storage device is present.
rbnSRStorageMountTime rbnSRStorageEntry 8 1.3.6.1.4.1.2352.2.24.1.2.1.1.8 | TimeTicks Integer | 0..4294967295 | The value of sysUpTime when this storage device was last mounted.
rbnSRStorageStatus rbnSRStorageEntry 9 1.3.6.1.4.1.2352.2.24.1.2.1.1.9 | Integer | 1—operational 2—degrading 3—failed | The functional status of this storage device.
rbnSRStorageErrors rbnSRStorageEntry 10 1.3.6.1.4.1.2352.2.24.1.2.1.1.10 | Counter32 | 0..4294967295 | The cumulative count of soft errors on this storage device.

### 1.40.5 rbnSseDiskStorageTable

This table provides details of these disks.

File Server System Blade is a card on the SmartEdge platform that manages data on hard disks connected to the card.

`Index:` rbnSseDiskSlot, rbnSseDiskNum

Table 129 describes the objects in rbnSseDiskStorageTable. All objects in the table are read-only unless otherwise specified.

Table 129 Objects in rbnSseDiskStorageTable
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnSseDiskSlot rbnSseDiskStorageEntry 1 1.3.6.1.4.1.2352.2.24.1.2.2.1.1 | RbnSlot Unsigned32 | 0..255 | The chassis slot number in which the disk resides. This object is not-accessible.
rbnSseDiskNum rbnSseDiskStorageEntry 2 1.3.6.1.4.1.2352.2.24.1.2.2.1.2 | Unsigned32 | 1..10 | The disk number used to identity the disk. This object is not-accessible.
rbnSseDiskState rbnSseDiskStorageEntry 3 1.3.6.1.4.1.2352.2.24.1.2.2.1.3 | Integer | 1—up 2—down | Operational status of the disk.
rbnSseDiskSize rbnSseDiskStorageEntry 4 1.3.6.1.4.1.2352.2.24.1.2.2.1.4 | Unsigned32 | 0..214748364 | Total size of the disk in GBytes.
rbnSseDiskUsed rbnSseDiskStorageEntry 5 1.3.6.1.4.1.2352.2.24.1.2.2.1.5 | Unsigned32 | 0..214748364 | Total disk space utilized in GBytes.

## 1.41 RBN-SYS-SECURITY-MIB

Defines objects and notifications related to system- and network-level security issues. Objects defined in this MIB are only accessible within the context identified in the SNMP protocol (that is, the community string in SNMPv1 or SNMPv2 or the contextName in SNMPv3).

### 1.41.1 RBN-SYS-SECURITY-MIB Notification Objects

This table provides a set of objects for monitoring security.

Table 130 describes objects for monitoring security.

For this function, the router samples data at the start and end of the interval configured using the `interval` command in malicious-traffic configuration mode. The difference between the start and end of the interval is called the delta value.

Table 130 Objects for Monitoring Security
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnSysSecNotifyEnable 1.3.6.1.4.1.2352.5.54.1.1.1 rbnSysSecThresholdObjects 1 | Bits | maliciousPkt (0) | Bit mask to enable or disable notifications triggered by crossing specific thresholds.
rbnMeasurementInterval 1.3.6.1.4.1.2352.5.54.1.1.2 rbnSysSecThresholdObjects 2 | Gauge32 | 1..3600 | Data-sampling interval configured with the `interval` command in malicious-traffic configuration mode; the default value is 60 seconds. When you set the sampling interval, it should be short enough that the sampled variable is unlikely to increase or decrease by more than the range of the variable.
rbnMaliciousPktsThresholdHi 1.3.6.1.4.1.2352.5.54.1.1.3 rbnSysSecThresholdObjects 3 | RbnUnsigned64 Octet string | SIZE (8) | High threshold. When the current delta value of the malicious packets counter is greater than or equal to this threshold, and the delta value at the last sampling interval was less than this threshold, an rbnMaliciousPktsThresholdHi notification is sent. Another rbnMaliciousPktsThresholdHi notification cannot be sent until an rbnMaliciousPktsThresholdLow notification has been sent. Configure the high threshold using the `threshold` command in malicious-traffic configuration mode
rbnMaliciousPktsThresholdLow rbnSysSecThresholdObjects 4 1.3.6.1.4.1.2352.5.54.1.1.4 | RbnUnsigned64 Octet string | SIZE (8) | Low threshold. When the current delta value of the malicious packets counter is less than or equal to this threshold, and the delta value at the last sampling interval was greater than this threshold, a rbnMaliciousPktsThresholdLow notification is sent. Another rbnMaliciousPktsThresholdLow notification cannot be sent until an rbnMaliciousPktsThresholdHi notification has been sent. Configure the low threshold using the `threshold` command in malicious-traffic configuration mode
rbnMaliciousPktsDelta 1.3.6.1.4.1.2352.5.54.1.2.2 rbnSysSecStatsObjects 2 | CounterBasedGauge64 Counter64 | 0..18446744073709551615 | The delta value of rbnMaliciousPktsCounters from the most recently completed sampling interval.
rbnMaliciousPktsCounter 1.3.6.1.4.1.2352.5.54.1.2.1 rbnSysSecStatsObjects 1 | Counter64 | 0..18446744073709551615 | A count of all malicious (dropped) packets, which can include but are not limited to: Malformed IP packets Malformed Layer 4 IP packets filtered by ACLs for specific faults IP packets identified as attempting to spoof a system IP packets that failed reassembly
rbnThresholdNotifyTime 1.3.6.1.4.1.2352.5.54.1.4.1 rbnSysSecNotifyObjects 1 | DateAndTime Octet string | SIZE (8) | The date and time of the notification.

## 1.42 RBN-TACACS-MIB

Defines notifications for tracking the Terminal Access Controller Access Control System Plus (TACACS+) server state (in accordance with Internet-Draft draft-grant-tacacs-02.txt).

### 1.42.1 TACACS+ Notification Objects

Table 131 describes the notification objects for RBN-TACACS-MIB. All objects in the table are accessible-for-notify.

Table 131 TACACS+ Notification Objects
Object and Object Identifier | Type | Value Range | Description
--- | --- | --- | ---
rbnTacacsContext rbnTacacsNotifyObjects 1 1.3.6.1.4.1.2352.2.33.1.3.1 | SnmpAdminString | 1..63 | The name of the context in which this server is configured.
rbnTacacsServerIndex rbnTacacsNotifyObjects 2 1.3.6.1.4.1.2352.2.33.1.3.2 | Unsigned32 | 1..4294967295 | A unique index value assigned to each TACACS server.
rbnTacacsServerAddressType rbnTacacsNotifyObjects 3 1.3.6.1.4.1.2352.2.33.1.3.3 | InetAddressType Integer | 0—unknown 1—ipv4 2—ipv6 16—dns | The type of address contained in the rbnTacacsServerAddress object.
rbnTacacsServerAddress rbnTacacsNotifyObjects 4 1.3.6.1.4.1.2352.2.33.1.3.4 | InetAddress Octet String | 0..255 | The TACACS+ server address.
rbnTacacsServerPort rbnTacacsNotifyObjects 5 1.3.6.1.4.1.2352.2.33.1.3.5 | Unsigned32 | 0..65535 | The TCP port number.
rbnTacacsServerState rbnTacacsNotifyObjects 6 1.3.6.1.4.1.2352.2.33.1.3.6 | RbnTacacsState Integer | 1—unknown 2—up 3—down | The current state of the TACACS+ server.
rbnTacacsServerReason rbnTacacsNotifyObjects 7 1.3.6.1.4.1.2352.2.33.1.3.7 | RbnTacacsReason Integer | 1—responding 2—packetTimeout 3—serverTimeout 4—serverError | The reason for the server's last state change.
rbnTacacsUserName rbnTacacsNotifyObjects 8 1.3.6.1.4.1.2352.2.33.1.3.8 | SnmpAdminString | 0..128 | The name of the user the system was trying to authenticate or send accounting information for when the TACACS+ server transitioned to 'down'. The 'username' is valid only when transitioning due to a packet-level timeout. When transitioning due to any other reason, the value for this object will be a string of zero (0) length.
rbnTacacsServerMsg rbnTacacsNotifyObjects 9 1.3.6.1.4.1.2352.2.33.1.3.9 | SnmpAdminString | 0..256 | A text string optionally provided by the TACACS+ server when the rbnTacacsServerReason object is 'serverError'. In all other cases, this is a string of zero (0) length.

## 1.43 Type Appendix

This section lists the supported MIB Types and their integer range.

### 1.43.1 RbnAlarmId

1—unknown

2—cpFail

3—cpBackplaneFail

4—diagFail

5—voltageFail

6—controllerSwitchFail

7—controllerTempCritical

8—controllerFail

9—controllerDiagFail

10—cpPowerOnDiagFail

11—controllerPowerOnDiagFail

12—cpOverheat

13—controllerOverheat

14—backplaneclkfail

15—btciferror

16—btcnotready

17—cpbackplanedegrade

18—cpcardcodemismatch

19—cpmismatch

20—cpmissing

21—cpresetcomplete

22—downloadcompleted

23—downloadfailed

24—syncfail

25—backupfail

26—controllercardcodemismatch

27—controllercardtypemismatch

28—controllermissing

29—controlleroverheat

30—controllerswitchauto

31—controllerswitchcompleted

32—controllerswitchexfailed

33—controllerswitchforced

34—controllerswitchmanual

35—localfantrayinventfail

36—localinventfail

37—localbackplaneinventfail

38—lostm2m

39—nonvolatilememfail

40—peerhwincompatible

41—peerinventfail

42—peermodeincompatible

43—peersharedformatmismatch

44—rtclockfail

45—mic1missing

46—mic2missing

47—mic1mismatch

48—mic2mismatch

49—mic1voltagefailure

50—mic2voltagefailure

51—mic1overheat

52—mic2overheat

53—mic1failure

54—mic2failure

55—mic1podfail

56—mic2podfail

57—mic1diagnosticfail

58—mic2diagnosticfail

59—ethtransceiverrxpowerhi

60—ethtransceiverrxpowerlo

61—ethtransceivertemphi

62—ethtransceivertemplo

63—ethtranceivervoltagehi

64—ethtranceivervoltagelo

65—ethtransceiverbiashi

66—ethtransceiverbiaslo

67—ethtransceivertxpowerhi

68—ethtransceivertxpowerlo

69—ethtransceiveraux1hi

70—ethtransceiveraux1lo

71—ethtransceiveraux2hi

72—ethtransceiveraux2lo

73—ethtransceiverlvcc5hi

74—ethtransceiverlvcc5lo

75—ethtransceiverlvcc3hi

76—ethtransceiverlvcc3lo

77—ethtransceiverlvcc2hi

78—ethtransceiverlvcc2lo

79—controllerbsdl2cacheerror

80—controllervxwl2cacheerror

81—fsServerDownAlarm

82—aseAsp1Down

83—aseAsp2Down

84—controllerSwNotSupported

90—cesPwOutage

91—cesLossOfConnectivity

### 1.43.2 RbnAlarmProbableCause

1—aIS

3—degradedSignal

4—farEndReceiverFailure

5—framingError

6—lossOfFrame

7—lossOfPointer

8—lossOfSignal

9—payloadTypeMismatch

10—transmissionError

12—excessiveBER

13—pathTraceMismatch

14—unavailable

15—signalLableMismatch

17—receiveFailure

18—transmitFailure

19—modulationFailure

20—demodulationFailure

21—linkFailure

22—configurationMismatch

23—concatenationMismatch

51—pbackplaneFailure

53—equipmentIdDuplication

54—externalIFDeviceProblem

55—lineCardProblem

56—multiplexerProblem

57—nEIdentifierDuplication

58—powerProblem

59—processorProblem

60—protectionPathFailure

61—receiverFailure

62—replaceableUnitMissing

63—replaceableUnitTypeMismatch

64—syncSourceMismatch

65—terminalProblem

66—timingProblem

67—transmitterFailure

68—trunkCardProblem

69—replaceableUnitProblem

70—realTimeClockFailure

101—airCompressorFailure

102—airConditioningFailure

103—airDryerFailure

104—batteryDischarging

105—batteryFailure

106—commercialPowerFailure

107—coolingFanFailure

108—engineFailure

109—fireDetectorFailure

110—fuseFailure

111—generatorFailure

112—lowBatteryThreshold

113—pumpFailure

114—rectifierFailure

115—rectifierHighVoltage

116—rectifierLowVoltage

117—ventilationsSystemFailure

118—enclosureDoorOpen

119—explosiveGas

120—fire

121—flood

122—highHumidity

123—highTemperature

124—highWind

125—iceBuildUp

126—intrusionDetection

127—lowFuel

128—lowHumidity

129—lowCablePressure

130—lowTemperature

131—lowWater

132—smoke

133—toxicGas

149—customized

151—storageCapacityProblem

152—memoryMismatch

153—corruptData

154—outOfCPUCycles

155—sfwrEnvironmentProblem

156—sfwrDownloadFailure

157—lossOfRealTime

158—reinitialized

159—operationNotification

160—operationFailure

1001—lossOfTimingSource

1002—apsChannelProcessingFailure

1003—apsByteFailure

1004—apsChannelMatchFailure

1005—apsModeMismatch

1007—lossOfTUMultiframeIndicator

1010—pathSelectorFailure

1011—blsrDefaultKBytes

1012—blsrInconsistentAPSCodes

1013—blsrNodeIdMismatch

1014—blsrImproperAPSCodes

1015—blsrSquelching

1016—blsrInvalidNeighbour

1017—blsrInvalidRingMap

1018—blsrInvalidRingId

1019—blsrIncompleteRingConfig

1020—blsrIncompleteETConfig

1021—blsrNodeIncorrectOrientation

1024—other

1025—pwOutage

### 1.43.3 RbnAlarmType

The type of the alarm.

rbnCardAlarmType:

1—other

2—communicationsAlarm

3—qualityOfServiceAlarm

4—processingErrorAlarm

5—equipmentAlarm

6—environmentalAlarm

7—integrityViolation

8—operationalViolation

9—physicalViolation

10—securityServiceOrMechanismViolation

11—timeDomainViolation

### 1.43.4 IANAItuProbableCause

1—aIS

2—callSetUpFailure

3—degradedSignal

4—farEndReceiverFailure

5—framingError

6—lossOfFrame

7—lossOfPointer

8—lossOfSignal

9—payloadTypeMismatch

10—transmissionError

11—remoteAlarmInterface

12—excessiveBER

13—pathTraceMismatch

14—unavailable

15—signalLabelMismatch

16—lossOfMultiFrame

17—receiveFailure

18—transmitFailure

19—modulationFailure

20—demodulationFailure

21—broadcastChannelFailure

22—connectionEstablishmentError

23—invalidMessageReceived

24—localNodeTransmissionError

25—remoteNodeTransmissionError

26—routingFailure

51—backplaneFailure

52—dataSetProblem

53—equipmentIdentifierDuplication

54—externalIFDeviceProblem

55—lineCardProblem

56—multiplexerProblem

57—nEIdentifierDuplication

58—powerProblem

59—processorProblem

60—protectionPathFailure

61—receiverFailure

62—replaceableUnitMissing

63—replaceableUnitTypeMismatch

64—synchronizationSourceMismatch

65—terminalProblem

66—timingProblem

67—transmitterFailure

68—trunkCardProblem

69—replaceableUnitProblem

70—realTimeClockFailure

71—antennaFailure

72—batteryChargingFailure

73—diskFailure

74—frequencyHoppingFailure

75—iODeviceError

76—lossOfSynchronisation

77—lossOfRedundancy

78—powerSupplyFailure

79—signalQualityEvaluationFailure

80—tranceiverFailure

81—protectionMechanismFailure

82—protectingResourceFailure

101—airCompressorFailure

102—airConditioningFailure

103—airDryerFailure

104—batteryDischarging

105—batteryFailure

106—commercialPowerFailure

107—coolingFanFailure

108—engineFailure

109—fireDetectorFailure

110—fuseFailure

111—generatorFailure

112—lowBatteryThreshold

113—pumpFailure

114—rectifierFailure

115—rectifierHighVoltage

116—rectifierLowFVoltage

117—ventilationsSystemFailure

118—enclosureDoorOpen

119—explosiveGas120—fire

121—flood

122—highHumidity

123—highTemperature

124—highWind

125—iceBuildUp

126—intrusionDetection

127—lowFuel

128—lowHumidity

129—lowCablePressure

130—lowTemperatue

131—lowWater

132—smoke

133—toxicGas

134—coolingSystemFailure

135—externalEquipmentFailure

136—externalPointFailure

151—storageCapacityProblem

152—memoryMismatch

153—corruptData

154—outOfCPUCycles

155—sfwrEnvironmentProblem

156—sfwrDownloadFailure

157—lossOfRealTimel

158—applicationSubsystemFailure

159—configurationOrCustomisationError

160—databaseInconsistency

161—fileError

162—outOfMemory

163—softwareError

164—timeoutExpired

165—underlayingResourceUnavailable

166—versionMismatch

201—bandwidthReduced

202—congestion

203—excessiveErrorRate

204—excessiveResponseTime

205—excessiveRetransmissionRate

206—reducedLoggingCapability

207—systemResourcesOverload

500—adapterError

501—applicationSubsystemFailture

502—bandwidthReducedX733

503—callEstablishmentError

504—communicationsProtocolError

505—communicationsSubsystemFailure

506—configurationOrCustomizationError

507—congestionX733

508—coruptData

509—cpuCyclesLimitExceeded

510—dataSetOrModemError

511—degradedSignalX733

512—dteDceInterfaceError

513—enclosureDoorOpenX733

514—equipmentMalfunction

515—excessiveVibration

516—fileErrorX733

517—fireDetected

518—framingErrorX733

519—heatingVentCoolingSystemProblem

520—humidityUnacceptable

521—inputOutputDeviceError

522—inputDeviceError

523—lanError

524—leakDetected

525—localNodeTransmissionErrorX733

526—lossOfFrameX733

527—lossOfSignalX733

528—materialSupplyExhausted

529—multiplexerProblemX733

530—outOfMemoryX733

531—ouputDeviceError

532—performanceDegraded

533—powerProblems

534—pressureUnacceptable

535—processorProblems

536—pumpFailureX733

537—queueSizeExceeded

538—receiveFailureX733

539—receiverFailureX733

540—remoteNodeTransmissionErrorX733

541—resourceAtOrNearingCapacity

542—responseTimeExecessive

543—retransmissionRateExcessive

544—softwareErrorX733

545—softwareProgramAbnormallyTerminated

546—softwareProgramError

547—storageCapacityProblemX733

548—temperatureUnacceptable

549—thresholdCrossed

550—timingProblemX733

551—toxicLeakDetected

552—transmitFailureX733

553—transmiterFailure

554—underlyingResourceUnavailable

555—versionMismatchX733

600—authenticationFailure

601—breachOfConfidentiality

602—cableTamper

603—delayedInformation

604—denialOfService

605—duplicateInformation

606—informationMissing

607—informationModificationDetectede

608—informationOutOfSequence

609—keyExpired

610—nonRepudiationFailure

611—outOfHoursActivity

612—outOfServic

613—proceduralError

614—unauthorizedAccessAttempt

615—unexpectedInformation

1024—other

### 1.43.5 IANAItuEventType

1—other

2—communicationsAlarm

3—qualityOfServiceAlarm

4—processingErrorAlarm

5—equipmentAlarm

6—environmentalAlarm

7—integrityViolation

8—operationalViolation

9—physicalViolation

10—securityServiceOrMechanismViolation

11—timeDomainViolation

### 1.43.6 ItuPerceivedSeverity

1—cleared

2—indeterminate

3—critical

4—major

5—minor

6—warning

### 1.43.7 CtlErrType

0—ctlrunt

1—hdr2long

2—dupSCCRQ

3—duppkt

4—droppkt

5—badCmType

6—avp2long

7—avpUnknown

8—typeNot1st

9—mtype000

10—cantUnhide

11—avpLen

12—missAvp

13—invalidAvp

14—avp2big

15—badAvpLen

16—rexmt

17—scksnderr

18—remWndoful

19—maxRexmts

20—sccrqColide

21—badVers

22—noChapRsp

23—authFailed

24—sesExists

25—badcrpsesi

26—cdnBadid

27—iccnBadid

28—dataRunt

29—badSCCRQna

30—badSCCRP

31—dupIcrq

32—badSCCCN

33—badMsgType

34—sccrqSteal

35—remXmtState

36—cdnThrottle

255—none

### 1.43.8 RbnVpnXcFlagsType and RbnVpnPwFlagsType

0—none

2—deletingSignal

3—deletingConfig

4—inLblmap

5—updating

6—up

7—inLdp

8—fromLdp

9—fromConfig

10—stale

11—expSet

12—ismUp

13—peerUp

14—remoteEncap

15—localCbit

16—remoteCbit

17—primary

18—backup

19—primaryAutoRevert

20—standby

21—cwMismatch

22—sigParamsMatch

23—encapError

### 1.43.9 RbnAlarmPerceivedSeverity

1—cleared

2—critical

3—major

4—minor

5—warning