Input/Output TS/IP

Input Status

ASI | Total Bit Rate (Mbps) |  | Packet Size (Bytes) |
| Valid Bit Rate (Mbps) |  |  |

| Total Bit Rate (Mbps) |  |  |

| Valid Bit Rate (Mbps) |  | Packet Size (Bytes) |
| C/N (dB) |  | BER |
| Eb/N0 (dB) |  |  |

| Packet Size (Bytes) |  |  |

| FEC |  | Guard Interval |
| FFT |  |  |

| Pilot Pattern |  | LDPC Size |
| Spectrum |  | BW Extension |
| ConstellRotation |  | L1 Constell |
| Network Id |  | Cell Id |
| T2 System Id |  | T2 Version |

IP | Total Bit Rate (Mbps) |  | Packet Size (Bytes) |
| Link Status |

Output Status

Mux Output Overflow |

T2 Modulator Max Bit Rate (Mbps) |
T2 Modulator Vaild Bit Rate (Mbps) |

Remux Status |
Remux Valid Bit Rate (Mbps) |

SI/PSI Priority |

CI Valid Bit Rate (Mbps) |
CI Total Bit Rate (Mbps) |