SNR-ERD-4 DEFINITIONS ::= BEGIN

IMPORTS
	MODULE-IDENTITY, OBJECT-IDENTITY, OBJECT-TYPE, NOTIFICATION-TYPE
		FROM SNMPv2-SMI
	enterprises, IpAddress, Counter					
		FROM RFC1155-SMI
	DisplayString
		FROM RFC1213-MIB
	NOTIFICATION-GROUP
		FROM SNMPv2-CONF
	; 

snr MODULE-IDENTITY
	LAST-UPDATED	"201810261200Z"
	ORGANIZATION	"NAG "
	CONTACT-INFO	"erd@nag.ru"
	DESCRIPTION
		"The MIB module for SNR-ERD"
	REVISION		"201504291200Z"
	DESCRIPTION
		"Initial revision." 
	::= { enterprises 40418 }


snr-erd		OBJECT IDENTIFIER	::= { snr 2 }
snr-erd-4	OBJECT IDENTIFIER	::= { snr-erd 6 }

measurements		OBJECT IDENTIFIER	 ::= { snr-erd-4 1 }

dio			OBJECT IDENTIFIER	::= { snr-erd-4 2 }
modules			OBJECT IDENTIFIER	::= { snr-erd-4 5 }
options			OBJECT IDENTIFIER	::= { snr-erd-4 10 }
diffparams		OBJECT IDENTIFIER	::= { snr-erd-4 11 }


oneWire		OBJECT IDENTIFIER	::= { measurements 1 }
sp			OBJECT IDENTIFIER	::= { measurements 30 }

GSM			OBJECT IDENTIFIER	::= { modules 1 }
RF			OBJECT IDENTIFIER	::= { modules 2 }

upsStatus		OBJECT IDENTIFIER	::= { diffparams 1 }

pid			OBJECT IDENTIFIER	::= { diffparams 10 }

traps			OBJECT IDENTIFIER	::= { snr-erd-4 0 }

crit			OBJECT IDENTIFIER	::= { options 10 }

-- measurements

adcSensor		OBJECT-TYPE
	SYNTAX		INTEGER
        MAX-ACCESS	read-only
        STATUS		current
        DESCRIPTION	"ADC sensor value"
::= { measurements 2 }

temperatureDHT		OBJECT-TYPE
	SYNTAX		INTEGER
        MAX-ACCESS	read-only
        STATUS		current
        DESCRIPTION	"DHT temperature value"
::= { measurements 8 }

humidityDHT		OBJECT-TYPE
	SYNTAX		INTEGER
        MAX-ACCESS	read-only
        STATUS		current
        DESCRIPTION	"DHT humidity value"
::= { measurements 9 }

-- dtsTable

dtsTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF dtsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION	"A list of temperature sensors values"
    ::= { oneWire 1 }

dtsEntry OBJECT-TYPE
    SYNTAX      dtsEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION	"An entry (conceptual row) in the dtsTable"
    INDEX   { dtsId } 
::= { dtsTable 1 }

dtsEntry ::=
    SEQUENCE {
        dtsId           	UInteger32,
	dtsName			OctetString,
        dtsTemp            	Integer,
		tempCritNotif		Integer,
		tempCritMin			Integer,
		tempCritMax			Integer
    }

dtsId 		OBJECT-TYPE
    SYNTAX      UInteger32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION	"Temperature sensor id"
    ::= { dtsEntry 1 }

dtsName 	OBJECT-TYPE
    SYNTAX      OCTET STRING
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION	"Name (max 20)"
    ::= { dtsEntry 2 }

dtsTemp 	OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Temperature value"
    ::= { dtsEntry 3 }
	
tempCritNotif	OBJECT-TYPE
	SYNTAX		INTEGER
		{
				No	(0),
				Yes	(1),
		}
        MAX-ACCESS	read-write
        STATUS		current
        DESCRIPTION	"Enable notifications on the critical temperature"
::= { dtsEntry 10 }
	
tempCritMin		OBJECT-TYPE
	SYNTAX		INTEGER
        MAX-ACCESS	read-write
        STATUS		current
        DESCRIPTION	"Minimal critical temperature. 
Up to -55 °C"
::= { dtsEntry 15 }

tempCritMax	OBJECT-TYPE
	SYNTAX		INTEGER
        MAX-ACCESS	read-write
        STATUS		current
        DESCRIPTION	"Maximum critical temperature. 
Up to +125°C"
::= { dtsEntry 16 }

-- shuntTable

shuntTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF shuntEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "A list of SNR-SHUNT values"
    ::= { oneWire 2 }

shuntEntry OBJECT-TYPE
    SYNTAX      shuntEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "An entry (conceptual row) in the shuntTable"
    INDEX   { pwrSensIdent }
    ::= { shuntTable 1 }

shuntEntry ::=
    SEQUENCE {
        shuntId      	UInteger32,
	shuntName	OctetString,
        shuntTemp       Integer,
        shuntVolt       Integer,
	shuntCurrent	Integer,
	shuntCapacity	Integer,
	shuntChrgCap	Integer,
	shuntDischCap	Integer,
	shuntEndOfChrg	OctetString,
	shuntDiscn	OctetString,
	shuntBatLive	TimeTicks,
	shuntDischTime	TimeTicks
    }

shuntId 	OBJECT-TYPE
    SYNTAX      UInteger32
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "SNR-SHUNT id"
    ::= { shuntEntry 1 }

shuntName OBJECT-TYPE
    SYNTAX      OCTET STRING
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
            "Name (max 20)"
    ::= { shuntEntry 2 }

shuntTemp OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Temperature value"
    ::= { shuntEntry 3 }

shuntVolt OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
            "Voltage"
    ::= { shuntEntry 4 }

shuntCurrent OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
            "Current"
    ::= { shuntEntry 5 }

shuntChrgLvl OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
            "Battery charge level (0..100%)"
    ::= { shuntEntry 6 }

shuntChrgCap 	OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Charge capacity"
    ::= { shuntEntry 7 }

shuntDischCap OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Discharge capacity"
    ::= { shuntEntry 8 }

shuntEndOfChrg OBJECT-TYPE
    SYNTAX      OCTET STRING
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "End of charge time"
    ::= { shuntEntry 9 }

shuntDiscn OBJECT-TYPE
    SYNTAX      OCTET STRING
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Disconnect time"
    ::= { shuntEntry 10 }

shuntBatLive OBJECT-TYPE
    SYNTAX      TimeTicks
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Battery using period"
    ::= { shuntEntry 11 }

shuntDischTime OBJECT-TYPE
    SYNTAX      TimeTicks
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Time to full discharge"
    ::= { shuntEntry 12 }


-- wirelessSensors

rfshtpTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF rfshtpEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "A list of wireless sensors values"
    ::= { measurements 10 }

rfshtpEntry OBJECT-TYPE
    SYNTAX      rfshtpEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "An entry (conceptual row) 
in the wrlssSensTable"
    INDEX   { wrlssSensIdent }
    ::= { rfshtpTable 1 }

rfshtpEntry ::=
    SEQUENCE {
        rfshtpId           OctetString,
        rfshtpName         OctetString,
        rfshtpTemp         Integer,
	rfshtpHum	   Integer,
	rfshtpPres	   Integer
    }

rfshtpId OBJECT-TYPE
    SYNTAX      OCTET STRING
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Wireless sensor id"
    ::= { rfshtpEntry 1 }

rfshtpName OBJECT-TYPE
    SYNTAX      OCTET STRING
    MAX-ACCESS  read-write
    STATUS      current
    DESCRIPTION
            "Name (max 20)"
    ::= { rfshtpEntry 2 }

rfshtpTemp OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Temperature value"
    ::= { rfshtpEntry 3 }

rfshtpHum OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Humidity value"
    ::= { rfshtpEntry 4 }

rfshtpPres OBJECT-TYPE
    SYNTAX      INTEGER
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "Pressure value"
    ::= { rfshtpEntry 5 }

-- sp

-- rsshtpTable
rsshtpTable		OBJECT-TYPE
	SYNTAX		SEQUENCE OF rsshtpEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION	"A list of SNR-RSsensor-H/T/P values"
::= { sp 1 }

rsshtpEntry OBJECT-TYPE
	SYNTAX		rsshtpEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION	"An entry (conceptual row) 
in the rsshtpTable"
	INDEX		{ rsshtpIdent }
::= { rsshtpTable 1 }

rsshtpEntry ::= SEQUENCE 
{
    rsshtpIdent	OctetString,
	rsshtpName	OctetString,
    rsshtpTemp	Integer,
	rsshtpHum	Integer,
	rsshtpPssr	Integer,
	tempCritNotif		Integer,
	tempCritMin			Integer,
	tempCritMax			Integer
}

rsshtpIdent		OBJECT-TYPE
	SYNTAX		OCTET STRING
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION	"SNR-RSsensor-H/T/P id"
::= { rsshtpEntry 1 }

rsshtpName		OBJECT-TYPE
    	SYNTAX      	OCTET STRING
    	MAX-ACCESS  	read-write
    	STATUS      	current
    	DESCRIPTION 	"Name (max 20)"
::= { rsshtpEntry 2 }

rsshtpTemp		OBJECT-TYPE
	SYNTAX		INTEGER
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION	"Temperature value 1"
::= { rsshtpEntry 3 }

rsshtpHum		OBJECT-TYPE
	SYNTAX		INTEGER
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION	"Humidity value"
::= { rsshtpEntry 4 }

rsshtpPssr		OBJECT-TYPE
	SYNTAX		INTEGER
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION	"Pressure value"
::= { rsshtpEntry 6 }

tempCritNotif	OBJECT-TYPE
	SYNTAX		INTEGER
		{
				No	(0),
				Yes	(1),
		}
        MAX-ACCESS	read-write
        STATUS		current
        DESCRIPTION	"Enable notifications on the critical temperature"
::= { rsshtpEntry 10 }
	
tempCritMin		OBJECT-TYPE
	SYNTAX		INTEGER
        MAX-ACCESS	read-write
        STATUS		current
        DESCRIPTION	"Minimal critical temperature. 
Up to -55 °C"
::= { rsshtpEntry 15 }

tempCritMax	OBJECT-TYPE
	SYNTAX		INTEGER
        MAX-ACCESS	read-write
        STATUS		current
        DESCRIPTION	"Maximum critical temperature. 
Up to +125°C"
::= { rsshtpEntry 16 }

-- rscounterTable

rscounterTable		OBJECT-TYPE
	SYNTAX		SEQUENCE OF rscounterEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION	"A list of SNR-RS-Counter"
::= { sp 5 }

rscounterEntry OBJECT-TYPE
	SYNTAX		rscounterEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION	"An entry (conceptual row) 
in the rscounterTable"
	INDEX		{ rscounterIdent }
::= { rscounterTable 1 }

rscounterEntry ::= SEQUENCE 
{
    rscounterIdent	OctetString,
	rscounterName	OctetString,
}

rscounterIdent		OBJECT-TYPE
	SYNTAX		OCTET STRING
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION	"SNR-RS-Counter id"
::= { rscounterEntry 1 }

rscounterName		OBJECT-TYPE
    	SYNTAX      	OCTET STRING
    	MAX-ACCESS  	read-write
    	STATUS      	current
    	DESCRIPTION 	"Name (max 20)"
::= { rscounterEntry 2 }


-- rsshtp1WTable
rsshtp1WTable		OBJECT-TYPE
	SYNTAX		SEQUENCE OF rsshtp1WEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION	"A list of temperature sensors 
are connected to SNR-RSsensor-H/T/P"
::= { sp 100 }

rsshtp1WEntry 		OBJECT-TYPE
	SYNTAX		rsshtp1WEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION	"An entry (conceptual row) 
in the rsshtp1WTable"
	INDEX		{ rsshtp1WIdent }
::= { rsshtp1WTable 1 }

rsshtp1WEntry ::= SEQUENCE 
{
        rsshtp1WIdent	UInteger32,
	rsshtp1WName	OctetString,
        rsshtp1WTemp	Integer,
	rsshtp1WMaster	OctetString,
	tempCritNotif		Integer,
	tempCritMin			Integer,
	tempCritMax			Integer
}

rsshtp1WIdent		OBJECT-TYPE
	SYNTAX		UInteger32
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION	"Temperature sensor id"
::= { rsshtp1WEntry 1 }

rsshtp1WName OBJECT-TYPE
    	SYNTAX      OCTET STRING
    	MAX-ACCESS  read-write
    	STATUS      current
    	DESCRIPTION "Name (max 20)"
::= { rsshtp1WEntry 2 }

rsshtp1WTemp		OBJECT-TYPE
	SYNTAX		INTEGER
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION	"Temperature value"
::= { rsshtp1WEntry 3 }

rsshtp1WMaster		OBJECT-TYPE
	SYNTAX		OCTET STRING
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION	"Name of the SNR-RSsensor-H/T/P 
which this temperature sensor 
is connected to"
::= { rsshtp1WEntry 4 }

tempCritNotif	OBJECT-TYPE
	SYNTAX		INTEGER
		{
				No	(0),
				Yes	(1),
		}
        MAX-ACCESS	read-write
        STATUS		current
        DESCRIPTION	"Enable notifications on the critical temperature"
::= { rsshtp1WEntry 10 }
	
tempCritMin		OBJECT-TYPE
	SYNTAX		INTEGER
        MAX-ACCESS	read-write
        STATUS		current
        DESCRIPTION	"Minimal critical temperature. 
Up to -55 °C"
::= { rsshtp1WEntry 15 }

tempCritMax	OBJECT-TYPE
	SYNTAX		INTEGER
        MAX-ACCESS	read-write
        STATUS		current
        DESCRIPTION	"Maximum critical temperature. 
Up to +125°C"
::= { rsshtp1WEntry 16 }

-- dio

diTable			OBJECT-TYPE
	SYNTAX		SEQUENCE OF diEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION	"A list of digital inputs values"
::= { dio 1 }

diEntry 		OBJECT-TYPE
	SYNTAX		diEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION	"An entry (conceptual row) 
in the diTable"
::= { diTable 1 }

diEntry ::= SEQUENCE 
{
	diName		OctetString,
    diAlarmName	OctetString,
	diState		Integer,
	diCnt		Counter
}

diName			OBJECT-TYPE
	SYNTAX		OCTET STRING
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION	"Digital input name"
::= { diEntry 1 }

diAlarmName		OBJECT-TYPE
	SYNTAX		OCTET STRING
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION	"Alarm name"
::= { diEntry 2 }

diState			OBJECT-TYPE
	SYNTAX		INTEGER
			{
				low	(0),
				high	(1),
				off	(2)
			}
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION	"Digital input state"
::= { diEntry 3 }

diCnt			OBJECT-TYPE
	SYNTAX		Counter
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION	"Digital input impulse counter"
::= { diEntry 4 }


doTable			OBJECT-TYPE
	SYNTAX		SEQUENCE OF doEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION	"A list of digital outputs values"
::= { dio 2 }

doEntry 		OBJECT-TYPE
	SYNTAX		doEntry
	MAX-ACCESS	not-accessible
	STATUS		current
	DESCRIPTION	"An entry (conceptual row) 
in the doTable"
::= { doTable 1 }

doEntry ::= SEQUENCE 
{
	doName			OctetString,
	doDeviceName	OctetString,
	doState			Integer,
	doResetTime		Integer
}

doName			OBJECT-TYPE
	SYNTAX		OCTET STRING
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION	"Digital output name"
::= { doEntry 1 }

doDeviceName	OBJECT-TYPE
	SYNTAX		OCTET STRING
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION	"Digital output custom name"
::= { doEntry 2 }

doState			OBJECT-TYPE
	SYNTAX		INTEGER
			{
				off	(0),
				on	(1),
				reload	(2)
			}
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION	"Digital output state"
::= { doEntry 3 }

doResetDelay		OBJECT-TYPE
	SYNTAX		INTEGER
	MAX-ACCESS	read-write
	STATUS		current
	DESCRIPTION	"Reload period (sec)"
::= { doEntry 4 }

uSenseState		OBJECT-TYPE
	SYNTAX		INTEGER
			{
				off	(0),
				on	(1)
			}
        MAX-ACCESS	read-only
        STATUS		current
        DESCRIPTION	"Voltage sensor state"
::= { dio 3 }

-- GSM

GsmModuleStatus		OBJECT-TYPE
	SYNTAX		INTEGER
			{
				No	(0),
				Yes	(1),
				NoSim	(2),
				Error	(3),
				Connected	(4)
			}
        MAX-ACCESS	read-only
        STATUS		current
        DESCRIPTION	"the status of the gsm module"
::= { GSM 1 }

GsmStrength		OBJECT-TYPE
	SYNTAX		INTEGER
        MAX-ACCESS	read-only
        STATUS		current
        DESCRIPTION	"the level of signal in dBm"
::= { GSM 2 }

ReconnCount		OBJECT-TYPE
	SYNTAX		INTEGER
        MAX-ACCESS	read-only
        STATUS		current
        DESCRIPTION	"the number of connection attempts"
::= { GSM 10 }

-- RF

RfModuleStatus		OBJECT-TYPE
	SYNTAX		INTEGER
			{
				No	(0),
				Yes	(1)
			}
        MAX-ACCESS	read-only
        STATUS		current
        DESCRIPTION	"the status of the rf module"
::= { RF 1 }

-- options

dataType		OBJECT-TYPE
	SYNTAX		INTEGER
			{
				integer	(0),
				float	(1),
				ufloat	(2)
			}
        MAX-ACCESS	read-write
        STATUS		current
        DESCRIPTION	"Values data type"
::= { options 1 }

-- crit

tempCritDHT		OBJECT-TYPE
	SYNTAX		INTEGER
        MAX-ACCESS	read-write
        STATUS		current
        DESCRIPTION	"Critical temperature. 
From -55 to +125°C"
::= { crit 10 }

humCrit		OBJECT-TYPE
	SYNTAX		INTEGER
        MAX-ACCESS	read-write
        STATUS		current
        DESCRIPTION	"Critical humidity. 
From 0 to 100%"
::= { crit 20 }

adcCritMin		OBJECT-TYPE
	SYNTAX		INTEGER
        MAX-ACCESS	read-write
        STATUS		current
        DESCRIPTION	"ADC IN critical min"
::= { crit 30 }

adcCritMax		OBJECT-TYPE
	SYNTAX		INTEGER
        MAX-ACCESS	read-write
        STATUS		current
        DESCRIPTION	"ADC IN critical max"
::= { crit 31 }

adcHysteresis	OBJECT-TYPE
	SYNTAX		INTEGER
        MAX-ACCESS	read-write
        STATUS		current
        DESCRIPTION	"ADC IN hysteresis"
::= { crit 35 }

-- diffparams

-- upsStatus

statusUPS		OBJECT-TYPE
	SYNTAX		INTEGER
			{
				fail	(1),
				ok	(0),
				unknown	(2) 
			}
        MAX-ACCESS	read-only
        STATUS		current
        DESCRIPTION	"UPS status"
::= { upsStatus 1 }

batteryVoltageUPS	OBJECT-TYPE
	SYNTAX		INTEGER
        MAX-ACCESS	read-only
        STATUS		current
        DESCRIPTION	"Battery voltage value"
::= { upsStatus 2 }

temperatureUPS		OBJECT-TYPE
	SYNTAX		INTEGER
	MAX-ACCESS	read-only
	STATUS		current
	DESCRIPTION	"Temperature value"
::= { upsStatus 3 }

inputVoltageUPS		OBJECT-TYPE
	SYNTAX		INTEGER
        MAX-ACCESS	read-only
        STATUS		current
        DESCRIPTION	"Input voltage value"
::= { upsStatus 4 }

outputVoltageUPS	OBJECT-TYPE
	SYNTAX		INTEGER
        MAX-ACCESS	read-only
        STATUS		current
        DESCRIPTION	"Output voltage value"
::= { upsStatus 5 }

currentUPS		OBJECT-TYPE
	SYNTAX		INTEGER
        MAX-ACCESS	read-only
        STATUS		current
        DESCRIPTION	"Current value"
::= { upsStatus 6 }

lastBatteryChangeUPS	OBJECT-TYPE
	SYNTAX		OCTET STRING
        MAX-ACCESS	read-only
        STATUS		current
        DESCRIPTION	"Last battery change date and time. 
APC only"
::= { upsStatus 7 }


-- pid

inputPID		OBJECT-TYPE
	
	SYNTAX		INTEGER
        
	MAX-ACCESS	read-write

        STATUS		current

        DESCRIPTION	"PID SNMP input value"

::= { pid 1 }


	
outputPercentPID	OBJECT-TYPE

	SYNTAX		INTEGER

        MAX-ACCESS	read-only

        STATUS		current

        DESCRIPTION	"PID output value. 
0 to 100%"

::= { pid 2 }



outputRealPID		OBJECT-TYPE

	SYNTAX		INTEGER

        MAX-ACCESS	read-only

        STATUS		current

        DESCRIPTION	"PID output value 
(voltage if PID runs in analog mode 
or time if PID runs in PWM mode)"

::= { pid 3 }



ypPID			OBJECT-TYPE

	SYNTAX		INTEGER

        MAX-ACCESS	read-only

        STATUS		current

        DESCRIPTION	"Proportional gain"

::= { pid 4 }



yiPID			OBJECT-TYPE

	SYNTAX		INTEGER

        MAX-ACCESS	read-only

        STATUS		current

        DESCRIPTION	"Integral gain"

::= { pid 5 }



ydPID			OBJECT-TYPE

	SYNTAX		INTEGER

        MAX-ACCESS	read-only

        STATUS		current

        DESCRIPTION	"Derivative gain"

::= { pid 6 }



errorPID		OBJECT-TYPE

	SYNTAX		INTEGER

        MAX-ACCESS	read-only

        STATUS		current

        DESCRIPTION	"Error. Difference between setpoint 
and input value"

::= { pid 7 }


-- Traps

DI1Alarm		NOTIFICATION-TYPE
	STATUS		current
	DESCRIPTION	"Input 1 Alarm fires"		
::= { traps 1 }

DI1Release		NOTIFICATION-TYPE
	STATUS		current
	DESCRIPTION	"Input 1 Alarm released"		
::= { traps 2 }

DI2Alarm		NOTIFICATION-TYPE
	STATUS		current
	DESCRIPTION	"Input 2 Alarm fires"		
::= { traps 3 }

DI2Release		NOTIFICATION-TYPE
	STATUS		current
	DESCRIPTION	"Input 2 Alarm released"		
::= { traps 4 }

DI3Alarm		NOTIFICATION-TYPE
	STATUS		current
	DESCRIPTION	"Input 3 Alarm fires"		
::= { traps 5 }

DI3Release		NOTIFICATION-TYPE
	STATUS		current
	DESCRIPTION	"Input 3 Alarm released"		
::= { traps 6 }

DI4Alarm		NOTIFICATION-TYPE
	STATUS		current
	DESCRIPTION	"Input 4 Alarm fires"		
::= { traps 7 }

DI4Release		NOTIFICATION-TYPE
	STATUS		current
	DESCRIPTION	"Input 4 Alarm released"		
::= { traps 8 }

DI5Alarm		NOTIFICATION-TYPE
	STATUS		current
	DESCRIPTION	"Input 5 Alarm fires"		
::= { traps 9 }

DI5Release		NOTIFICATION-TYPE
	STATUS		current
	DESCRIPTION	"Input 5 Alarm released"		
::= { traps 10 }

uSenseAlarm		NOTIFICATION-TYPE
	STATUS		current
	DESCRIPTION	"Signifies that Phase sensor 
Alarm fires"		
::= { traps 11 }

uSenseRelease	NOTIFICATION-TYPE
	STATUS		current
	DESCRIPTION	"Signifies that Phase sensor 
Alarm released"		
::= { traps 12 }

reloutOn		NOTIFICATION-TYPE
	STATUS		current
	DESCRIPTION	"Signifies that Rele was swithed on 
by Thermostat or Gigrostat mode"		
::= { traps 13 }

reloutOff		NOTIFICATION-TYPE
	STATUS		current
	DESCRIPTION	"Signifies that Rele was swithed off 
by Thermostat or Gigrostat mode"		
::= { traps 14 }

DO1On			NOTIFICATION-TYPE
	STATUS		current
	DESCRIPTION	"Signifies that Output 1 was swithed on 
by Thermostat or Gigrostat mode"		
::= { traps 15 }

DO1Off			NOTIFICATION-TYPE
	STATUS		current
	DESCRIPTION	"Signifies that Output 1 was swithed off 
by Thermostat or Gigrostat mode"		
::= { traps 16 }

DO2On			NOTIFICATION-TYPE
	STATUS		current
	DESCRIPTION	"Signifies that Output 2 was swithed on 
by Thermostat or Gigrostat mode"		
::= { traps 17 }

DO2Off			NOTIFICATION-TYPE
	STATUS		current
	DESCRIPTION	"Signifies that Output 2 was swithed off 
by Thermostat or Gigrostat mode"		
::= { traps 18 }

DO3On			NOTIFICATION-TYPE
	STATUS		current
	DESCRIPTION	"Signifies that Output 3 was swithed on 
by Thermostat or Gigrostat mode"		
::= { traps 19 }

DO3Off			NOTIFICATION-TYPE
	STATUS		current
	DESCRIPTION	"Signifies that Output 3 was swithed off 
by Thermostat or Gigrostat mode"		
::= { traps 20 }

DO4On			NOTIFICATION-TYPE
	STATUS		current
	DESCRIPTION	"Signifies that Output 4 was swithed on 
by Thermostat or Gigrostat mode"		
::= { traps 21 }

DO4Off			NOTIFICATION-TYPE
	STATUS		current
	DESCRIPTION	"Signifies that Output 4 was swithed off 
by Thermostat or Gigrostat mode"		
::= { traps 22 }

DO5On			NOTIFICATION-TYPE
	STATUS		current
	DESCRIPTION	"Signifies that Output 5 was swithed on 
by Thermostat or Gigrostat mode"		
::= { traps 23 }

DO5Off			NOTIFICATION-TYPE
	STATUS		current
	DESCRIPTION	"Signifies that Output 5 was swithed off 
by Thermostat or Gigrostat mode"		
::= { traps 24 }

tempSensorAlarm		NOTIFICATION-TYPE
	STATUS			current
	DESCRIPTION		"Temperature alarm"		
::= { traps 29 }

tempSensorRelease	NOTIFICATION-TYPE
	STATUS			current
	DESCRIPTION		"Temperature release"		
::= { traps 30 }

adcSensorAlarm		NOTIFICATION-TYPE
	STATUS			current
	DESCRIPTION		"Voltage sensor alarm"		
::= { traps 31 }

adcSensorRelease	NOTIFICATION-TYPE
	STATUS		current
	DESCRIPTION	"Voltage sensor release"		
::= { traps 32 }

humSensorAlarm		NOTIFICATION-TYPE
	STATUS			current
	DESCRIPTION		"Humidity alarm"		
::= { traps 33 }

humSensorRelease	NOTIFICATION-TYPE
	STATUS			current
	DESCRIPTION		"Humidity release"		
::= { traps 34 }

task1Done		NOTIFICATION-TYPE
	STATUS		current
	DESCRIPTION	"Task 1 done"		
::= { traps 36 }

task2Done		NOTIFICATION-TYPE
	STATUS		current
	DESCRIPTION	"Task 2 done"		
::= { traps 37 }

task3Done		NOTIFICATION-TYPE
	STATUS		current
	DESCRIPTION	"Task 3 done"		
::= { traps 38 }

task4Done		NOTIFICATION-TYPE
	STATUS		current
	DESCRIPTION	"Task 4 done"		
::= { traps 39 }

pingLost		NOTIFICATION-TYPE
	STATUS		current
	DESCRIPTION	"Ping lost"		
::= { traps 45 }

batteryChargeLow	NOTIFICATION-TYPE
	STATUS			current
	DESCRIPTION		"Battery charge is low"		
::= { traps 47 }

upsUtilityFail		NOTIFICATION-TYPE
	STATUS			current
	DESCRIPTION		"UPS utility fail"		
::= { traps 50 }

upsUtilityOk		NOTIFICATION-TYPE
	STATUS			current
	DESCRIPTION		"UPS utility OK"		
::= { traps 51 }

-- erd4Group

erd4Group		NOTIFICATION-GROUP  
	NOTIFICATIONS 
	{
		DI1Alarm,
		DI1Release,
		DI2Alarm,
		DI2Release,
		DI3Alarm,
		DI3Release,
		DI4Alarm,
		DI4Release,
		DI5Alarm,
		DI5Release,
		uSenseAlarm,
		uSenseRelease,
		reloutOn,
		reloutOff,
		DO1On,
		DO1Off,
		DO2On,
		DO2Off,
		DO3On,
		DO3Off,
		DO4On,
		DO4Off,
		DO5On,
		DO5Off,
		tempSensorAlarm,
		tempSensorRelease,
		adcSensorAlarm,
		adcSensorRelease,
		humSensorAlarm,
		humSensorRelease,
		task1Done,
		task2Done,
		task3Done,
		task4Done,
		pingLost,
		batteryChargeLow,
		upsUtilityFail,
		upsUtilityOk
	}
	STATUS			current
	DESCRIPTION		"Notifications"
::= { snr-erd-4 99 }

END
