This is the Intel(R) RSTe 4.7 PV F6 installation and driver zip files.
The contents of this zip file include the F6 installation drivers and the standard OS drivers to
support manual driver installation activities.  The following are the directories and their 
contents included in RSTe_4.7.0.xxx_F6-drivers.zip:

iaStorA.free.win7.32bit.4.7.0.xxxx   – The 32 bit ACHI drivers for Windows 7.
iaStorA.free.win7.64bit.4.7.0.xxxx   – The 64 bit ACHI drivers for Windows 7 and Windows Server 2008 R2.
iaStorA.free.win8.32bit.4.7.0.xxxx   – The 32bit AHCI drivers for Windows 8.1 and Windows 10-RS2
iaStorA.free.win8.64bit.4.7.0.xxxx   – The 64 bit AHCI drivers for Windows 8.1/ Windows 10RS2 /Server 2012/Server 2012 R2/Server 2016.


The same driver version applies to the drivers for manual installation.

For further questoins, please contact you Intel FAE.
