V707R302C001
ADD|recommended FW

V707R302C000B002
FIX|CRM20250819033947 issue with traffic forwarding in a VxLAN-network when a static route is configured in some cases

V707R302C000B001
FIX|CRM20250723032922 issue with DHCP packets reach the CPU via L3 routing

V707R301C011B008
FIX|CRM20250520030808 issue with lack of multicast streams forwarding to Mrouter-port (according to RFC 4541)

V707R301C011
ADD|recommended FW
FIX|CRM20250506030373 issue with replacing VLAN MAC with CPU MAC in option of DHCP messages

V707R301C009
FIX|CRM20250304028293 issue with incorrect TCAM utilization

V707R301C007B001
FIX|CRM20250207027664 issue with high fanspeed on auto mode

V707R301C007
FIX|CRM20250123027499 recommended FW
FIX|CRM20241204026044 issue with fanspeed periodically changing with no reason
FIX|CRM20241121025476 incorrect working of the command 'switchport mode trunk allow-null'
ADD|CRM20240910023602 add password encryption for archive command at running config
FIX|CRM20240710022146 issue with DHCP packets are transmitted between isolated ports
ADD|CRM20230418014019 add IP SLA (NQA) function
ADD|CRM20240704021993 add opportunity to check advertised/received routes via BGP at VRF
FIX|CRM20240515020729 add command 'clear arp-cache static [vlanid <VID>]' to clear static ARP-records
FIX|CRM20240607021322 issue with configuration 'ip default-gateway'
FIX|CRM20240520020832 issue with Dynamic ARP Inspection and isolation port
FIX|CRM20240515020730 issue with routing packet which should be encapsulated in a multicast Ethernet frame according to static-multicast ARP-record (required command: 'no arp check')
FIX|CRM20240702021940 issue with accidental reboot after configuration router bgp in some cases
