V707R401C006B009
FIX|CRM20260430044802 improve compatibility of ZTP operation

V707R401C006B007
ADD|CRM20260413043932 remove limitation of file extension for configuration of DHCP option Bootfile

V707R401C006B004
FIX|CRM20260319042805 add command 'bgp log-neighbor-changes' (BGP configuration mode) to enable logging of changes between BGP states

V707R401C006B003
FIX|CRM20260320042860 issue with statistics of interface NVE
FIX|CRM20260414043998 issue with EVPN/VxLAN tunnels in case of a few tunnel interfaces

V707R401C006B001
ADD|CRM20260121040722 add remarks for named ACL 
ADD|CRM20260205041406 add command 'alias exec <Alias> <Command>' with the ability to create up to 256 aliases for commands 

V707R401C004B013
ADD|CRM20250721032841 add support for 2,5G speed on SFP+ ports ('force2500m-full')
ADD|CRM20251010035990 add command "info-center format rfc5424" to change syslog message format to RFC 5424 standard

V707R401C004B011
FIX|CRM20260211041687 issue with incorrect formation of UDP Payload when transferring files via the TFTP
FIX|CRM20260126040878 issue with DHCP relay ignoring unicast flag in DHCP packets

V707R401C004B010
FIX|CRM20260210041615 add missing punctuation marks to the interface information output

V707R401C004B008
FIX|CRM20260213041757 issue with tUsrRoot task in some cases of Fan-out port mode configuration

V707R401C004B004
FIX|CRM20260122040782 issue with switch hanging in some cases when a large number of VLANs are created

V707R401C004B003
ADD|CRM20260121040718 add new OIDs for flood-control in branch .priPortEntry (1.3.6.1.4.1.40418.7.100.3.2.1)

V707R401C004
ADD|recommended FW

V707R401C003B020
FIX|CRM20251226039592 issue with incorrect temperature values in some cases

V707R401C003B019
FIX|CRM20251128038171 add command 'mls qos burst-mode (dynamic | standard)' to select the buffer allocation mechanism

V707R401C003B016
ADD|CRM20251112037374 add tcpdump function from CPU (command branch in enable mode: 'capture ...')

V707R401C003B012
FIX|CRM20251211038786 issue with starting OSPFv3 neighborship when a large number of routes are transmitted
FIX|CRM20251128038180 remove unsupported counters from interface statistic

V707R401C003B010
FIX|CRM20251125038017 add the 'hardware tunnel-capacity <0-2048>' command to expand the number of routes as FEC 

V707R401C003B009
FIX|CRM20250930035839 automatically send a BGP Route-refresh when the associated Route-map changes
FIX|CRM20251021036430 issue with error in tasks checkTask and tftpCopyFile in some cases

V707R401C003B008
FIX|CRM20251105037087 issue with switch rebooting by error in task "zL2_shell" in some cases (one more case)
FIX|CRM20250901034524 add WRR algorithm for QoS

V707R401C003B002
FIX|CRM20251007035910 issue with switch rebooting by error in task "zL2_shell" in some cases

V707R401C003B001
FIX|CRM20250820034001 issue with incorrect output of 'show l3-table' 

V707R401C002B001
FIX|CRM20250717032661 issue with drops related to L3 MTU in some cases

V707R401C000B000
FIX|CRM20250610031459 change FW version from V707R301CxxxBxxx to V707R401CxxxBxxx

V707R301C011B009
ADD|CRM20250610031459 add MTU configuration to port configuration mode

V707R301C011B008
FIX|CRM20250520030808 issue with lack of multicast streams forwarding to Mrouter-port (according to RFC 4541)

V707R301C011
ADD|recommended FW
FIX|CRM20250506030373 issue with replacing VLAN MAC with CPU MAC in option of DHCP messages

V707R301C010
FIX|CRM20250521030818 switch stuck by LED SHUTOFF task afterwards 8-12 weeks since startup 

V707R301C009B002
FIX|CRM20250507030410 issue with drop packets with ttl=1 when mc-lag is configured

V707R301C009
FIX|CRM20250304028293 issue with incorrect TCAM utilization

V707R301C007
FIX|CRM20250123027499 recommended FW
FIX|CRM20241204026044 issue with fanspeed periodically changing with no reason
FIX|CRM20241121025476 incorrect working of the command 'switchport mode trunk allow-null'
ADD|CRM20240910023602 add password encryption for archive command at running config
FIX|CRM20240710022146 issue with DHCP packets are transmitted between isolated ports
ADD|CRM20230418014019 add IP SLA (NQA) function
ADD|CRM20240704021993 add opportunity to check advertised/received routes via BGP at VRF
FIX|CRM20240515020729 add command 'clear arp-cache static [vlanid <VID>]' to clear static ARP-records
FIX|CRM20240607021322 issue with configuration 'ip default-gateway'
FIX|CRM20240520020832 issue with Dynamic ARP Inspection and isolation port
FIX|CRM20240515020730 issue with routing packet which should be encapsulated in a multicast Ethernet frame according to static-multicast ARP-record (required command: 'no arp check')
FIX|CRM20240702021940 issue with accidental reboot after configuration router bgp in some cases
