V705R203C001B013
FIX|CRM20230428014149 fail to config ipv6 ospf network point-to-point

﻿V705R203C001B012
FIX|CRM20230411013951 issue with dst cache overflow in some cases

﻿V705R203C001B011
FIX|CRM20230329013788 issue with USB-port

﻿V705R203C001B010
ADD|CRM20221213012751 add arbitrary UDP-port for syslog

﻿V705R203C001B008
FIX|CRM20230313013556 Switch become unavailable out of cache overflow

V705R203C001B006
ADD|CRM20221216012772 Validity Management of Switch Passwords
ADD|CRM20221220012792 Feature with automatic restart when the switch temperature is too low or too high

V705R203C001B005
ADD|CRM20221216012774 Switch web import SSL certificate

﻿V705R203C001B004
FIX|CRM20230209013216 high cpu utilization due to the inefficient interaction between the switch and CPU

7.6.3.2(R0005.0085)
FIX|CRM20221013012155 issue with BFD on loopback ports

﻿7.6.3.2(R0005.0084)
FIX|CRM20221024012254 issue with radius auth on Windows client

﻿7.6.3.2(R0005.0083)
ADD|CRM20220721011329 An possibility to use more stronger algorithms with 'service password-encryption'
ADD|CRM20220816011606 Add VRRP plaintext authentication

7.6.3.2(R0005.0082)
FIX|CRM20221024012259 issue with copy running config via FTP, SFTP

7.6.3.2(R0005.0081)
FIX|CRM20221020012221 issue with snmpwalk output for snmpv3

7.6.3.2(R0005.0079)
ADD|CRM20220719011297 Adjust the VRF quantity to 1024

﻿7.6.3.2(R0005.0078)
ADD|CRM20211215008619 add command "show vsf config detail" 
FIX|CRM20211207008506 show transceiver detail |load balancing algorithm problem |VSF flow problem
