Here is UPS SafeMate help doc and comment(version and other).

/*==================English Readme==============================*/
1.Software  installation and operation
i) soft installation
	copy the package ups_manager to you favorite directory , example :/root/tmp
                 Use the tar command to extract files from the diskette or software package:  
                        tar -xzvf  safemate1.0v.linux.tar.gz
                 Change the working directory to /tmp. 
                         cd /root/tmp
                 Execute the installation program:
                         ./install.linux.sh
                The installation program will not execute in some shell scripts. If this happens, change to another shell script and  try again.
                the installation program  will automatically copy files to the default location   "/etc/RichComm/ups_manager/" and modify the system startup file to contain the 
                ups_manager for UNIX daemon process. 
        ii) start program 
                The installation program        will automatically start the main program . 
                 you can start it use following command:
                        ./ups_netcomm start
        iii) stop program
                 you can start it use following command:
                ./ups_netcomm stop
        iv) config program
                 you can start it use following command:
                ./ups_config
2.software package 
./ups_netcomm
./ups_status
./ups_config
./shutdown.sh
./ups_netcomm
./ups_netcomm start                                    Star Monitor
./ups_netcomm stop                                     Stop Monitor
./ups_config				                           Config System
./ups_status										   Look State
./TimeCfg.conf
./install.linux.sh
./Readme
./SendMSG.sh
./startup.add

3.contact us and technical support
