EMR3.0 Management

Muxing Setting > Program Muxing >
Backup Parameters

- Backup Switch:

- Current State: Main

Backup Program (Note:If the main program and the backup program has the same PCR,that require they must be homogenous!)

Program | Card | Port | Program No | Sevice Name | Current Bitrate | Bitrate Upper Limit(Kbps) | Bitrate Lower Limit(Kbps)
--- | --- | --- | --- | --- | --- | --- | ---
Main | ... | ... | Program... | ... | ... |  |
Backup |  |  |  |  |  |  |