EMR3.0 Management

Cards >

- Card Parameter
- Port Parameter

Param Set

- Alarm Switch:

- Card Function:

Port Setting

- Port 1:
- Port 3:
- Port 5:

- Port 2:
- Port 4:

Decon. Status Info

- Sync Status:

- Input Bitrate:

Decon. Param Set

- Input Source Select:
- Alarm Switch:

- Input Packet Length:

Con. Param Set

- Output Bitrate(bps):
- Suggest Mux Delay(us):

- Output Packet Length:
- Output Mux Delay(us):