EMR3.0 Management

Cards >

- Card Set
- Port Param

Video Param

- Time Statistic:

- Video On/Off:
- Rate Control:
- Brightness:
- Contrast:
- Saturation:
- Chroma:
- Video Select:
- Video Rate:
- Input Resolution:

- GOP Struct:
- Scan Style:
- Output Resolution:
- Aspect Ratio:
- Video Pattern:
- Encoder Switch:
- Profile:
- Level:
- Time Clear:

Audio Param

- Audio On/Off:
- Audio Select:
- Audio Rate:
- Volume:

- Audio Standard:
- Track Style:
- Sampling Freq:
- Embedded Chan:

TS Info

- Program No:
- Service Name:
- Service Provider:
- PMT PID:

- PCR PID:
- Video PID:
- Audio PID: