TANTRAX

Cards >

- Card Set
- Port1
- Port2

- Alarm Switch:

Video Parameter

- Video Switch:
- Video Pattern:
- Video Bitrate Control:
- Video Bitrate(bps):
- Avg VBR Rate(bps):

- GOP Structure:
- GOP Size:
- Aspect Ratio:
- Video Resolution:
- Video No Input Out:

Audio Parameter

- MP2 Audio Switch:
- MP2 Audio Input:
- MP2 Audio Mode:
- MP2 Volume Level:
- MP2 Audio Rate:
- MP2 Audio Samplerate:
- Embedded Channel Sel:
- Audio No Input Out:

- AC3 ENC Switch:
- AC3 Audio Input:
- AC3 Audio Mode:
- AC3 Volume Level:
- AC3 Audio Rate:
- AC3 Audio Samplerate:
- AC3 ENC Delay(ms):

- DRA Encode Switch:
- DRA Audio Input:
- DRA Audio Mode:
- DRA Audio Rate:
- DRA Audio Samplerate:
- DRA ENC Delay(ms):

TS Stream Set

- Multiplex Switch:
- Program No:
- Service Name:
- Service Provide:
- PCR PID:

- PMT PID:
- Video PID:
- MPEG2 Audio PID:
- AC3 Audio PID:
- DRA Audio PID:

VBI Parameter

- TT Switch:
- TT PID:
- CC Switch:
- CC Field2 Switch:

- CC Field1 Switch:
- Field1 Line Num:
- Field2 Line Num: