TANTRAX

Cards >

- Receive Set
- Card Param
- Status Info

Card Set

- Interface Sel:

- PCR Correct:

Input Channel Backup

- Channel Rate Limit(Mbps):

- Main Prior:

Gbe1 Parameters

- IP Address:
- Gateway:
- Interface Type:
- SFP Impedance:
- Alarm Switch:

- Subnet Mask:
- MAC Address: mac
- MDI Mode:
- SFP Out Amp:

Gbe2 Parameters

- IP Address:
- Gateway:
- Interface Type:
- SFP Impedance:
- Alarm Switch:

- Subnet Mask:
- MAC Address: mac
- MDI Mode:
- SFP Out Amp: