EMR3.0 Management

Cards >

- Card Set
- Port 1
- Port 2

Video Param

- Video Info:

- Time Statistics:

- Rate Control:
- Video Rate(bps):
- Scan Style:
- Resolution:

- GOP Struct:
- Time Clear:
- Work Mode:

Audio Param

- Audio1 Info:
- Audio2 Info:

- Audio1 Delay(ms):
- Audio2 Delay(ms):
- Audio Select:
- Embedded Chan:

- Audio Rate:
- Volume:
- Audio Standard:
- Track Style:

TS Info

- Program No:
- Service Name:
- Service Provider:
- PMT PID:

- PCR PID:
- Video PID:
- Audio1 PID:
- Audio2 PID: