EMR3.0 Management

Cards > card7--Main Gbe Card > Receive Set > Gbe3

- Receive Set
- Transmit Set
- Card Param
- ARP Param
- Backup Param
- Status Info

- GBE1
- GBE2
- GBE3
- GBE4

Port Display:

| Port | Basic Param | Expand Param
--- | --- | --- | ---
Receive IP | Recv Port | Alarm Switch | Recv Mode | Source IP1 | Source IP2 | Protocol | Ref Switch | Ref Bitrate(bps)

Add Port

Add Port Num : |  | at most ports
Receive IP : |  | A.B.C.D
IP Step Value : |  | step value of part D
Receive Port : |  |
Port Step Value : |  | step value of rec port
Alarm Switch : |  | port alarm switch
Receive Mode : |  | IGMP V3 receive mode
Source IP1 : |  | IGMP V3 source IP1
Source IP2 : |  | IGMP V3 source IP2
NTP : |
Ref Bitrate(bps) : |  | IP input ref bitrate
Ref Switch : |  | IP input ref switch

Batch Modify

Receive IP : |  |
Receive IP Step : |
Receive Port : |  |
Alarm Switch : |  |
Receive Mode : |  |
Source IP1 : |  |
Source IP2 : |  |
NTP : |  |
Ref Switch : |  |
Ref Bitrate(bps) : |  |