EMR3.0 Management

Cards >

- Param Setting
- Status Info

Card Setting

- Alarm Switch:

Modulation Setting

- Input Source:
- Modulation Standard:
- FEC Rate & Constellation:
- Constellation Amplitude Normalization:
- FEC-Frame Type:

- Base Band Process:
- Reference Clock:
- Pilot Switch:
- Spectrum Inversion:
- Roll-off Factor:

Output Setting

- Symbol Rate(Ksps):
- Output Frequency(KHz):

- Output Level(dBuV):
- RF Output Switch:

Updating now,please wait. . .