EMR3.0 Management

Cards > card7--Main Gbe Card > Backup Param > Input GBE backup

- Receive Set
- Transmit Set
- Card Param
- ARP Param
- Backup Param
- Status Info

- Input GBE backup
- Output GBE backup
- Output port backup

GBE1 Parameters

- Backup Switch:
- Backup Mode:

- Switching Condition:
- Min Effective Rate threshold(bps):
- Max Effective Rate threshold(bps):

GBE2 Parameters

- Backup Switch:
- Backup Mode:

- Switching Condition:
- Min Effective Rate threshold(bps):
- Max Effective Rate threshold(bps):

GBE3 Parameters

- Switching Condition:

- Min Effective Rate threshold(bps):
- Max Effective Rate threshold(bps):

GBE4 Parameters

- Switching Condition:

- Min Effective Rate threshold(bps):
- Max Effective Rate threshold(bps):