TANTRAX

Cards >

- Receive Set
- Card Param
- Status Info

- GBE1
- GBE2

| Port | Basic Param | Expand Param
--- | --- | --- | ---
Receive IP | Recv Port | Alarm Switch | Recv Mode | Source IP1 | Source IP2 | Ref Switch | Ref Bitrate(bps) | Specified PID

Batch Modify

Receive IP : |  |
Receive Port : |  |
Alarm Switch : |  |
Receive Mode : |  |
Source IP1 : |  |
Source IP2 : |  |
Ref Switch : |  |
Ref Bitrate(bps) : |  |
Specified PID : |  |