EMR3.0 Management

Cards >

- Card Set
- Port 1
- Port 2

- Status Info
- Parameter Set

Decode Set

- Decode Switch:
- Sync Mode:
- SDI Out Select:
- Error Handle:

- CC Switch:
- CC Delay(frame):
- CC Line Num(line):

Decode Program Set

- PID Mode:
- Program Select:
- Decode PCR PID:

- Decode Video PID:
- Decode Audio PID:
- Teletext PID:

Video Decode Set

- Video Pattern:
- Aspect Ratio:

- Image Scaling:

Audio Decode Set

- Output Mute:
- Vol Attenuation(dB):

- Audio Mode:
- Embedded Mode: