TANTRAX

Cards >

- ASI Param.
- DS3 Param.

In Param.

- Loop Switch:
- DS3/E3 Switch Mode:
- Frame Format:
- RS Decode Switch:
- DeInterla Switch:
- Descramble Switch:
- PID Set:

- Input Switch:
- Multi Protocol:
- Bit Sequence:
- TS Pkt Length:
- In Sys Rate:
- In Val Rate:
- PID Set Rate:

Out Param.

- Out Pkt Length:
- Out Bit Sequence:
- Frame Format:
- Scramble Switch:

- EnInterla Switch:
- RS Encode Switch:
- Out Valid Rate: