EMR3.0 Management

Cards >

- Card Set
- Port 1
- Port 2

VideoEncode Information

- Video Information:

- Video On/Off:
- Video Bitrate(bps):
- Video Input:
- Output Resolution:
- Profile:
- Level:
- Aspect Ratio:

- GOP Structure:
- GOP Size:
- IDR Frequency(GOPs):
- Entropy Coding:
- OP Video Loss:
- Test Pattern:

AudioEncode Information 1

- Audio Information:

- Audio Status:
- Audio Encoding Type:
- L R Channel:
- Audio Bitrate:

- Volume:
- Mode:
- Delay(ms):

AudioEncode Information 2

- Audio Information:

- Audio Status:
- Audio Encoding Type:
- L R Channel:
- Audio Rate:

- Volume:
- Mode:
- Delay(ms):

TS Information

- Program No.:
- Service Name:
- Service Provider:
- PMT PID:

- PCR PID:
- Video PID:
- Audio 1 PID:
- Audio 2 PID:

Text Information

- Start PosX:

- Start PosY:

- Text Content: