EMR3.0 Management

Muxing Setting > Program Muxing >
PSI/SI Set

Source Card | Source Port | Source PID | Current PID | PID Type
--- | --- | --- | --- | ---

Service Info

- Service Identifier:
- Service Name:
- Provider Name:
- EIT Schedule Flag:
- EIT Present Following Flag:

- Character Encoding:
- Service Type:
- Custom Type:
- Running Status:
- Encryption Status:

Service Info

- Service Identifier:
- Service Name:
- Maj_Channel:
- Min_Channel:

- Channel_TSID:
- Service Type:
- Modulation_Mode:
- Program_Source: