EMR3.0 Management

General

- Alarm:

Video

- Switch:
- Format:
- Bitrate Mode:
- Bitrate (bps):
- VBR (bps):

- GOP Structure:
- GOP Size:
- Aspect Ratio:
- Resolution:
- No Source Control:

Audio

- Embedded Channel:
- No Source Control:
- MP2 Coding:
- MP2 Input:
- MP2 Mode:
- MP2 Volume:
- MP2 Bitrate:
- MP2 Sample Rate:
- Digital Sample Rate:

- AC3 Coding:
- AC3 Input:
- AC3 Mode:
- AC3 Volume:
- AC3 Bitrate:
- AC3 Sample Rate:
- AC3 Coding Delay (ms):
- Embeded Sample Rate:

- DRA Coding:
- DRA Input:
- DRA Mode:
- DRA Bitrate:
- DRA Sample Rate:
- DRA Coding Delay (ms):
- Embeded Sample Rate:

TS

- Multiplex:
- Service ID:
- Service Name:
- Service Provider:
- PCR PID:

- PMT PID:
- Video PID:
- MP2 PID:
- AC3 PID:
- DRA PID:

VBI

- CC:
- CC Even Field:
- CC Odd Field:
- TT:

- Even Field Line:
- Odd Field Line:
- TT PID: