EMR3.0 Management

- Config
- Monitor

Video Encode

- Encode:
- Brightness:
- Contrast:
- Saturation:
- Hue:
- Bitrate(bps):
- Selection:
- Output Resolution:
- Profile:
- Level:
- Aspect Ratio:

- GOP Structure:
- GOP Size:
- IDR Frequency(GOPs):
- Entropy Coding:
- OP Video Loss:
- Test Pattern:

Audio Encode

- Status:
- Encoding Type:
- L R Channel:
- Bitrate:

- Volume:
- Mode:
- Delay(ms):

TS

- Service ID:
- Service Name:
- Service Provider:
- PMT PID:

- PCR PID:
- Video PID:
- Audio PID:

TXT

- Start PosX:

- Start PosY:

- Text Content: