  AppVersion = 42000
[GENERAL]
  ConnectMode = 0
  CurrentFile = "E:\版本控制\EMR3.0平台版本\3系列\V3.0.3.0\EMR3.0_媒体综合处理平台_V3.0.3.0版本提交\下发\07_升级文件\bootloader\bootloader4m.bin"
  DataFileSAddr = 0x10000000
  GUIMode = 0
  HostName = ""
  TargetIF = 0
  USBPort = 0
  USBSerialNo = 0x00000000
[JTAG]
  Device0_ID = 0x0792603F
  Device0_IRLen = 0x00000004
  Device0_Name = "ARM926EJ-S Core"
  IRLen = 0
  MultipleTargets = 0
  NumDevices = 1
  Speed0 = 5
  Speed1 = 8000
  TAP_Number = 0
  UseAdaptive0 = 0
  UseAdaptive1 = 0
  UseMaxSpeed0 = 0
  UseMaxSpeed1 = 1
[CPU]
  CheckCoreID = 1
  ChipName = "Analog ADuC7020x62"
  ClockSpeed = 0x00000000
  Core = 0xFFFFFFFF
  CoreID = 0x0792603F
  DeviceFamily = 0x00000000
  EndianMode = 0
  HasInternalFlash = 0
  InitStep0_Action = "Reset"
  InitStep0_Comment = "Reset and halt target"
  InitStep0_Value0 = 0x00000000
  InitStep0_Value1 = 0x00000000
  InitStep10_Action = "Write 32bit"
  InitStep10_Comment = ""
  InitStep10_Value0 = 0xFFFFF804
  InitStep10_Value1 = 0xFFFF0000
  InitStep11_Action = "Write 32bit"
  InitStep11_Comment = ""
  InitStep11_Value0 = 0xFFFFEC00
  InitStep11_Value1 = 0x01010101
  InitStep12_Action = "Write 32bit"
  InitStep12_Comment = ""
  InitStep12_Value0 = 0xFFFFEC04
  InitStep12_Value1 = 0x1F1F1F1F
  InitStep13_Action = "Write 32bit"
  InitStep13_Comment = ""
  InitStep13_Value0 = 0xFFFFEC08
  InitStep13_Value1 = 0x007F007F
  InitStep14_Action = "Write 32bit"
  InitStep14_Comment = ""
  InitStep14_Value0 = 0xFFFFEC0C
  InitStep14_Value1 = 0x001F1003
  InitStep15_Action = "Write 32bit"
  InitStep15_Comment = "csa"
  InitStep15_Value0 = 0xFFFFEF1C
  InitStep15_Value1 = 0x00010102
  InitStep1_Action = "Write 32bit"
  InitStep1_Comment = "enable use reset"
  InitStep1_Value0 = 0xFFFFFD08
  InitStep1_Value1 = 0xA5000501
  InitStep2_Action = "Write 32bit"
  InitStep2_Comment = "disable watchdog"
  InitStep2_Value0 = 0xFFFFFD44
  InitStep2_Value1 = 0x00008000
  InitStep3_Action = "Write 32bit"
  InitStep3_Comment = "ckgr bypass osc, main ena"
  InitStep3_Value0 = 0xFFFFFC20
  InitStep3_Value1 = 0x00004002
  InitStep4_Action = "Delay"
  InitStep4_Comment = ""
  InitStep4_Value0 = 0x00000000
  InitStep4_Value1 = 0x00000001
  InitStep5_Action = "Write 32bit"
  InitStep5_Comment = "plla"
  InitStep5_Value0 = 0xFFFFFC28
  InitStep5_Value1 = 0x202A3F01
  InitStep6_Action = "Delay"
  InitStep6_Comment = ""
  InitStep6_Value0 = 0x00000000
  InitStep6_Value1 = 0x00000001
  InitStep7_Action = "Write 32bit"
  InitStep7_Comment = "mckr"
  InitStep7_Value0 = 0xFFFFFC30
  InitStep7_Value1 = 0x00001302
  InitStep8_Action = "Delay"
  InitStep8_Comment = ""
  InitStep8_Value0 = 0x00000000
  InitStep8_Value1 = 0x00000001
  InitStep9_Action = "Write 32bit"
  InitStep9_Comment = ""
  InitStep9_Value0 = 0xFFFFF870
  InitStep9_Value1 = 0xFFFF0000
  NumInitSteps = 16
  RAMAddr = 0x00200000
  RAMSize = 0x00004000
  UseAutoSpeed = 0x00000001
  UseRAM = 1
[FLASH]
  aSectorSel[0] = 
  AutoDetect = 1
  BankName = ""
  BankSelMode = 1
  BaseAddr = 0x10000000
  CheckId = 0
  CustomRAMCode = "G:\boot_loader_new\boot_loader_new_Data\Debug\rom.bin"
  DeviceName = "Auto detected flash memory"
  EndBank = 511
  NumBanks = 1
  OrgNumBits = 16
  OrgNumChips = 1
  StartBank = 0
  UseCustomRAMCode = 0
[PRODUCTION]
  AutoPerformsErase = 1
  AutoPerformsHardLock = 0
  AutoPerformsHardUnlock = 0
  AutoPerformsProgram = 1
  AutoPerformsSecure = 0
  AutoPerformsSoftLock = 0
  AutoPerformsSoftUnlock = 1
  AutoPerformsStartApp = 0
  AutoPerformsUnsecure = 0
  AutoPerformsVerify = 1
  Delay = 0x000001F4
  EraseType = 2
  ProgramSN = 0
  SNAddr = 0x00000000
  SNInc = 0x00000001
  Threshold = 0x00000BB8
  VerifyType = 1
