//history:
//V1.0.9:2019/01/15
    a¡¢update ver
//V1.0.8:2016/08/10
    a¡¢add Si2183_drv.out £¬MN88436_drv_V%.out(for C562)
//V1.0.7:2016/01/13
//  a.add todRecv_V%.out
//V1.0.6:2016/01/10
//  a.add M88DS3103_drv_V%.out,C52xCI_V%.out
//V1.0.5:2015/08/27
//  a.add fpgaiic_V%.out,GX1121C_V%.out and Si2168_drv_V%.out
//V1.0.4:2015/07/29
//  a.add serial_V%.out
//V1.0.3:2015/06/29
//  a.add osal.out and .dxt8243_V%.out
//  b.add OS_API_Init(),and dxt8243_info_register()
//V1.0.2:2015/05/21
//  a.delete bb_bkupInit(), which is called automatically from.
//  b.add basicCard, demodCard and some chip module.
//V1.0.1:2014/08/25
//  merge spi and iic into bus lib; add libCommon, psiMudule, ipptbkup and ciLibV2.x.y lib
//V1.0.0: 2014/04/15
//  this file has version from now
ld(0, 0, "/tffs0/lib/osal_V%.out")
ld(0, 0, "/tffs0/lib/libCommon_V%.out")
ld(0, 0, "/tffs0/back_board/zlib.out")
ld(0, 0, "/tffs0/back_board/yaffs.out")
ld(0, 0, "/tffs0/back_board/xlog.out")
ld(0, 0, "/tffs0/back_board/xmlParameter.out")
ld(0, 0, "/tffs0/lib/bus_V%.out")
ld(0, 0, "/tffs0/lib/psiModule_V%.out")
ld(0, 0, "/tffs0/back_board/back.out")
ld(0, 0, "/tffs0/back_board/menu.out")
ld(0, 0, "/tffs0/webserver/WebServer.out")
ld(0, 0, "/tffs0/lib/lock_machine_V%.out")
ld(0, 0, "/tffs0/back_board/bb.out")
ld(0, 0, "/tffs0/back_board/fecSel.out")
ld(0, 0, "/tffs0/webserver/mux.out")
ld(0, 0, "/tffs0/back_board/scr.out")
ld(0, 0, "/tffs0/back_board/backup.out")
ld(0, 0, "/tffs0/webserver/appWeb.out")
ld(0, 0, "/tffs0/back_board/lcd_new.out")
ld(0, 0, "/tffs0/lib/inOutCommon_V%.out")
ld(0, 0, "/tffs0/lib/libav_V%.out")
ld(0, 0, "/tffs0/lib/ciLib_V%.out")
ld(0, 0, "/tffs0/lib/DemodModule_V%.out")
ld(0, 0, "/tffs0/DESC_C510CI/c510.out")
ld(0, 0, "/tffs0/lib/Si2183_drv.out")
ld(0, 0, "/tffs0/DVBT2_C544/C544.out")
ld(0, 0, "/tffs0/lib/ipptbkup_V%.out")
ld(0, 0, "/tffs0/lib/basicCard_V%.out")
ld(0, 0, "/tffs0/lib/demodCard_V%.out")
ld(0, 0, "/tffs0/lib/fpgaiic_V%.out")
ld(0, 0, "/tffs0/lib/serial_V%.out")
ld(0, 0, "/tffs0/lib/dxt8243_V%.out")
ld(0, 0, "/tffs0/lib/cxd2838er_drv_V%.out")
ld(0, 0, "/tffs0/lib/MN88436_drv_V%.out")
ld(0, 0, "/tffs0/lib/GX1121C_V%.out")
ld(0, 0, "/tffs0/lib/ATBM888x_drv_V%.out")
ld(0, 0, "/tffs0/lib/Si2168_drv_V%.out")
ld(0, 0, "/tffs0/lib/M88DS3103_drv_V%.out")
ld(0, 0, "/tffs0/lib/C52xCI_V%.out")
ld(0, 0, "/tffs0/lib/todRecv_V%.out")
ld(0, 0, "/tffs0/lib/mxl542_drv_V%.out")
ld(0, 0, "/tffs0/lib/si2166_drv_V%.out")

osal_info_register()
OS_API_Init()
libcommon_info_register()
bus_info_register()
in_out_common_info_register()
serial_fpga_info_register()
dxt8243_info_register()
libav_info_register()
ciLib_info_register()
ciLibPro_info_register()
ciIf_info_register()
demod_info_register()
ipPtBk_info_register()
psi_info_register()
basic_card_info_register()
demod_card_info_register()
cxd2838erDrv_info_register()
tod_recv_task_init()
C52xCI_info_register()
bb_Init(0)
bb_scrInit(0)//little emr need delete hare
