Input Config

10GbE Input Configuration

Port Configuration | Port 1 | Port 2
--- | --- | ---
IP Address |  |
Subnet Mask |  |
Gateway |  |
MAC Address |  |
Input Switch |  |
Speed Select |  |
Speed State |  |
GbE Input Name |  |
Port Pair Configuration |
Primary Port |
Current Active Port |
Packet Format | 188
Redundancy Configuration |
Backup method |
Detention Mode of 1+1 |
Backup Enabled |
Check Time (100ms) |
Revert To Primary |
Revert Check Time (100ms) |
Backup Mode |
Gratuitous ARP |
Send Enabled |
Send Interval (s) |
IGMP Setting |
Send IGMP Version |