Input Config

GbE Input Configuration

Port Configuration | Port 1 | Port 2 | Port 3 | Port 4
--- | --- | --- | --- | ---
IP Address |  |  |  |
Subnet Mask |  |  |  |
Gateway |  |  |  |
MAC Address |  |  |  |
Input Switch |  |  |  |
Speed Select |  |  |  |
Speed State |  |  |  |
GbE Input Name |  |  |  |
Port Pair Configuration | Port Pair 1 | Port Pair 2
Primary Port |  |
Current Active Port |  |
GbE Loop Out Cofiguration |
Loop Out Switch |  |
IP Address |  |
MAC Address |  |
Redundancy Configuration |
Backup method |
Detention Mode of 1+1 |
Backup Enabled |
Check Time (100ms) |
Revert To Primary |
Revert Check Time (100ms) |
Backup Mode |
Gratuitous ARP |
Send Enabled |
Send Interval (s) |
IGMP Setting |
Send IGMP Version |