PBI-DXP3800MF-TRAP-V2-MIB DEFINITIONS ::= BEGIN 

IMPORTS         
    NOTIFICATION-TYPE																				FROM SNMPv2-SMI
    pbiTrapModule, pbiTrapEventAgentName, pbiTrapEventAgentIpAddress, pbiTrapEventAgentMac,pbiTrapEventCode, 
    pbiTrapEventSpecificProblem, pbiTrapEventSeverity, pbiTrapEventGeneratedTime				FROM PBI-TRAP-MAIN-MIB;

pbiTrapModuleDxp3800mf	OBJECT IDENTIFIER	::= { pbiTrapModule 38 }

pbiNotificationDxp3800mfPrefix	MODULE-IDENTITY
        LAST-UPDATED "201410310600Z"
        ORGANIZATION "PBI"
        CONTACT-INFO "
        		Lei He
				E-mail: lhe@pbicn.com"
        DESCRIPTION "
                This file defines the MIB of DXP3800MF-Trap-v2."
        REVISION	"201406180200Z"
        DESCRIPTION "
        		Start to define this MIB file." 
        REVISION	"201406180600Z"
        DESCRIPTION "
        		Finish to define this MIB file, which version is v1.0."				       		
        REVISION	"201410310600Z"
        DESCRIPTION "
        		Optimize the source code,fix code bugs,which version is v1.1."	                		
        REVISION	"201502120600Z"
        DESCRIPTION "
        		Add power event,which version is v1.2."		                		
         		                		
       ::= { pbiTrapModuleDxp3800mf 2 }

pbiNotificationsDxp3800mf	OBJECT IDENTIFIER	::= { pbiNotificationDxp3800mfPrefix 0 }
      		
pbiNotificationsDxp3800mfPowerOn	NOTIFICATION-TYPE
		
		OBJECTS	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity, 
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		STATUS	current

		DESCRIPTION
				"Power On."
		::= {pbiNotificationsDxp3800mf 1}
		
pbiNotificationsDxp3800mfReboot	NOTIFICATION-TYPE

		OBJECTS	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity,
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		STATUS	current 

		DESCRIPTION
				"Reboot."
		::= {pbiNotificationsDxp3800mf 2}
		
pbiNotificationsDxp3800mfASIInUnlock	NOTIFICATION-TYPE

		OBJECTS	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity,
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		STATUS	current 

		DESCRIPTION
				"ASI In Unlock."
		::= {pbiNotificationsDxp3800mf 3}
		
pbiNotificationsDxp3800mfASIInLock	NOTIFICATION-TYPE

		OBJECTS	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity,
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		STATUS	current 

		DESCRIPTION
				"ASI In Lock."
		::= {pbiNotificationsDxp3800mf 4}
		
pbiNotificationsDxp3800mfASI1OutUnlock	NOTIFICATION-TYPE

		OBJECTS	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity,
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		STATUS	current 

		DESCRIPTION
				"ASI1 Out Unlock."
		::= {pbiNotificationsDxp3800mf 5}
		
pbiNotificationsDxp3800mfASI1OutLock	NOTIFICATION-TYPE

		OBJECTS	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity,
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		STATUS	current 

		DESCRIPTION
				"ASI1 Out Lock."
		::= {pbiNotificationsDxp3800mf 6}
		
pbiNotificationsDxp3800mfASI2OutUnlock	NOTIFICATION-TYPE

		OBJECTS	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity,
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		STATUS	current 

		DESCRIPTION
				"ASI2 Out Unlock."
		::= {pbiNotificationsDxp3800mf 7}
		
pbiNotificationsDxp3800mfASI2OutLock	NOTIFICATION-TYPE

		OBJECTS	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity,
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		STATUS	current 

		DESCRIPTION
				"ASI2 Out Lock."
		::= {pbiNotificationsDxp3800mf 8}
				
pbiNotificationsDxp3800mfASI3OutUnlock	NOTIFICATION-TYPE

		OBJECTS	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity,
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		STATUS	current 

		DESCRIPTION
				"ASI3 Out Unlock."
		::= {pbiNotificationsDxp3800mf 9}
		
pbiNotificationsDxp3800mfASI3OutLock	NOTIFICATION-TYPE

		OBJECTS	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity,
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		STATUS	current 

		DESCRIPTION
				"ASI3 Out Lock."
		::= {pbiNotificationsDxp3800mf 10}
				
pbiNotificationsDxp3800mfASI4OutUnlock	NOTIFICATION-TYPE

		OBJECTS	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity,
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		STATUS	current 

		DESCRIPTION
				"ASI4 Out Unlock."
		::= {pbiNotificationsDxp3800mf 11}
		
pbiNotificationsDxp3800mfASI4OutLock	NOTIFICATION-TYPE

		OBJECTS	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity,
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		STATUS	current 

		DESCRIPTION
				"ASI4 Out Lock."
		::= {pbiNotificationsDxp3800mf 12}
    
pbiNotificationsDxp3800mfRemux1OutputBitrateOverflow	NOTIFICATION-TYPE

		OBJECTS	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity,
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		STATUS	current 

		DESCRIPTION
				"Remux1 Output Bitrate Overflow."
		::= {pbiNotificationsDxp3800mf 13}

pbiNotificationsDxp3800mfRemux1OutputBitrateOK	NOTIFICATION-TYPE

		OBJECTS	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity,
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		STATUS	current 

		DESCRIPTION
				"Remux1 Output Bitrate OK."
		::= {pbiNotificationsDxp3800mf 14}

pbiNotificationsDxp3800mfRemux2OutputBitrateOverflow	NOTIFICATION-TYPE

		OBJECTS	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity,
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		STATUS	current 

		DESCRIPTION
				"Remux2 Output Bitrate Overflow."
		::= {pbiNotificationsDxp3800mf 15}

pbiNotificationsDxp3800mfRemux2OutputBitrateOK	NOTIFICATION-TYPE

		OBJECTS	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity,
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		STATUS	current 

		DESCRIPTION
				"Remux2 Output Bitrate OK."
		::= {pbiNotificationsDxp3800mf 16}

pbiNotificationsDxp3800mfRemux3OutputBitrateOverflow	NOTIFICATION-TYPE

		OBJECTS	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity,
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		STATUS	current 

		DESCRIPTION
				"Remux3 Output Bitrate Overflow."
		::= {pbiNotificationsDxp3800mf 17}

pbiNotificationsDxp3800mfRemux3OutputBitrateOK	NOTIFICATION-TYPE

		OBJECTS	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity,
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		STATUS	current 

		DESCRIPTION
				"Remux3 Output Bitrate OK."
		::= {pbiNotificationsDxp3800mf 18}

pbiNotificationsDxp3800mfRemux4OutputBitrateOverflow	NOTIFICATION-TYPE

		OBJECTS	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity,
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		STATUS	current 

		DESCRIPTION
				"Remux4 Output Bitrate Overflow."
		::= {pbiNotificationsDxp3800mf 19}

pbiNotificationsDxp3800mfRemux4OutputBitrateOK	NOTIFICATION-TYPE

		OBJECTS	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity,
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		STATUS	current 

		DESCRIPTION
				"Remux4 Output Bitrate OK."
		::= {pbiNotificationsDxp3800mf 20}



		
pbiNotificationsDxp3800mfTSIPPortLinkDown	NOTIFICATION-TYPE

		OBJECTS	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity,
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		STATUS	current 

		DESCRIPTION
				"TS/IP Port Link Down."
		::= {pbiNotificationsDxp3800mf 21}

pbiNotificationsDxp3800mfTSIPPortLinkUp100M 	NOTIFICATION-TYPE

		OBJECTS	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity,
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		STATUS	current 

		DESCRIPTION
				"TS/IP Port Link Up/100M ."
		::= {pbiNotificationsDxp3800mf 22}
		
pbiNotificationsDxp3800mfTSIPPortLinkUp1000MFull 	NOTIFICATION-TYPE

		OBJECTS	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity,
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		STATUS	current 

		DESCRIPTION
				"TS/IP Port Link Up/1000M full."
		::= {pbiNotificationsDxp3800mf 23}
		
pbiNotificationsDxp3800mfGigabitInUnlock	NOTIFICATION-TYPE

		OBJECTS	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity,
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		STATUS	current 

		DESCRIPTION
				"Gigabit In Unlock."
		::= {pbiNotificationsDxp3800mf 24}

pbiNotificationsDxp3800mfGigabitInLock	NOTIFICATION-TYPE

		OBJECTS	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity,
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		STATUS	current 

		DESCRIPTION
				"Gigabit In Lock."
		::= {pbiNotificationsDxp3800mf 25}
		
pbiNotificationsDxp3800mfGigabitOutUnlock	NOTIFICATION-TYPE

		OBJECTS	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity,
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		STATUS	current 

		DESCRIPTION
				"Gigabit Out Unlock."
		::= {pbiNotificationsDxp3800mf 26}
		
pbiNotificationsDxp3800mfGigabitOutLock	NOTIFICATION-TYPE

		OBJECTS	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity,
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		STATUS	current 

		DESCRIPTION
				"Gigabit Out Lock."
		::= {pbiNotificationsDxp3800mf 27}
		
pbiNotificationsDxp3800mfControlLinkDown	NOTIFICATION-TYPE

		OBJECTS	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity,
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		STATUS	current 

		DESCRIPTION
				"Control Link Down."
		::= {pbiNotificationsDxp3800mf 28}
		
pbiNotificationsDxp3800mfControlLinkUp	NOTIFICATION-TYPE

		OBJECTS	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity,
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		STATUS	current 

		DESCRIPTION
				"Control Link Up."
		::= {pbiNotificationsDxp3800mf 29}

pbiNotificationsDxp3800mfAccessFromAnInvalidCommunity	NOTIFICATION-TYPE

		OBJECTS	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity,
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		STATUS	current 

		DESCRIPTION
				"Access from an invalid community."
		::= {pbiNotificationsDxp3800mf 30}

pbiNotificationsDxp3800mfPower1ErrorLog	NOTIFICATION-TYPE
		
		OBJECTS	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity, 
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		STATUS	current

		DESCRIPTION
				"Power1 Error."
		::= {pbiNotificationsDxp3800mf 31}

pbiNotificationsDxp3800mfPower2ErrorLog	NOTIFICATION-TYPE
		
		OBJECTS	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity, 
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		STATUS	current

		DESCRIPTION
				"Power2 Error."
		::= {pbiNotificationsDxp3800mf 32}

pbiNotificationsDxp3800mfPower1OKLog	NOTIFICATION-TYPE
		
		OBJECTS	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity, 
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		STATUS	current

		DESCRIPTION
				"Power1 OK."
		::= {pbiNotificationsDxp3800mf 33}

pbiNotificationsDxp3800mfPower2OKLog	NOTIFICATION-TYPE
		
		OBJECTS	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity, 
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		STATUS	current

		DESCRIPTION
				"Power2 OK."
		::= {pbiNotificationsDxp3800mf 34}


END
