PBI-DXP3800MF-TRAP-V1-MIB DEFINITIONS ::= BEGIN   

IMPORTS
    pbiTrapModule, pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, 
    pbiTrapEventSeverity, pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem				FROM PBI-TRAP-MAIN-MIB;

pbiTrapModuleDxp3800mf	OBJECT IDENTIFIER	::= { pbiTrapModule 38 }

pbiTrapsDxp3800mf	MODULE-IDENTITY
        LAST-UPDATED "201410310600Z"
        ORGANIZATION "PBI"
        CONTACT-INFO "
        		Lei He
				E-mail: lhe@pbicn.com"
        DESCRIPTION "
                This file defines the MIB of DXP3800MF-Trap-v1."
        REVISION	"201406180200Z"
        DESCRIPTION "
        		Start to define this MIB file."  
        REVISION	"201406180600Z"
        DESCRIPTION "
        		Finish to define this MIB file, which version is v1.0." 				   		
        REVISION	"201410310600Z"
        DESCRIPTION "
        		Optimize the source code,fix code bugs,which version is v1.1."	                		
        REVISION	"201502120600Z"
        DESCRIPTION "
        		Add power event,which version is v1.2."	                		
        ::= { pbiTrapModuleDxp3800mf 1 }
           
pbiTrapsDxp3800mfPowerOn	TRAP-TYPE
		ENTERPRISE	pbiTrapsDxp3800mf
		VARIABLES	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity, 
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		DESCRIPTION
				"Power On."
		::= 1    
		
pbiTrapsDxp3800mfReboot	TRAP-TYPE
		ENTERPRISE	pbiTrapsDxp3800mf
		VARIABLES	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity, 
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		DESCRIPTION
				"Reboot."
		::= 2 		
		
pbiTrapsDxp3800mfASIInUnlock	TRAP-TYPE
		ENTERPRISE	pbiTrapsDxp3800mf
		VARIABLES	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity, 
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		DESCRIPTION
				"ASI In Unlock."
		::= 3    
		
pbiTrapsDxp3800mfASIInLock	TRAP-TYPE
		ENTERPRISE	pbiTrapsDxp3800mf
		VARIABLES	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity, 
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		DESCRIPTION
				"ASI In Lock."
		::= 4   
		
pbiTrapsDxp3800mfASI1OutUnlock	TRAP-TYPE
		ENTERPRISE	pbiTrapsDxp3800mf
		VARIABLES	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity, 
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		DESCRIPTION
				"ASI1 Out Unlock."
		::= 5   
		
pbiTrapsDxp3800mfASI1OutLock	TRAP-TYPE
		ENTERPRISE	pbiTrapsDxp3800mf
		VARIABLES	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity, 
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		DESCRIPTION
				"ASI1 Out Lock."
		::= 6   
pbiTrapsDxp3800mfASI2OutUnlock	TRAP-TYPE
		ENTERPRISE	pbiTrapsDxp3800mf
		VARIABLES	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity, 
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		DESCRIPTION
				"ASI2 Out Unlock."
		::= 7   
		
pbiTrapsDxp3800mfASI2OutLock	TRAP-TYPE
		ENTERPRISE	pbiTrapsDxp3800mf
		VARIABLES	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity, 
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		DESCRIPTION
				"ASI2 Out Lock."
		::= 8   
		
pbiTrapsDxp3800mfASI3OutUnlock	TRAP-TYPE
		ENTERPRISE	pbiTrapsDxp3800mf
		VARIABLES	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity, 
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		DESCRIPTION
				"ASI3 Out Unlock."
		::= 9   
		
pbiTrapsDxp3800mfASI3OutLock	TRAP-TYPE
		ENTERPRISE	pbiTrapsDxp3800mf
		VARIABLES	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity, 
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		DESCRIPTION
				"ASI3 Out Lock."
		::= 10   
		
pbiTrapsDxp3800mfASI4OutUnlock	TRAP-TYPE
		ENTERPRISE	pbiTrapsDxp3800mf
		VARIABLES	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity, 
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		DESCRIPTION
				"ASI4 Out Unlock."
		::= 11   
		
pbiTrapsDxp3800mfASI4OutLock	TRAP-TYPE
		ENTERPRISE	pbiTrapsDxp3800mf
		VARIABLES	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity, 
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		DESCRIPTION
				"ASI4 Out Lock."
		::= 12   

pbiTrapsDxp3800mfRemux1OutputBitrateOverflow	TRAP-TYPE
		ENTERPRISE	pbiTrapsDxp3800mf
		VARIABLES	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity, 
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		DESCRIPTION
				"Remux1 Output Bitrate Overflow."
		::= 13

pbiTrapsDxp3800mfRemux1OutputBitrateOK	TRAP-TYPE
		ENTERPRISE	pbiTrapsDxp3800mf
		VARIABLES	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity, 
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		DESCRIPTION
				"Remux1 Output Bitrate OK."
		::= 14

pbiTrapsDxp3800mfRemux2OutputBitrateOverflow	TRAP-TYPE
		ENTERPRISE	pbiTrapsDxp3800mf
		VARIABLES	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity, 
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		DESCRIPTION
				"Remux2 Output Bitrate Overflow."
		::= 15

pbiTrapsDxp3800mfRemux2OutputBitrateOK	TRAP-TYPE
		ENTERPRISE	pbiTrapsDxp3800mf
		VARIABLES	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity, 
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		DESCRIPTION
				"Remux2 Output Bitrate OK."
		::= 16

pbiTrapsDxp3800mfRemux3OutputBitrateOverflow	TRAP-TYPE
		ENTERPRISE	pbiTrapsDxp3800mf
		VARIABLES	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity, 
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		DESCRIPTION
				"Remux1 Output Bitrate Overflow."
		::= 17

pbiTrapsDxp3800mfRemux3OutputBitrateOK	TRAP-TYPE
		ENTERPRISE	pbiTrapsDxp3800mf
		VARIABLES	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity, 
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		DESCRIPTION
				"Remux1 Output Bitrate OK."
		::= 18

pbiTrapsDxp3800mfRemux4OutputBitrateOverflow	TRAP-TYPE
		ENTERPRISE	pbiTrapsDxp3800mf
		VARIABLES	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity, 
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		DESCRIPTION
				"Remux1 Output Bitrate Overflow."
		::= 19

pbiTrapsDxp3800mfRemux4OutputBitrateOK	TRAP-TYPE
		ENTERPRISE	pbiTrapsDxp3800mf
		VARIABLES	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity, 
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		DESCRIPTION
				"Remux1 Output Bitrate OK."
		::= 20
		
pbiTrapsDxp3800mfTSIPPortLinkDown	TRAP-TYPE
		ENTERPRISE	pbiTrapsDxp3800mf
		VARIABLES	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity, 
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		DESCRIPTION
				"TS/IP Port Link Down."
		::= 21		  

pbiTrapsDxp3800mfTSIPPortLinkUp100M 	TRAP-TYPE
		ENTERPRISE	pbiTrapsDxp3800mf
		VARIABLES	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity, 
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		DESCRIPTION
				"TS/IP Port Link Up/100M ."
		::= 22	
		
pbiTrapsDxp3800mfTSIPPortLinkUp1000Mfull 	TRAP-TYPE
		ENTERPRISE	pbiTrapsDxp3800mf
		VARIABLES	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity, 
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		DESCRIPTION
				"TS/IP Port Link Up/1000M full ."
		::= 23
		
pbiTrapsDxp3800mfGigabitInUnlock	TRAP-TYPE
		ENTERPRISE	pbiTrapsDxp3800mf
		VARIABLES	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity, 
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		DESCRIPTION
				"Gigabit In Unlock."
		::= 24
		
pbiTrapsDxp3800mfGigabitInLock	TRAP-TYPE
		ENTERPRISE	pbiTrapsDxp3800mf
		VARIABLES	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity, 
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		DESCRIPTION
				"Gigabit In Lock."
		::= 25
		
pbiTrapsDxp3800mfGigabitOutUnlock	TRAP-TYPE
		ENTERPRISE	pbiTrapsDxp3800mf
		VARIABLES	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity, 
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		DESCRIPTION
				"Gigabit Out Unlock."
		::= 26

pbiTrapsDxp3800mfGigabitOutLock	TRAP-TYPE
		ENTERPRISE	pbiTrapsDxp3800mf
		VARIABLES	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity, 
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		DESCRIPTION
				"Gigabit Out Lock."
		::= 27	
		
pbiTrapsDxp3800mfControlLinkDown	TRAP-TYPE
		ENTERPRISE	pbiTrapsDxp3800mf
		VARIABLES	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity, 
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		DESCRIPTION
				"Control Link Down."
		::= 28
		
pbiTrapsDxp3800mfControlLinkUp	TRAP-TYPE
		ENTERPRISE	pbiTrapsDxp3800mf
		VARIABLES	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity, 
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		DESCRIPTION
				"Control Link Up."
		::= 29
		
pbiTrapsDxp3800mfAccessFromAnInvalidCommunity	TRAP-TYPE
		ENTERPRISE	pbiTrapsDxp3800mf
		VARIABLES	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity, 
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		DESCRIPTION
				"Access from an invalid community."
		::= 30

pbiTrapsDxp3800mfPower1ErrorLog	TRAP-TYPE
		ENTERPRISE	pbiTrapsDxp3800mf
		VARIABLES	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity, 
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		DESCRIPTION
				"Power1 Error."
		::= 31

pbiTrapsDxp3800mfPower2ErrorLog	TRAP-TYPE
		ENTERPRISE	pbiTrapsDxp3800mf
		VARIABLES	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity, 
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		DESCRIPTION
				"Power2 Error."
		::= 32

pbiTrapsDxp3800mfPower1OKLog	TRAP-TYPE
		ENTERPRISE	pbiTrapsDxp3800mf
		VARIABLES	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity, 
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		DESCRIPTION
				"Power1 OK."
		::= 33

pbiTrapsDxp3800mfPower2OKLog	TRAP-TYPE
		ENTERPRISE	pbiTrapsDxp3800mf
		VARIABLES	{ pbiTrapEventAgentName, pbiTrapEventAgentIpAddress,pbiTrapEventAgentMac, pbiTrapEventCode, pbiTrapEventSeverity, 
							pbiTrapEventGeneratedTime, pbiTrapEventSpecificProblem  } 
		DESCRIPTION
				"Power2 OK."
		::= 34


END
