7.0.3.5(R0217.0142)
FIX|MT5123 memory leaking

7.0.3.5(R0217.0140)
FIX|MT5082 memory leaking by walking many SNMP OIDs

7.0.3.5(R0217.0139)
FIX|MT5023 Interface vlan 1 doesn't respond on arp request	

7.0.3.5(R0217.0137)
FIX|MT4990 SNMP set user failed

7.0.3.5(R0217.0134)
FIX|MT4827 Problem with infinite lease time

7.0.3.5(R0217.0132)
FIX|MT4915 lldp packets with more than one management address are discarded

7.0.3.5(R0217.0130)
FIX|MT4883 ip-acl via SNMP
FIX|MT4886 problem with deleting dhcp snooping binding static entry

7.0.3.5(R0217.0128)
FIX|MT4380 dhcp_relay_and _binding

7.0.3.5(R0217.0124)
FIX|MT4778 MAC-IP ACL via SNMP

7.0.3.5(R0217.0119)
FIX|MT4616 tNAC task hangup by dhcpv6 option22 packets

7.0.3.5(R0217.0118)
FIX|MT4589 add default management ip

7.0.3.5(R0217.0115)
FIX|MT4453 Lose load-balance config after reload

7.0.3.5(R0217.0112)
FIX|MT4418 port-security switch freezes

7.0.3.5(R0217.0110)
FIX|MT4399 force speed on combo ports results to inoperability of port

7.0.3.5(R0217.0108)
FIX|MT4295 Problem with multicast if use chain of switches
FIX|MT4218 Incorrect syntax for LldpPortId

7.0.3.5(R0217.0104)
FIX|MT4259 drop IS-IS packet when enable QinQ on other port

7.0.3.5(R0217.0102)
FIX|MT4218 Incorrect syntax for LldpPortId

7.0.3.5(R0217.0101)
FIX|MT4201 high cpu load when using ip dhcp snooping user-control

7.0.3.5(R0217.0099)
FIX|MT4158 IGMP queries are being droped when no proxy enabled
FIX|MT4181 cpu 100% after nearly 18 weeks of working

7.0.3.5(R0217.0097)
FIX|MT4153 port-security issue

7.0.3.5(R0217.0095)
FIX|MT4099 improve Port-security log/trap

7.0.3.5(R0217.0094)
ADD| Auto recovery for port-security violation restrict

7.0.3.5(R0217.0093)
FIX|MT4091 port-security and dhcp snooping blackhole issue

7.0.3.5(R0217.0089)
ADD|MT4042 Log for failed authentification by console and SSH

7.0.3.5(R0217.0086)
FIX|MT3973 walk snmp while upgrading cause upgrade failure 

7.0.3.5(R0217.0085)
FIX|MT3906 Very big CPU usage by IGMP packets

7.0.3.5(R0217.0083)
ADD|MT3922 add ip info in dhcp snooping logs
FIX|MT3932 show tech-support info
FIX|MT3995  Interface vlan does not available

7.0.3.5(R0217.0081)
FIX|MT3927 igmp snooping authentication free-rule doesn't work with igmpv3
7.0.3.5(R0217.0075)
FIX|MT3904 snmpv3 issue

7.0.3.5(R0217.0073)
FIX|MT3895 "/n" in show logging buffer

7.0.3.5(R0217.0069)
ADD|MT3817 lldp management-address tlv

7.0.3.5(R0217.0067)
FIX|MT3810 CLI freezes and ICMP losses

7.0.3.5(R0217.0066)
FIX|MT3810 ungrade failure when configuration with vlan 1-4094

7.0.3.5(R0217.0065)
FIX|MT3669 Doesn't answer by telnet

7.0.3.5(R0217.0060)_nos
FIX| MT3717 IGMP-A00B 

7.0.3.5(R0217.0052)_nos
FIX| BF70199 switch console access without password by ctrl+D

7.0.3.5(R0217.0041)
--------------------------------------------------------------
[69756] dhcp option 38 is not inserted to all dhcp Solicication packets

7.0.3.5(R0217.0020)
[68698]DSCP/COS non-trust port
[69159]DHCP snooping drops packets with option 80
[69430]IGMP join packets come back from port which send out

7.0.3.1(B0125.0002)
[68730] savi block DHCPv6 packets

7.0.3.5(B0207.0001)
[68816] ifAdminStatus OID ifOperStatus can not sparate
[68786] It is impossible to remove trunk vlan from Port-Channel

7.0.3.1(B0082.0002)
[65486] igmp snooping source and snooping can do together by mib
