V705R002C012B017
FIX|CRM20250205027615 issue with incorrect output of SNMP Object dot1qFdbDynamicCount (OID: 1.3.6.1.2.1.17.7.1.2.1.1.2) at the first request
FIX|CRM20250214027809 issue with tIPTimer task freezing in some cases

V705R002C012B016
FIX|CRM20250122027471 switch not add option 82 to unicast DHCP packets while using DHCP relay
FIX|CRM20241206026090 add command 'erps node-id priority mode (standard | private)' for changing behavior ERPS NR messages according to G.8032/Y.1344 standard

V705R002C012B015
FIX|CRM20250207027659 after enabling port-security sticky on port word 'sticky' disappears when enabling STP

V705R002C012B014
FIX|CRM20250113027186 change values of SNMP object radiusAutServerHostAccessMode (OID 1.3.6.1.4.1.40418.7.100.10.5.5.1.6), new values: Access-mode MAB - 3, Access-mode IGMP - 4

V705R002C012B013
FIX|CRM20250114027210 issue with vlan-isolation and igmp-packets 
FIX|CRM20250113027195 rebooted by watchdog with error in task tIgmpsnoopingv3 in some cases

V705R002C012B009
FIX|CRM20241210026225 issue with SNMPv3 and msgAuthoritativeEngineBoots do not increase after reboot

V705R002C012B008
ADD|CRM20241216026417 add features for mac-address flapping prevention function
FIX|CRM20241216026388 add deleting of DACL from port after break of client authentication

V705R002C012
ADD|recommended FW

V705R002C011B052
FIX|CRM20241126025791 incorrect storm-control settings via SNMP when ports are in LAG

V705R002C011B050
FIX|CRM20241202025955 issue with adding port to LAG when port-security is enabled on other ports
ADD|CRM20240919023804 add SNMP trap branch .1.3.6.1.4.1.40418.7.101.133 for monitoring VSF stack state

V705R002C011B046
ADD|CRM20240125018545 add variations of ZTP operation with DHCP option 125

V705R002C011B044
FIX|CRM20241030024874 delete captive-portal from running-config

V705R002C011B041
ADD|CRM20240910023617 add command 'logging event link-status include speed-duplex' to check speed and duplex in logs when port goes in UP state

V705R002C011B040
FIX|CRM20241018024543 issue with memory leaking in process tSnmpd
ADD|CRM20241029024860 add prompt before changing VSF/Stand-alone mode

V705R002C011B037
ADD|CRM20240611021374 add SNMP OID for NTP configuration

V705R002C011B034
FIX|CRM20240830023358 break down of L3-network after VSF split
FIX|CRM20240807022867 fail to access WEB-interface via domain name in some cases
FIX|CRM20240918023762 issue with configuring ACL via SNMP

V705R002C011B032
FIX|CRM20240704021997 switch uses incorrect IP-address of TFTP-server during the auto-provisioning in some cases
FIX|CRM20240830023348 issue with removing SVI which configured at 'no passive-interface vlan X'

V705R002C011B030
ADD|CRM20240918023764 add support for OIDs tree fdbMacInfo (.1.3.6.1.4.1.40418.7.100.40)
ADD|CRM20240911023619 add posibility to get information about memory via SNMP in bytes

V705R002C011B029
ADD|CRM20240712022209 MAC-address flapping prevention functionality
ADD|CRM20240730022665 full support for wildcard masks
ADD|CRM20240711022177 add ability to discard both untagged frames on trunk/hybrid port and tagged frames where VLAN tag = PVID (command 'switchport trunk|hybrid native-vlan not-forward')
FIX|CRM20240910023593 issue with forming arguments in TACACS+ packet

V705R002C011B025
ADD|CRM20240117018395 add password encryption for archive command at running config

V705R002C011B023
FIX|CRM20240722022455 issue with logging while ERPS changeover
FIX|CRM20240801022744 issue with traffic flood with using Port-channel in some cases

V705R002C011B019
FIX|CRM20240816023043 issue with DHCP snooping and unicast DHCP packet in some cases
FIX|CRM20240820023125 corrected the standard format of syslog messages

V705R002C011B017
ADD|CRM20240506020438 add ability to change syslog message format
ADD|CRM20240515020729 add command 'clear arp-cache static [vlanid <VID>]' to clear static ARP-records
ADD|CRM20240506020439 add RADIUS attribute Framed-IP-address for dot1x and MAB authenticated users using the DHCP Snooping binding table
FIX|CRM20240715022268 change RADIUS service-type attribute in default

V705R002C011B016
FIX|CRM20240408019880 add ability configure different RADIUS-server for MAB and 802.1x authentication
ADD|CRM20240611021373 add command 'mac-authentication-bypass user-ip-from dhcpsnooping enable' to output IP-addresses of clients authenticated via MAB
ADD|CRM20240531021127 add command 'dot1x user-ip-from dhcpsnooping enable' to output IP-addresses of clients authenticated via dot1x

V705R002C011B013
FIX|CRM20240704021993 add opportunity to check advertised/received routes via BGP at VRF

V705R002C011B012
FIX|CRM20240710022146 issue with DHCP packets are transmitted between isolated ports

V705R002C011B009
ADD|CRM20240515020732 change name of button for port configuration on WEB-interface

V705R002C011B007
ADD|CRM20240618021559 add command 'show switch default info'

V705R002C011B005
ADD|CRM20240130018638 add AES algo encryption for user passwords, NTP, SNMP keys at running-config
ADD|CRM20240620021650 add ability to assign MGMT-interface to any VRF

V705R002C011B004
ADD|CRM20240409019902 add IP SLA (NQA) function

V705R002C011B001
ADD|CRM20240520020835 added the ability to use special characters in local user passwords

V705R002C011
ADD|add new stable FW version
FIX|CRM20240520020833 corrected erratas in some commands at CLI

V705R002C010B025
FIX|CRM20240607021322 issue with configuration 'ip default-gateway'

V705R002C010B024
FIX|CRM20240606021291 switch returned DDM value via SNMP only from the first unit at VSF stack
FIX|CRM20240613021427 issue with packet statistics length (1024~1518) on SFP ports

V705R002C010B023
FIX|CRM20240524020952 fix wrong ID of IGMP Snooping authentication NAS-Port

V705R002C010B021
FIX|CRM20240417020096 issue with export info-center config by convert VSF mode

V705R002C010B019
ADD|CRM20240125018537 add config backup to a remote server during the execution of the 'write' command

V705R002C010B013
FIX|CRM20240422020180 add passwords encryption to the command 'show aaa config'
FIX|CRM20240422020181 fix problem with unencrypted keys for some protocols in running-config

V705R002C010B009
ADD|CRM20240425020291 change value of TX signal to -40 dBm when there is no output signal
ADD|CRM20240424020254 add restarting of VSF members via the WEB-interface
FIX|CRM20240429020370 issue with ping and SSH-connection by domain name
ADD|CRM20240427020325 issue with showing IPv6 routes in the WEB-interface

V705R002C010B008
FIX|CRM20240410019943 issue with showing Lease time in output of DHCP Snooping table

V705R002C010B007
ADD|CRM20240222018894 add command 'show archive config differences ...' to compare configuration files

V705R002C010B006
FIX|CRM20240305019144 issue with task zOSPF in some cases

V705R002C010B003
FIX|CRM20240408019881 issue with rebooting switch with error in task tLldp 

V705R002C010B002
ADD|CRM20240329019693 add command 'passive-interface default' for OSPF

V705R002C010B001
FIX|CRM20240329019686 issue with incorrect processing of NFS-packets
FIX|CRM20240410019929 issue with incorrect names of button in WEB-Interface
ADD|CRM20240117018399 add ability to assign same IPv6 link-local address to different interfaces

V705R002C010
ADD|recommended FW

V705R002C009B015
FIX|CRM20240328019672 using the OSPF authentication area method if OSPF authentication on the port is not configured

V705R002C009B013
FIX|CRM20240228019013 add OID 1.0.8802.1.1.2.1.1.7.1 to enable LLDP Management-address TLV on ports
FIX|CRM20240129018590 issue with HTTP authorization when HTTPS is enabled
ADD|CRM20240109018204 change value of RX signal to -40 dBm when there is no signal
FIX|CRM20240228019018 issue with incorrect MAC-addresses in outputting of ARP debug in some cases

V705R002C009B011
FIX|CRM20240223018920 issue with outputting gateway ARP by SNMP in some cases

V705R002C009B010
FIX|CRM20240228019025 WEB-interface doesn't work via VRF

V705R002C009B008
FIX|CRM20240313019314 wrong description of some commands at "copy" mechanism
FIX|CRM20240219018830 fixed various errors at SNMP LLDP 

V705R002C009B007
FIX|CRM20240207018765 fixed high CPU utilization on the last recommended FW (V705R002C009)

V705R002C009B004
ADD|CRM20240125018544 add new PWR/DIAG LED state
FIX|CRM20240229019047 high delay while pinging switch
FIX|CRM20240207018757 switch returns DDM value via SNMP from another port in some cases
FIX|CRM20240220018862 issue with IGMP report messages while using command to replace MAC

V705R002C009B003
ADD|CRM20231128017278 add command to disable logs of user log-in on switch

V705R002C009B001
FIX|CRM20240111018259 issue with configuring rate-violation and LBD at the same time
FIX|CRM20240117018392 issue with incorrect output of SNMP OID (dot1dStpDesignatedRoot) in some cases

V705R002C009
ADD|recommended FW
FIX|CRM20240117018394 port link not up in low-temperature environment

V705R002C008
ADD|recommended FW

V705R002C007B003
FIX|CRM20240117018394 high temperature readings via SNMP if the temperature is below 0

V705R002C007B002
FIX|CRM20240111018253 issue with incorrect output at the WEB-Interface in some cases

V705R002C007B001
FIX|CRM20240109018213 issue with the operation of the ACL, which restricts using TCP-connection flags
FIX|CRM20240109018213 issue with link on ports at low temperatures in some cases

V705R002C007
FIX|CRM20231023016526 issue with lack of some options for config HTTPS secure-ciphersuite at the WEB-Interface
ADD|new WEB design

V705R002C006B010
ADD|CRM20230919016056 add logging to the function "rate-violation" without configured any violation control method

V705R002C006
ADD|ADD new stable FW version

V705R002C005B016
FIX|CRM20231201017319 issue with service password-encryption
FIX|CRM20231122017172 issue with unicast ARP gets into other VLAN in some cases

V705R002C005B015
ADD|CRM20231116017031 add ability to disable CLI prompt

V705R002C005B013
FIX|CRM20231023016524 stop forwarding packets via Port-channel on ERPS-ring in some cases
FIX|CRM20231024016544 correct spanning-tree BPDU counters

V705R002C005B012
FIX|CRM20231102016729 issue with VTY auth through RADIUS in stack

V705R002C005B011
FIX|CRM20231009016276 issue with shortcut keys in some cases

V705R002C005B010
FIX|CRM20231010016310 issue with info-center and watchdog task: zIMI
ADD|CRM20230922016119 add route-map features
ADD|CRM20230919016057 self-defined subscriber-id for specific interface

V705R002C005B008
FIX|CRM20230919016052 switch flooding incorrect messages about PoE at logs
FIX|CRM20231009016290 rebooted by watchdog with error in task tSnmpd in some cases

V705R002C005B006
FIX|CRM20230926016159 fail to save the current config to startup config via WEB in some cases

V705R002C005B005
FIX|CRM20231009016275 issue when MAC-addresses are not studied in some cases

V705R002C005B004
ADD|CRM20230922016118 realize descriptions for L3-interfaces

V705R002C005B003
FIX|CRM20230831015748 issue with packets transit via VSF in some cases

V705R002C005B002
FIX|CRM20230829015717 issue with drop packets in queues in some cases

V705R002C005
ADD|ADD new stable FW version

V705R002C004B020
FIX|CRM20230823015641 issue with getting IP default gateway from ARP table via SNMP request

V705R002C004B016
ADD|CRM20230615014721 add rule-id to ACL 

V705R002C004B014
ADD|CRM20230601014581 add information about Port-Channel interfaces via command "show interface status"

V705R002C004B011
ADD|CRM20230727015308 add output for stack when switch boot

V705R002C004B010
FIX|CRM20230810015517 incorrect work of the switch with the configured dhcp-client

V705R002C004B008
ADD|CRM20230518014385 decrease number of mac-notification messages 

V705R002C004B007
FIX|CRM20230727015310 switch stuck and reboot with Watchdog task tMSTP in some cases

V705R002C004B005
FIX|CRM20230704014986 switch reboot if description contain '%'

V705R002C004B004
FIX|CRM20230731015362 issue with creating user via SNMP in some cases

V705R002C004B002
FIX|CRM20230726015292 doesn't transmit Radius Accept-Request encapsulating Nak-Message

V705R002C003B006
FIX|CRM20230714015139 command 'show clock' doesn’t show seconds

V705R002C003B001
FIX|CRM20230620014804 issue with 'ip tftp-client source'
FIX|CRM20230425014114 issue with low speed in some cases

V705R002C002B038
ADD|CRM20235118013535 snmp-view requirements

V705R002C002B029
FIX|CRM20230602014592 constant high CPU utilization and reboot by Watchdog in some cases

V705R002C002B025
FIX|CRM20230602014593 issue with BPDU-tunnel and QinQ
FIX|CRM20230116013013 changing SSH key

V705R002C002B022
ADD|CRM20220722011334 add an opportunity to configure IP source address for TFTP usage
ADD|CRM20230404013852 add arbitrary UDP-port for syslog

V705R002C002B021
FIX|CRM20230517014367 failed to read switch power information through SNMP

V705R002C002B020
FIX|CRM20230602014591 BFD static route doesn't disappear from routing table

V705R002C002B019
FIX|CRM20230530014543 doesn't appear link on SFP ports in some cases

V705R002C002B018 
ADD|CRM20230330013809 add an ability to configure source-ip address at info-center

V705R002C002B016
ADD|CRM20230508014213 turn off/on PoE for VCT automatically
FIX|CRM20230511014277 tSshdSessionTask0 task hang

V705R002C002B015
FIX|CRM20230504014165 switch becomes unavailable after copy-paste configuration

V705R002C002B013
FIX|CRM20230329013787 fixed opportunity to enable Port-group with storm-control in some cases

V705R002C002B012
FIX|CRM20230419014030 issue with SNMP OID for ifLastChange

V705R002C002B010
FIX|CRM20230420014046 issue with ports in stack after adding VLAN in supervlan

V705R002C002B008
FIX|CRM20230331013814 sometimes switch drop IGMP-reports

V705R002C002B007
FIX|CRM20230210013220 stack reboot after adding VLAN in supervlan

V705R002C002B003
ADD|CRM20220816011607 requirements for dot1x&MAB
FIX|CRM20230310013530 issue with QinQ and BPDU-tunnel user-defined-protocol

V705R002C002B002
ADD|CRM20221220012798 add command to show MD5SUM 
FIX|CRM20230403013841 switch becomes unavailable after "show anti-arpscan"

V705R002C002B001
ADD|CRM20230222013359 support command "show vsf config detail"

7.5.3.6(R0004.0521)
ADD|CRM20230216013283 Port Isolation SNMP MIB Requirements

7.5.3.6(R0004.0519)
ADD|CRM20221216012772 Validity Management of Switch Passwords

7.5.3.6(R0004.0518)
ADD|CRM20221124012599 Ability to turn off/on PoE for VCT automatically

﻿7.5.3.6(R0004.0517)
FIX|CRM20230209013218 issue with OSPF NSSA and AF changing
FIX|CRM20230131013082 issues with port-group + loopback-detection

7.5.3.6(R0004.0511)
ADD|CRM20230118013034 add ability to change mac-address format for RADIUS

﻿7.5.3.6(R0004.0509)
FIX|CRM20230118013031 can't delete file from flash
FIX|CRM20230201013091 device in voice-vlan can't get ip address

7.5.3.6(R0004.0508)
FIX|CRM20230202013120 issue with lldp while using Q-in-Q

﻿7.5.3.6(R0004.0505)
FIX|CRM20220310009555 issue with plain text password for SNMPv3 user

﻿7.5.3.6(R0004.0504)
ADD|CRM20221213012755 add ethernet-oam session state log

7.5.3.6(R0004.0503)
FIX|CRM20230112012992 An error is reported after the IMG upgrade is not recognized during startup

7.5.3.6(R0004.0500)
FIX|CRM20221130012655 issue with load running-config from command
ADD|CRM20221130012658 add tcnguard/tc-guard on switch

7.5.3.6(R0004.0498)
ADD|CRM20221130012655 add SNMP-FRAMEWORK-MIB:snmpEngineID.0

7.5.3.6(R0004.0496)
FIX|CRM20221213012753 issue with some LLDP MED tlv

﻿7.5.3.6(R0004.0495)
FIX|CRM20221202012668 LACP states down without "anti-arpscan trust supertrust-port" on Port-Channel
ADD|CRM20221130012652 add "Lease time" field at "ip DHCP snooping binding" table

7.5.3.6(R0004.0493)
FIX|CRM20221130012654 lose dchp default-gateway after link flap

7.5.3.6(R0004.0490)
ADD|CRM20220816011607 requirements for dot1x&mab

7.5.3.6(R0004.0489)
FIX|CRM20221013012155 issue with BFD on loopback ports

7.5.3.6(R0004.0485)
FIX|CRM20221116012494 error prompt when configuring ip address on tunnel interface

﻿﻿7.5.3.6(R0004.0484)
FIX|CRM20221025012289 issue with ethernet-oam

7.5.3.6(R0004.0482)
ADD|CRM20220816011599 add erps unprotected-instance

7.5.3.6(R0004.0481)
FIX|CRM20220929012074 issue with erps 

7.5.3.6(R0004.0480)
ADD|CRM20220909011853 add command "show erps instance" to display the protected vlan information

7.5.3.6(R0004.0476)
FIX|CRM20220826011711 issue with SFP+ modules 

﻿7.5.3.6(R0004.0472)
FIX|CRM20220830011748 tSnmpd task memory leak

7.5.3.6(R0004.0471)
ADD|CRM20220816011606 Add VRRP plaintext authentication

﻿7.5.3.6(R0004.0470)
FIX|CRM20220829011725 switch reboot in shell

7.5.3.6(R0004.0469)
FIX|CRM20220829011724 issue with erps+mac-move on port-channel interfaces

﻿7.5.3.6(R0004.0468)
FIX|CRM20220823011673 issue with erps mac-flap
ADD|CRM20220606010739 issue with multicast traffic on BLK port in RSTP

7.5.3.6(R0004.0467)
FIX|CRM20220725011358 The encryption algorithm sha256 is enabled and login cannot be enabled

7.5.3.6(R0004.0465)
FIX|CRM20220714011237 issue with 'dot1x re-authentication'

7.5.3.6(R0004.0463)
FIX|CRM20220721011331 Poe affects VCT detection

7.5.3.6(R0004.0461)
ADD|CRM20220720011308 add ability to view vlans in instance by snmp while spanning tree is not enable

7.5.3.6(R0004.0460)
FIX|CRM20220718011279 Cfm function mepid cannot be configured

7.5.3.6(R0004.0459)
FIX|CRM20220719011301 issue with ifLastChange OID

7.5.3.6(R0004.0458)
FIX|CRM20220623010964 issue with option 82 toward cisco server 
ADD|CRM20220704011110 add oid for getting Vlan MAC

7.5.3.6(R0004.0456)
FIX|CRM20220606010741 issue with switch stuck and reboot by watchdog “tCpuRxLimitNotify”

7.5.3.6(R0004.0455)
FIX|CRM20220616010867 issue with spanning-tree output

﻿﻿﻿﻿7.5.3.6(R0004.0453)
FIX|CRM20220606010740 memory leak in stack on AM

7.5.3.6(R0004.0452)
FIX|CRM20220518010465 issue with stack fall apart

7.5.3.6(R0004.0449)
ADD|CRM20220520010515 add oid for getting mac addresses on port

7.5.3.6(R0004.0448)
ADD|CRM20220516010453 add bfd echo

7.5.3.6(R0004.0447)
ADD|CRM20220330009789 add LACP dynamic aggregation port status change log

7.5.3.6(R0004.0445)
FIX|CRM20220426010163 issue with 'show erps ring' output
FIX|CRM20220419009986 issue with RIP authentication
ADD|CRM20220505010281 add port-led shutoff

7.5.3.2(R0004.0444)
FIX|CRM20220420010015 Unable to upgrade using http
FIX|CRM20220422010053 IPv6 BGP update source uses interface loopback1,BGP neighbors cannot be established

7.5.3.2(R0004.0443)
FIX|CRM20220420009998 issue with dhcp pool in vrf

7.5.3.2(R0004.0442)
ADD|CRM20220407009877 managment vrf features

7.5.3.2(R0004.0441)
FIX|CRM20220411009906 issue with automatic restart

7.5.3.2(R0004.0440)
ADD|CRM20220321009686 add loopback swapmac function of port

7.5.3.2(R0004.0439)
ADD|CRM20220407009877 managment vrf features

7.5.3.2(R0004.0437)
FIX|CRM20220406009856 issue with high latency

7.5.3.2(R0004.0435)
FIX|CRM20220402009818 issue with bgp ipv6 default route announce

7.5.3.2(R0004.0434)
FIX|CRM20220310009556 issue with high latency 

7.5.3.2(R0004.0433)
FIX|CRM20220317009645 wrong time in sh users while using ssh keys 

7.5.3.2(R0004.0432)
ADD|CRM20220307009522 support 64 secondary IP address 

7.5.3.2(R0004.0431)
ADD|CRM20220303009471 port loopback swapmac

7.5.3.2(R0004.0427)
FIX|CRM20220223009354 DHCP option82 subscriber-id format vs-cisco
FIX|CRM20220225009366 issue with https 2022-3-10

7.5.3.2(R0004.0426)
FIX|CRM20220223009351 add 'configure terminal' alias

7.5.3.2(R0004.0424)
FIX|CRM20220225009371 issue with ospf point-to-multipoint

7.5.3.2(R0004.0423)
ADD|CRM20220223009349 syslog support udp port

7.5.3.2(R0004.0422)
ADD|CRM20220207009147 increase quantity sub vlans per supervlan
ADD|CRM20220207009149 displaying interface configuration in port-channel

7.5.3.2(R0004.0421)
ADD|CRM20220218009280 issue with isolate and ip arp inspection

7.5.3.2(R0004.0420)
ADD|CRM20220208009159 issue with admin-scope ranges RFC5059 / S5750Ev2

7.5.3.2(R0004.0419)
ADD|CRM20220207009144 issue with POE command

7.5.3.2(R0004.0418)
ADD|CRM20211116008144 add DHCP server for VRF

7.5.3.2(R0004.0417)
ADD|CRM20211028007860 add info-center possibility for VRF

7.5.3.2(R0004.0416)
ADD|CRM20211112008080 issue with 'sh port-group'

7.5.3.2(R0004.0414)
FIX|CRM20211210008564 issue with 'switchport port-security violation recovery'

7.5.3.2(R0004.0410)
FIX|CRM20211222008721 issue with isolate and ip arp inspection 

7.5.3.2(R0004.0408)
FIX|CRM20211214008603 add show command to see dhcp snooping autosave file

7.5.3.2(R0004.0404)
FIX|CRM20211028007851 'sh tcam usage'in VSF mode

7.5.3.2(R0004.0403)
FIX|CRM20210914007249 dhcp snooping user-bind autosave timer

7.5.3.2(R0004.0402)
FIX|CRM20211118008178 static arp is not take effect

7.5.3.2(R0004.0401)
FIX|CRM20211014007633 change 'sh log' output

7.5.3.2(R0004.0400)
ADD|CRM20211028007858 issue with 'ip pim rp-candidate' when multiple multicast networks

7.5.3.2(R0004.0399)
FIX|CRM20211126008321 issue with BFD MAD
FIX|CRM20211028007865 issue with 'authentication ip access-class'

7.5.3.2(R0004.0397)
FIX|CRM20211123008230 VSF SNMP OIDS

7.5.3.2(R0004.0394)
FIX|CRM20211014007633 change 'sh log' output

7.5.3.2(R0004.0389)
FIX|CRM20211009007549 issue with bpdu-tunnel-protocol-stp

7.5.3.2(R0004.0388)
FIX|CRM20211009007552 issue with '::ffff: deny by security IPv6 or ACL:FAULT'

7.5.3.2(R0004.0387)
FIX|CRM20210929007501 issue with OSPF

7.5.3.2(R0004.0385)
FIX|CRM20210916007279 issue with SNMP unavailability

7.5.3.2(R0004.0384)
FIX|CRM20210916007271 issue with SNTP

7.5.3.2(R0004.0383)
FIX|CRM20210915007258 issue with capture via VTY 

7.5.3.2(R0004.0382)
FIX|CRM20210625006214 Flow Control issue

7.5.3.2(R0004.0381)
FIX|CRM20210914007238 issue with ip dhcp snooping binding

7.5.3.2(R0004.0380)
FIX|CRM20210909007168 issue with cross-stack LAG to MLAG Extreme

7.5.3.2(R0004.0377)
FIX|CRM20210830007011 issue with ip dhcp snooping binding

7.5.3.2(R0004.0372)
FIX|CRM20210826006961 issue with http load cfg by eth0
FIX|CRM20210826006964 issue with VSF stack and MAB

7.5.3.2(R0004.0370)
FIX|CRM20210825006944 RSTP rapid recovery of connectivity

7.5.3.2(R0004.0369)
FIX|CRM20210823006934 issue with NTP via multicast/broadcast

7.5.3.2(R0004.0367)
FIX|CRM20210806006773 issue with radius-server access-mode

7.5.3.2(R0004.0364)
FIX|CRM20210802006742 issue with dot1qVlanStaticUntaggedPorts

7.5.3.2(R0004.0361)
FIX|CRM20210723006653 issue with port-group message

7.5.3.2(R0004.0360)
FIX|CRM20210721006637 issue with cpu-protect

7.5.3.2(R0004.0358)
FIX|CRM20210623006185 vrf features
FIX|CRM20210716006602 issue with multicast

7.5.3.2(R0004.0356)
FIX|CRM20210708006484 issue with ‘bpdu-tunnel multi-protocol group’
FIX|CRM20210611006108 LLDP management-address IPv6 and autonegotiation information

7.5.3.2(R0004.0354)
FIX|CRM20210617006129 fan error logs.

7.5.3.2(R0004.0353)
FIX|CRM20210702006371 issue with 1.3.6.1.2.1.31.1.1.1.18 (ifAlias)

7.5.3.2(R0004.0352)
FIX|CRM20210528005955 VRF supports TACACS and SNMP protocols

7.5.3.2(R0004.0350)
FIX|CRM20210517005839 issue with DHCP Relay

7.5.3.2(R0004.0346)
FIX|CRM20210603006013 issue with vlan-flow-statistics via SNMP

7.5.3.2(R0004.0343)
FIX|CRM20210428005616 DHCPv6 Relay Agent Notification for Prefix Delegation

7.5.3.2(R0004.0341)
FIX|CRM20210524005886 Issue with logging actions via web-interface 

7.5.3.2(R0004.0340)
FIX|CRM20210423005531 VSF member console lock 
FIX|CRM20210517005836 issue with LLDP link aggregation status

7.5.3.2(R0004.0338)
FIX|CRM20210511005785 flow control issue 

7.5.3.2(R0004.0336)
FIX|CRM20210326005148 'clear counters','clear counters interface...' SNMP OIDs
FIX|CRM20210324005088 BPDU tunnel user defined protocol, show statistical requirements

7.5.3.2(R0004.0334)
FIX|CRM20210414005400 dhcp-reply broadcasting via dhcp-relay

7.5.3.2(R0004.0332)
FIX|CRM20210407005274 issue with multiple BFD sessions in different router OSPF

7.5.3.2(R0004.0328)
FIX|CRM20210326005146 4600-52x port based protocol VLAN

7.5.3.2(R0004.0325)
FIX|CRM20210309004820 issue with BGP

7.5.3.2(R0004.0323)
FIX|CRM20201119003297 BPDU tunnel user defined protocol requirements

7.5.3.2(R0004.0322)
FIX|CRM20210225004614 -802.1p for IGMP message

7.5.3.2(R0004.0321)
FIX|CRM20210315004917 issue with flood in syslog

7.5.3.2(R0004.0320)
FIX|CRM20210219004231 -EFMOAM must be supported on the physical port even if it is in the LAG

7.5.3.2(R0004.0319)
FIX|CRM20210304004744 double DHCP offer and ack

7.5.3.2(R0004.0318)
FIX|CRM20210302004701 issue with "interface-id"

7.5.3.2(R0004.0317)
FIX|CRM20210302004698 issue with 'debug ip dhcp relay packet'

7.5.3.2(R0004.0316)
FIX|CRM20210208004220 options 37, 38 in the wrong place into DHCPv6-RELAY-FORWARD meassge

7.5.3.2(R0004.0315)
FIX|CRM20210208004219 issue with OID erpsNodeState

7.5.3.2(R0004.0314)
FIX|CRM20210128004145 snmpwalk error

7.5.3.2(R0004.0313)
FIX|CRM20210202004179 issue with service-policy and LACP

7.5.3.2(R0004.0312)
FIX|CRM20210127004140 wrong packet type for op.37 and op.38

7.5.3.2(R0004.0310)
FIX|CRM20210119004006 issue with 'rejected by security IP'

7.5.3.2(R0004.0307)
FIX|CRM20201211003550 -OAM message should include dying gasp info(4600-28X)

7.5.3.2(R0004.0306)
FIX|CRM20201211003550 -OAM message should include dying gasp info(4600-28X)	

7.5.3.2(R0004.0305)
FIX|CRM20201211003560 Autoconfiguration on vlan interface(4600-52X)

7.5.3.2(R0004.0304)
FIX|CRM20201231003797 issue with 'ip dhcp snooping suppress'

7.5.3.2(R0004.0301)
FIX|CRM20201211003558 cpu-rx-limitnotify protocol all enable on（S4600-52x）

7.5.3.2(R0004.0300)
FIX|CRM20200910002346（problem with SP algorithm）
FIX|CRM20201211003558 - cpu-rx-limitnotify protocol all enable(4600-52x)

7.5.3.2(R0004.0299)
FIX|CRM20201118003291 problem with high SFP temperature

7.5.3.2(R0004.0298)
FIX|CRM20201201003411 issue with IP DHCP snooping binding and unicast ack

7.5.3.2(R0004.0296)
ADD|CRM20201126003374 add "show bandwidth control"

7.5.3.2(R0004.0295)
FIX|CRM20201116003256 incorrect description of interface-id option
FIX|CRM20201015002789 MT722 send SNMP trap when switch reloaded
FIX|CRM20201015002790 MT722 Management of local users via SNMP
FIX|CRM20201015002792 MT722 send dying gasp to syslog
FIX|CRM20201015002794 MT722 enable/disable web interface via snmp

7.5.3.2(R0004.0294)
FIX|CRM20201106003163 tL2Input rask hang up 
FIX|CRM20201015002788 MT722 TCN-guard (TCN-Restriction)

7.5.3.2(R0004.0292)
FIX|CRM20201029003027 Web interface POE where Chinese is displayed

7.5.3.2(R0004.0291)
FIX|CRM20201014002746 togrther use with  mab and dhcp snooping issue 

7.5.3.2(R0004.0290)
FIX|CRM20201022002899 loopback port with led issue 

7.5.3.2(R0004.0287)
FIX|CRM20201014002744 wrong format of TACACS+ accounting messages

7.5.3.2(R0004.0286)
FIX|CRM20200910002346 problem with SP algorithm

7.5.3.2(R0004.0285)
FIX|CRM20201009002666 wrong output 'sh fan'
FIX|CRM20200930002629 reboot when autoupgrade

7.5.3.2(R0004.0284)
FIX|CRM20200928002610  issue with 'info-center loghost N prefix off'

7.5.3.2(R0004.0283)
FIX|CRM20200923002547  long ping with snmp monitoring

7.5.3.2(R0004.0281)
FIX|CRM20200906002285  issue with 'snmp-server ddm-mib enable'
FIX|CRM20200910002364  issue with 'info-center loghost N prefix off'

7.5.3.2(R0004.0280)
FIX|CRM20200908002322   capture match issue
FIX|CRM20200908002316   wrong values in sFlow packets

7.5.3.2(R0004.0279)
Critical|CRM20200828002189  tNACTask hang up

7.5.3.2(R0004.0275)
FIX|CRM20200731001769  QinQ + DHCP snooping

7.5.3.2(R0004.0274)
FIX|CRM20200806001835  issu with OSPF
FIX|CRM20200724001663  default nexthop problem in vrf

7.5.3.2(R0004.0272)
FIX|CRM20200716001440  issue with 'copy sftp...' and IPv6 address

7.5.3.2(R0004.0270)
FIX|CRM20200703001277  Radius authentication failed

7.5.3.2(R0004.0266)
FIX|MT20200609000959  QINQ from one to diff vlans
FIX|MT20200610000976  iftype of port-channel issue

7.5.3.2(R0004.0265)
ADD|MT20200527000820   Adding nandflash in 'dir'

7.5.3.2(R0004.0264)
ADD|MT20200601000864  Loopback Detection messages on DCN Switches

7.5.3.2(R0004.0263)
FIX|MT20200520000751  port security via SNMP issue
	
7.5.3.2(R0004.0258)
add|MT10292  issue with upgrading FW via web

7.5.3.2(R0004.0257)
add|MT10113 autoprovision

7.5.3.2(R0004.0256)
critical|20200429000530 task tLOAD hangs up

7.5.3.2(R0004.0253)
FIX|20200421000446 memory leaking issue relate to MT10134

7.5.3.2(R0004.0251)
FIX|MT10284 MGMT-port and NBNS 

7.5.3.2(R0004.0249)
FIX|MT10269 issue set portHybridTaggedAllowedVlanAdd	

7.5.3.2(R0004.0248)
critical|MT10265 task hangs up	
FIX|MTMT10245 hardware limit 1k  

7.5.3.2(R0004.0247)
FIX|MT10228 ip ospf cost 1;10 can't present in show run 

7.5.3.2(R0004.0246)
critical|MTMT12130 issue with cpu-rx NORMAL traffic

7.5.3.2(R0004.0244)
critical|MT10134 memory leaking issue	 
FIX|MT10135 authentication access-class telnet

7.5.3.2(R0004.0241)
critical|MT9986 issue with cpu-rx NORMAL traffic 

7.5.3.2(R0004.0239)
FIX|MT9950 vlan range in class-map	

7.5.3.2(R0004.0238)
FIX|MT9923 change info-center Logging format (the order of hostname/IP/time) to be the same as old syslog

7.5.3.2(R0004.0237)
FIX|MT9915 failed to delete ipv6 DHCP pool on switch

7.5.3.2(R0004.0236)
FIX|MT9868 monitor session access-list issue

7.5.3.2(R0004.0235)
ADD|MT9757 ssh-key access

7.5.3.2(R0004.0234)
FIX|MT9706 slow load with isolate-port group under vlan

7.5.3.2(R0004.0231)
FIX|MT9705 issue with archive

7.5.3.2(R0004.0229)
FIX|MT9541 issue with "[NSM]Report is invalid length" 

7.5.3.2(R0004.0228)
FIX|MT8990 BGP configuration logic

7.5.3.2(R0004.0227)
FIX|MT9406 ipv6 VRRP virtual ipv6 address issue

7.5.3.2(R0004.0226)
FIX|MT9418 issue with info-center record-cmd

7.5.3.2(R0004.0221)
ADD|MT9113 STP bpdu-tunnel with port-channel
FIX|MT9143 PIM memory leaking 

7.5.3.2(R0004.0215)
FIX|MT8902 RFC3509 compliance, 'ospf abr-type cisco' to be default config

7.5.3.2(R0004.0208)
FIX|MT9109 BGP peer-group configuration issue

7.5.3.2(R0004.0203)
FIX|MT8988 BGP configuration logic
FIX|MT9044 PIM unresolved cache issue

7.5.3.2(R0004.0202)
ADD|MT9036 ERPS work with CFM

7.5.3.2(R0004.0198)
ADD|MT8959 trap/syslog for ERPS

7.5.3.2(R0004.0197)
FIX|MT8938 STP issue on VSF

7.5.3.2(R0004.0195)
FIX|MT8909 Issue with bandwith control 

7.5.3.2(R0004.0194)
FIX|MT8903 socket leaking by tNTP

7.5.3.2(R0004.0193)
FIX|MT8865 add command 'power inline static'

7.5.3.2(R0004.0191)
FIX|MT8806 RPF-peer IP-address not changing after creating route

7.5.3.2(R0004.0190)
FIX|MT8820 ddmDiagnosisIfIndex issue

7.5.3.2(R0004.0189)
FIX|MT8610 interface link flap caused by snmpwalk OID 1.3.6.1.2.1.31.xxx

7.5.3.2(R0004.0186)
FIX|MT8759 switch reload when configuring snmpv3 authPriv 3des
FIX|MT8772 Q-in-Q with "pppoe intermediate agent"
FIX|MT8771 LLDP-MIB::lldpLocPortId and LLDP-MIB::lldpLocPortIdSubtype does not match 

7.5.3.2(R0004.0184)
FIX|MT8689 ssh dispatch run fatal error
ADD|MPLS and OPENFlOW1.0

7.5.3.2(R0004.0183)
FIX|MT8686 PoE issue with Cisco AP
add new command 'power inline high-inrush disable|enable' and 'power inline high-inrush mode swi|at' under port

7.5.3.2(R0004.0180)
FIX|MT8709 LLDP PortIdSubtype issue

7.5.3.2(R0004.0179)
FIX|MT8702 issue of vlan-translation with BGP

7.5.3.2(R0004.0178)
FIX|MT8703 DC power on or off cause trap messages
FIX|MT8709 ddmDiagnosisIfIndex shows all interfaces, set 'snmp-server ddm-electronic-hidden enable' as default

7.5.3.2(R0004.0175)
FIX|MT8654 Fatal error of task tSnmpd

7.5.3.2(R0004.0174)
ADD|MT8583 power status OID
PowerIndex:get power number(power1-AC;power2-DC)
PowerPresent:get power's status of present(1:present; 0: not present; 2-unknown)
PowerSupply:get power's supply status(1:up; 0:shutdown;2-unknown)

7.5.3.2(R0004.0173)
FIX|MT8660 OSPF issue with vlan-translation

7.5.3.2(R0004.0171)
FIX|MT8656 1.3.6.1.2.1.10.7.2.1.19 (dot3StatsDuplexStatus) always return 2

7.5.3.2(R0004.0170)
ADD|MT8572 "neighbor X.X.X.X override-capability" in vrf address-family mode

7.5.3.2(R0004.0169)
FIX|MT8584 trap messages for power AC to DC

7.5.3.2(R0004.0167)
FIX|MT8436 RADIUS attributes for bandwidth control on MAB

7.5.3.2(R0004.0165)
FIX|MT8560 VCT issue with across-pair short

7.5.3.2(R0004.0162)
FIX|MT8505 dhcp snooping discard dhcp packets with double tagged

7.5.3.2(R0004.0159)
FIX|MT8486 Issue with DAI and Port-channel

7.5.3.2(R0004.0157)
FIX|MT8446 no traps on AC power on/off 

7.5.3.2(R0004.0156)
FIX|MT8446 no traps on AC power on/off 

7.5.3.2(R0004.0155)
FIX|MT8463 S5750Ev2 Issue with 'show running-config | begin/include/exclude'

7.5.3.2(R0004.0154)
ADD|MT8377 synchronization of logfile

7.5.3.2(R0004.0152)
ADD|MT8390 transfer user privilege via radius server, add new private attribute DCN-Privilege-Level
ADD|MT8321 new commands to match dscp and flow-label in ipv6 ACL
ADD|MT8319 new commands 'pass-through-dscp' and 'pass-throught-cos' under policy-map

7.5.3.2(R0004.0151)
FIX|MT8409 task tftpCopyFile hangup when upgrading error img file
ADD|MT8391 add new command "load running-config from tftp://"

7.5.3.2(R0004.0150)
ADD|MT8392 get sfp speed and wavelength info via snmp
ADD|MT8363 snmp trap login\logout

7.5.3.2(R0004.0149)
FIX|MT8350 doesn't change report source-address for IGMPv3
ADD|MT8353 snmp OIDs for mrpp

7.5.3.2(R0004.0148)
FIX|MT8371 S5750E-28F-SI-R logging issue

7.5.3.2(R0004.0147)
FIX|MT8376 hide password in log
FIX|MT8369 issue with interface VLAN statistics , add command "vlan-flow-statistics" under interface vlan
FIX|MT8355 lacp timeout short leads to freeze the switch
FIX|MT8309 DHCP Snooping intersepts PXE BINL packets

7.5.3.2(R0004.0146)
FIX|MT8351 issue with QinQ and bpdu-tunnel stp

7.5.3.2(R0004.0145)
FIX|MT8339 ncorrect messages order in 'show log'

7.5.3.2(R0004.0143)
FIX| ip arp inspection limit-rate doesn't work on slave member

7.5.3.2(R0004.0141)
ADD|MT8295 add “ip dhcp snooping binding usercontrol” on interface port-channel 

7.5.3.2(R0004.0140)
ADD|MT8298 add LLDP dot3 TLV
ADD|MT8294 ip dhcp snooping binding user-control [vlan] [max-user]

7.5.3.2(R0004.0138)
ADD|MT8292 IGMP proxy with static igmp group requirement
FIX|MT8305 can't delete ip acl rule with dscp
ADD|MT8296 add arp-inspection under VSF mode
FIX|MT8304 Issue with DHCP Snooping untrusted ports 
ADD|MT8297 add command "(no)mld snooping drop (report | query)"

7.5.3.2(R0004.0136)
FIX|MT8277 VSF mode. Isolate-port in VLAN mode with portchannel doesn't work

7.5.3.2(R0004.0134)
FIX|MT8219 router bgp network advertise routes which doesn't actually know 
FIX| memory leaking caused by configuring “ntp server host” 

7.5.3.2(R0004.0132)
FIX|MT8251 Port isolation in VLAN mode affects all VLANs

7.5.3.2(R0004.0131)
FIX|MT8219 router bgp network advertise routes which doesn't actually know

7.5.3.2(R0004.0129)
FIX|MT8234 ntp server host issue

7.5.3.2(R0004.0126)
ADD|MT8209 `mls qos trust` for port-channel interface

7.5.3.2(R0004.0125)
FIX|MT8203 'mls qos queue statistics enable' doesn't save in 'show run' after reboot

7.5.3.2(R0004.0124)
ADD|MT8173 SNMP OID for dropped packets count in 'show mls qos queue statistics' 
ADD|MT8166 command and user privilege

7.5.3.2(R0004.0123)
ADD|MT8171 copy command in vrf

7.5.3.2(R0004.0122)
FIX|MT8164 add new command "interface mode sgmii" on sfp port

7.5.3.2(R0004.0120)
FIX|MT8166 command and user privilege

7.5.3.2(R0004.0119)
FIX|MT8167 S5750Ev2 igmp snooping doesn't work with flexible QinQ

7.5.3.2(R0004.0118)
FIX|MT8146 Problem with NFS fragmented packets

7.5.3.2(R0004.0117)
FIX|MT8136 incorrect Martian NLRI
ADD|MT8138 set COS on L3 interface
FIX|MT8002 reboot by tTelnetClientTask

7.5.3.2(R0004.0116)
FIX|MT8139 NTP server transmits the local time (including timezone) instead of GMT time

7.5.3.2(R0004.0114)
FIX|MT8132 `show tech no-more` freezes switch
FIX|MT8129 BGP session closes due to UPDATE with 0xD0 attribute flag 
FIX|MT8126 In VSF mode reload SM cause AM restart
FIX|MT8131 “show vlan” hangup with 4094 vlans

7.5.3.2(R0004.0113)
ADD|MT8122 bgp override-capability by default

7.5.3.2(R0004.0111)
ADD|MT8090 add command "archive running-config"

7.5.3.2(R0004.0108)
ADD|MT7937 5750Ev2 Disable logging for interface
add new command "no logging event link-status" on port and "no logging event link-status global"

7.5.3.2(R0004.0107)
FIX|MT8060 hardware license issue
ADD|MT7912 power monitoring , released new SNMP mib file "DCN_private_2.1.60_trap_notify"
ADD|MT8043 DHCPv6-solicit DUID type 4 (RFC6355) support

7.5.3.2(R0004.0101)
FIX|MT8039 ipv6 ssh issue

7.5.3.2(R0004.0095)
FIX|MT7999 switch freezed as telnet client

7.5.3.2(R0004.0094)
FIX|MT8013 S5750Ev2 show mls qos queue statistics issue

7.5.3.2(R0004.0092)
FIX|MT8000 S5750Ev2 did not support Entity MIB (rfc2737)

7.5.3.2(R0004.0091)
ADD|MT7929 S5750E-28F-SI-R apply service-policy to port-channel

7.5.3.2(R0004.0090)
FIX|MT7934 S5750E R2 can't configure OSPF filter-policy with prefix-list

7.5.3.2(R0004.0089)
ADD|MT7923 new key exchange algorithms for SSH. 
kex algorithm: diffie-hellman-group14-sha1，curve25519-sha256@libssh.org，curve25519-sha256，diffie-hellman-group14-sha256，diffie-hellman-group16-sha512，diffie-hellman-group1-sha1
symmetric encryption algorithm: aes128-cbc，aes256-cbc，aes256-ctr，aes128-ctr，3des-ctr，3des-cbc

7.5.3.2(R0004.0088)
FIX|MT7913 S5750Ev2  `enable` gives no effect for privilege 1 user

7.5.3.2(R0004.0086)
FIX|MT7860 byte-order error when show info-center direction loghost channel 2

7.5.3.2(R0004.0085)
FIX|MT7841 Speed negotiation on 1G and 10G ports

7.5.3.2(R0004.0083)
FIX|MT7811 PIM doesn't set random multicast groups in MFC due to SPT bit not set

7.5.3.2(R0004.0081)
ADD|MT7767 default `mac-address-table bucket size` value to be 4

7.5.3.2(R0004.0080)
FIX|MT7738 switch drop dhcp packets even dhcp snooping specify different vlan

7.5.3.2(R0004.0076)
FIX|MT7758 S5750ER2 problem with VCT 

7.5.3.2(R0004.0075)
FIX|MT7743 show power issue and trap issue

7.5.3.2(R0004.0074)
ADD|MT7664 add command "show log" as "show info-center logsdram"

7.5.3.2(R0004.0071)
FIX|MT7737 show ip igmp snooping vlan X no return when switch is learning new igmp groups

7.5.3.2(R0004.0069)
FIX|MT7725 console freeze when show ip igmp snooping vlan x 

7.5.3.2(R0004.0067)
FIX|MT7711 S5750Ev2 freeze when receive 20 pps IGMP packets

7.5.3.2(R0004.0066)
FIX|MT7685 S5750Ev2 abnormal logs on vsf port

7.5.3.2(R0004.0062)
FIX|MT7644 S5750Ev2 can't auto-negotiate to 100M

7.5.3.2(R0004.0061)
FIX|MT7631 S5750Ev2 - info-center loghost wrong facility 

7.5.3.2(R0004.0059)
FIX|MT7608 S5750E-28F-SI-R `clock timezone`
FIX|MT7607 S5750Ev2 - `show clock`

7.5.3.2(R0004.0057)
FIX|MT7609 S5750E-28F-SI-R combo-port doesn’t forward traffic with 10/100-FD

7.5.3.2(R0004.0055)
ADD|MT7535 info-center log new on the top

7.5.3.2(R0004.0053)
FIX|MT7539 S5750Ev2 reboot after "show run" with "logging" command

7.5.3.2(R0004.0052)
FIX|MT7490 freeze after no ip route bfd
