7.5.3.0(R0010.0221)
FIX|MT9042 no label for null route 
FiX|MT9099 PIM unresolved cache issue 

7.5.3.0(R0010.0219)
FIX|MT9055 IPv4 Multicast issue

7.5.3.0(R0010.0217)
FIX|MT8923 unexpected rebooted by zOPENFLOW

7.5.3.0(R0010.0215)
FIX|MT8890 vlan-flow-statistics issue

7.5.3.0(R0010.0213)
ADD|MT8691 increase interface vlan statistics limit to be 256 at most，add new command ‘show tcam usage’ to check L4 resources usage
ADD|MT8718 add VPLS peer state change trap OID ---101.127.1

7.5.3.0(R0010.0212)
FIX|MT8594 default route in VRF

7.5.3.0(R0010.0211)
FIX|MT8833 ddmDiagnosisIfIndex issue

7.5.3.0(R0010.0210)
FIX|MT8814 VPLS and ERPS issue

7.5.3.0(R0010.0208)
FIX|MT8698 'ssh dispatch run fatal' error 

7.5.3.0(R0010.0206)
FIX|MT8592 all line protocol of interface vlan up

7.5.3.0(R0010.0205)
FIX|MT7785 hangup due to skb leaking
FIX|MT8578 VSF member2 skb leaking

7.5.3.0(R0010.0202)
FIX|MT8491 "show mpls enable" displays only to terminal monitor

7.5.3.0(R0010.0195)
ADD|MT8268 new command “vlan-flow-statistics” under interface vlan

7.5.3.0(R0010.0194)
FIX|MT8290 reboot due to tSnmpd

7.5.3.0(R0010.0193)
FIX|MT8275 low CPU rate-limit for ICMP messages

7.5.3.0(R0010.0191)
FIX|MT8243 invalid traffic statistics on L3 Interface, add command `vlan-flow-statistic`

7.5.3.0(R0010.0190)
FIX|MT8197 issue with arp when xconnect in portchannel

7.5.3.0(R0010.0189)
FIX|MT8202 `loopback-detection specified-vlan 2-4094` on trunk ports cause high CPU load 

7.5.3.0(R0010.0187)
ADD|MT8119 `mls qos trust` for port-channel interface

7.5.3.0(R0010.0186)
FIX|MT7894 ldp downstream-on-demand mode don't request labels for FEC in vrf

7.5.3.0(R0010.0184)
FIX|MT8047 snmp-server config disappears frequently

7.5.3.0(R0010.0182)
FIX|MT8033 monitor session destination interface removal issue

7.5.3.0(R0010.0181)
FIX|MT8002 reboot by tTelnetClientTask
FIX|MT8003 doesn't display `ip ospf cost 10` in running-config

7.5.3.0(R0010.0179)
FIX|MT8007 can't remove sys.log file correctly

7.5.3.0(R0010.0177)
FIX|MT7976 ip dhcp conflict ping-detection in vrf

7.5.3.0(R0010.0175)
ADD|MT7880 apply service-policy to port-channel

7.5.3.0(R0010.0174)
FIX|MT7892 snmpv3 doesn't support 3des

7.5.3.0(R0010.0173)
FIX|MT7738 dhcp snooping drops dhcp frames with ethernet trailer

7.5.3.0(R0010.0171)
ADD|MT7630 new key exchange algorithms for SSH. 
kex algorithm: diffie-hellman-group14-sha1，curve25519-sha256@libssh.org，curve25519-sha256，diffie-hellman-group14-sha256，diffie-hellman-group16-sha512，diffie-hellman-group1-sha1
symmetric encryption algorithm: aes128-cbc，aes256-cbc，aes256-ctr，aes128-ctr，3des-ctr，3des-cbc

7.5.3.0(R0010.0170)
FIX|MT7748 NTP server uses wrong source on respond

7.5.3.0(R0010.0169)
ADD|MT7708 add command “snmp-server fdbMacInfoTable-mib enable | disable”

7.5.3.0(R0010.0168)
FIX|MT7533 summary-LSA from stub-area shorter than Extrernal-LSA default

7.5.3.0(R0010.0166)
FIX|MT7637 large output is truncated sometimes via SSH

7.5.3.0(R0010.0163)
ADD|MT7578 add command “l3-interface care vlan”

7.5.3.0(R0010.0161)
ADD|MT7485 detailed bgp log-neighbor-changes

7.5.3.0(R0010.0159)
FIX|MT7529 1.3.6.1.2.1.10.7.2.1.19 (dot3StatsDuplexStatus) always return 2
FIX|MT7483 web-management-interface not available in vrf

7.5.3.0(R0010.0154)
FIX|MT7411 LLDP packets with ipv6 management address TLV and with Protocol identity TLV did not accespted by switches

7.5.3.0(R0010.0151)
FIX|MT7275 on combo ports flow-control enabled as default

7.5.3.0(R0010.0147)
ADD|MT6849 clear specific arp
ADD|MT6849 oid for fdb entries count

7.5.3.0(R0010.0146)
ADD|MT6905 QoS statistics SNMP oid

7.5.3.0(R0010.0145)
FIX|MT7088 vfi problem
ADD|DHCPv6-solicit DUID type 4 (RFC6355) support

7.5.3.0(R0010.0138)
FIX|MT7116 snmp config 

7.5.3.0(R0010.0136)
FIX|MT7052 OSPF task hangup

7.5.3.0(R0010.0133)
FIX|MT6949 TACACS+ authentification critical exception

7.5.3.0(R0010.0128)
FIX|MT6972 BGP inappropriate "unsupported capabilty" NOTIFICATION usage

7.5.3.0(R0010.0127)
FIX|MT6914 egress xconnect EXP-COS mapping

7.5.3.0(R0010.0126)
FIX|MT6781 L3-traffic mls qos statistics

7.5.3.0(R0010.0125)
FIX|MT6853 dont save vacl after reboot
FIX|MT6844 does not work with more than 512 l3 interfaces

7.5.3.0(R0010.0123)
FIX|MT6782 reboot by watchdog

7.5.3.0(R0010.0121)
FIX|MT6764 timezone isnt save after reload

7.5.3.0(R0010.0120)
FIX|MT6699 dhcp relay via vrf

7.5.3.0(R0010.0119)
ADD|MT6511 switchport association multicast-vlan x out-tag feature

7.5.3.0(R0010.0117)
FIX|MT6679 incorrect source ip for SNMP in vrf

7.5.3.0(R0010.0116)
FIX|MT6681 ECMP hardware router overflow
FIX|MT6678 ECMP CPU source ip

7.5.3.0(R0010.0114)
FIX|MT6657 "From running CPU USAGE" displays incorrectly

7.5.3.0(R0010.0113)
FIX|MT6589 MPLS over l2-vc fixed

7.5.3.0(R0010.0111)
FIX|MT6584 swtich crashed by unknown-smac packets with high pps when mac-address-learning control is enabling

7.5.3.0(R0010.0109)
FIX|MT6424 MPLS VPN recovery problem

7.5.3.0(R0010.0108)
FIX|MT6419 CPU stats issue

7.5.3.0(R0010.0107)
FIX|MT6429 mac-address-table blackhole 00-00-00-00-00-00

7.5.3.0(R0010.0106)
FIX|MT6421 SNMP oid correction

7.5.3.0(R0010.0105)
FIX|MT6410 BGP sessions not disabled in the peer-group 

7.5.3.0(R0010.0102)
FIX|MT6379 logging in vrf (cosmetic)

7.5.3.0(R0010.0101)
FIX|MT6312 logging source-ip

7.5.3.0(R0010.0098)
FIX|MT6335 Openflow manufacturer description

7.5.3.0(R0010.0095)
FIX|MT6285 logging facility/level/source-ip

7.5.3.0(R0010.0092)
FIX|MT6246 DHCP server doesn't work on interface bound to VRF

7.5.3.0(R0010.0091)
FIX|MT6204 Fix critical issue on SNR-S300G-24FX

7.5.3.0(R0010.0090)
FIX|MT6176 multicast load-balancing on port-group, add command "no-unicast disable/enable"

7.5.3.0(R0010.0086)
FIX|MT6110 port isolation does not work between physical port and port-channel

7.5.3.0(R0010.0084)
FIX|MT6009 VPLS doesn't work with Cisco CSR
FIX|MT5917 task DhcpRcv hangup

7.5.3.0(R0010.0082)
FIX|MT5992 OSPF algo and link detection issue
FIX|MT5993 multicast drops every 5 minutes
FIX|MT6002 monitor session& port-range ACL issue

7.5.3.0(R0010.0081)
FIX|MT5978 unable to add openflow rules

7.5.3.0(R0010.0080)
FIX|MT5971 critical issue on VSF HA (packets can't reach CPU)
FIX|RDM57035 release new boot.rom version 7.3.126 for jffs2 file system problem

7.5.3.0(R0010.0079)
FIX|MT5905 MTU in MPLS L2 VPN less than configured

7.5.3.0(R0010.0078)
FIX|MT5950 sh clock
ADD|0005805: add ssh, snmp, tftp, radius feature in VRF

7.5.3.0(R0010.0073)
FIX|MT5851 Multicast with well-know address are not forwarded via xconnect

7.5.3.0(R0010.0072)
FIX|MT5864 did not balance multicast traffic in port-channel

7.5.3.0(R0010.0070)
ADD|MT5721 match vlan range in class-map
FIX|MT5664 supervlan issue

7.5.3.0(R0010.0069)
ADD| ERPS G.8032 support

7.5.3.0(R0010.0066)
FIX|MT5588 bad PDU length error on VSF firmware
