                              Silicom LTD.
                    Silicom Red Rock Canyon (RRC) series
                            RELEASE RRC_BPD_2r12
                              (8/10/2019)

                              RELEASE NOTES

These notes describe the software for Silicom Red Rock Canyon / FM10K series.
Online versions of the user guide in HTML formats is located in the \manuals folder
of the Silicom RRC Software CD.
These notes provide last minute corrections (if any) to the user manual for this product package.

This release CD contains software drivers and manual for the following products:

Content aware redirector products:
==================================
PE310G4DBiR-SRD/LRD - Quad port 10 Giga Ethernet Fiber SR/LR PCI-E3 x8 Adapter with Bypass and content aware redirector feature based on Intel FM10420 chip.
PE310G4DBiR-ER - Quad port 10 Giga Ethernet Fiber ER PCI-E3 x8 Adapter with Bypass and content aware redirector feature based on Intel FM10420 chip.
PE310G4DBiR-DA - Quad port 10 Giga Ethernet DA (Direct Attached) PCI-E3 x8 Adapter with Bypass and content aware redirector feature based on Intel FM10420 chip.
PE310G4DBiR-T   - Quad port 10 Giga Ethernet Copper PCI-E3 x8 Adapter with Bypass and content aware redirector feature based on Intel FM10420 chip.
PE325G2DSIR-XR - Dual port 25 Giga Ethernet Fiber XR  PCI-E3 x8 Adapter low profile with  content aware redirector feature based on Intel FM10420 chip.
PE340G2DBiR-QS41/43/QL4 - Dual port 40 Giga Ethernet Fiber SR4 100/300m /LR4 PCI-E3 x16 Adapter with Bypass and content aware redirector feature, Intel FM10420 chip.
PE3100G2DQiR-ZS4 - Dual port 100 Giga Ethernet Fiber XR4  PCI-E3 x16 Adapter with  content aware redirector feature based on Intel FM10420 chip.
PE3100G2DQiRL-ZS4 - Dual port 100 Giga Ethernet Fiber XR4  PCI-E3 2x8 Adapter low profile with content aware redirector feature based on Intel FM10420 chip.
PE3100G2DQIR8-QX4/ZS4/ZL4/QS41/QS43/QL4 - Dual port Fiber 100 Gigabit Ethernet PCI Express Content Director Server Adapter based on Intel FM10840 chip.

This CD release include also driver and api for the redirector module of the products.

Drivers support:
================

Intel based bypass product currently support the following OS:
Linux kernel 2.4.x & 2.6.x, 3.x.x

Release content
===============
This release contains the following software programs:

User guide
===========
Linux content aware redirector programmer guide documentation	\manual\RRC_RDFI_PG.pdf

Linux:
--------
Director rdif driver RRC 		\Linux\Redirect\RD_RRC_Control\rdif-6.0.10.7.30.1.tar.gz

Intel FM10K NIC/Bypass driver		\Linux\Network_Drivers\IntelFM10k_NicBP\fm10k-0.26.1.sl.3.2.tar.gz
Intel FM10K  Intel Org driver			\Linux\Network_Drivers\IntelFM10k_Org\fm10k-0.26.1.tar.gz

					



